;
; MFA XP Lite Label file. Valid from software V2.00
;
; (C) MFA XP Automotive Systems 2013
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Misc
001,1,Battery
001,2,NWM
001,3,Ignition
001,4,S-Contact
;
002,0,Boost pressure
002,1,Raw AD
002,2,Voltage
002,3,Result
002,4,Spare
;
003,0,Oil pressure
003,1,Raw
003,2,Resistance
003,3,Result
003,4,Spare
;
;---------------------------------------------------
;
; adaption
;
;---------------------------------------------------
;
A001,0,Max. engine torque in NM (0 = Use CAN)
;
;
;---------------------------------------------------
;
; Long Coding
;
;---------------------------------------------------
;
;
; {Basic Setup}
LC,00,0,Bring MFA XP Lite to front after ignition is on
LC,00,1,Show raw boost pressure instead of height corrected
LC,00,2,Set exhaust flap to open during ignition on (otherwise flap state is normal)
LC,00,3~4,08,Language: German
LC,00,3~4,10,Language: English
; {Boost source}
LC,00,5~7,00,Boost source: OFF
LC,00,5~7,20,Boost source: CAN 0...2.5bar
LC,00,5~7,40,Boost source: CAN 0...5bar
LC,00,5~7,60,Boost source: Box internal
LC,00,5~7,80,Boost source: VW 250kPA
LC,00,5~7,A0,Boost source: VW 300kPA
LC,00,5~7,C0,Boost source: VW 400kPA
; {Units Setup}
LC,01,0,Temperature Unit: °F instead of °C
LC,01,1,Speed Unit: MPH instead of KM/H
LC,01,2,Power Unit: KW instead of HP
LC,01,3,Torque Unit: LBF instead of NM
LC,01,4,Pressure Unit: PSI instead of BAR
; {Screen 1/Line 1}
LC,02,0~7,00,Screen 1/Line 1: Off
LC,02,0~7,01,Screen 1/Line 1: Engine Oil Temperature
LC,02,0~7,02,Screen 1/Line 1: Engine Intake Temperature
LC,02,0~7,03,Screen 1/Line 1: Engine Cooling Temperature
LC,02,0~7,04,Screen 1/Line 1: Outside Temperature
LC,02,0~7,05,Screen 1/Line 1: Engine RPM
LC,02,0~7,06,Screen 1/Line 1: Oil Pressure
LC,02,0~7,07,Screen 1/Line 1: Boost
LC,02,0~7,08,Screen 1/Line 1: Engine Power
LC,02,0~7,09,Screen 1/Line 1: Engine Power Loss
LC,02,0~7,0A,Screen 1/Line 1: Engine Power Wheel
LC,02,0~7,0B,Screen 1/Line 1: Engine Torque
LC,02,0~7,0C,Screen 1/Line 1: Engine Torque Loss
LC,02,0~7,0D,Screen 1/Line 1: Engine Torque Wheel
LC,02,0~7,0E,Screen 1/Line 1: Engine Pedal Position
LC,02,0~7,0F,Screen 1/Line 1: Engine Throttle Position
LC,02,0~7,10,Screen 1/Line 1: Wheel speed Front Left
LC,02,0~7,11,Screen 1/Line 1: Wheel speed Front Right
LC,02,0~7,12,Screen 1/Line 1: Wheel speed Back Left
LC,02,0~7,13,Screen 1/Line 1: Wheel speed Back Right
LC,02,0~7,14,Screen 1/Line 1: Brake Pressure
LC,02,0~7,15,Screen 1/Line 1: G across
LC,02,0~7,16,Screen 1/Line 1: Gierrate
LC,02,0~7,17,Screen 1/Line 1: Steering Angle
LC,02,0~7,18,Screen 1/Line 1: Haldex Clutch Open
LC,02,0~7,19,Screen 1/Line 1: Haldex Overtemp
LC,02,0~7,1A,Screen 1/Line 1: Haldex Transmitted Torque
LC,02,0~7,1B,Screen 1/Line 1: Haldex Oil Temperature
LC,02,0~7,1C,Screen 1/Line 1: Car Speed
LC,02,0~7,1D,Screen 1/Line 1: Fuel Content
LC,02,0~7,1E,Screen 1/Line 1: Voltage
LC,02,0~7,1F,Screen 1/Line 1: DSG Current Gear
; {Screen 1/Line 2}
LC,03,0~7,00,Screen 1/Line 2: Off
LC,03,0~7,01,Screen 1/Line 2: Engine Oil Temperature
LC,03,0~7,02,Screen 1/Line 2: Engine Intake Temperature
LC,03,0~7,03,Screen 1/Line 2: Engine Cooling Temperature
LC,03,0~7,04,Screen 1/Line 2: Outside Temperature
LC,03,0~7,05,Screen 1/Line 2: Engine RPM
LC,03,0~7,06,Screen 1/Line 2: Oil Pressure
LC,03,0~7,07,Screen 1/Line 2: Boost
LC,03,0~7,08,Screen 1/Line 2: Engine Power
LC,03,0~7,09,Screen 1/Line 2: Engine Power Loss
LC,03,0~7,0A,Screen 1/Line 2: Engine Power Wheel
LC,03,0~7,0B,Screen 1/Line 2: Engine Torque
LC,03,0~7,0C,Screen 1/Line 2: Engine Torque Loss
LC,03,0~7,0D,Screen 1/Line 2: Engine Torque Wheel
LC,03,0~7,0E,Screen 1/Line 2: Engine Pedal Position
LC,03,0~7,0F,Screen 1/Line 2: Engine Throttle Position
LC,03,0~7,10,Screen 1/Line 2: Wheel speed Front Left
LC,03,0~7,11,Screen 1/Line 2: Wheel speed Front Right
LC,03,0~7,12,Screen 1/Line 2: Wheel speed Back Left
LC,03,0~7,13,Screen 1/Line 2: Wheel speed Back Right
LC,03,0~7,14,Screen 1/Line 2: Brake Pressure
LC,03,0~7,15,Screen 1/Line 2: G across
LC,03,0~7,16,Screen 1/Line 2: Gierrate
LC,03,0~7,17,Screen 1/Line 2: Steering Angle
LC,03,0~7,18,Screen 1/Line 2: Haldex Clutch Open
LC,03,0~7,19,Screen 1/Line 2: Haldex Overtemp
LC,03,0~7,1A,Screen 1/Line 2: Haldex Transmitted Torque
LC,03,0~7,1B,Screen 1/Line 2: Haldex Oil Temperature
LC,03,0~7,1C,Screen 1/Line 2: Car Speed
LC,03,0~7,1D,Screen 1/Line 2: Fuel Content
LC,03,0~7,1E,Screen 1/Line 2: Voltage
LC,03,0~7,1F,Screen 1/Line 2: DSG Current Gear
; {Screen 1/Line 3}
LC,04,0~7,00,Screen 1/Line 3: Off
LC,04,0~7,01,Screen 1/Line 3: Engine Oil Temperature
LC,04,0~7,02,Screen 1/Line 3: Engine Intake Temperature
LC,04,0~7,03,Screen 1/Line 3: Engine Cooling Temperature
LC,04,0~7,04,Screen 1/Line 3: Outside Temperature
LC,04,0~7,05,Screen 1/Line 3: Engine RPM
LC,04,0~7,06,Screen 1/Line 3: Oil Pressure
LC,04,0~7,07,Screen 1/Line 3: Boost
LC,04,0~7,08,Screen 1/Line 3: Engine Power
LC,04,0~7,09,Screen 1/Line 3: Engine Power Loss
LC,04,0~7,0A,Screen 1/Line 3: Engine Power Wheel
LC,04,0~7,0B,Screen 1/Line 3: Engine Torque
LC,04,0~7,0C,Screen 1/Line 3: Engine Torque Loss
LC,04,0~7,0D,Screen 1/Line 3: Engine Torque Wheel
LC,04,0~7,0E,Screen 1/Line 3: Engine Pedal Position
LC,04,0~7,0F,Screen 1/Line 3: Engine Throttle Position
LC,04,0~7,10,Screen 1/Line 3: Wheel speed Front Left
LC,04,0~7,11,Screen 1/Line 3: Wheel speed Front Right
LC,04,0~7,12,Screen 1/Line 3: Wheel speed Back Left
LC,04,0~7,13,Screen 1/Line 3: Wheel speed Back Right
LC,04,0~7,14,Screen 1/Line 3: Brake Pressure
LC,04,0~7,15,Screen 1/Line 3: G across
LC,04,0~7,16,Screen 1/Line 3: Gierrate
LC,04,0~7,17,Screen 1/Line 3: Steering Angle
LC,04,0~7,18,Screen 1/Line 3: Haldex Clutch Open
LC,04,0~7,19,Screen 1/Line 3: Haldex Overtemp
LC,04,0~7,1A,Screen 1/Line 3: Haldex Transmitted Torque
LC,04,0~7,1B,Screen 1/Line 3: Haldex Oil Temperature
LC,04,0~7,1C,Screen 1/Line 3: Car Speed
LC,04,0~7,1D,Screen 1/Line 3: Fuel Content
LC,04,0~7,1E,Screen 1/Line 3: Voltage
LC,04,0~7,1F,Screen 1/Line 3: DSG Current Gear
; {Screen 1/Line 4}
LC,05,0~7,00,Screen 1/Line 4: Off
LC,05,0~7,01,Screen 1/Line 4: Engine Oil Temperature
LC,05,0~7,02,Screen 1/Line 4: Engine Intake Temperature
LC,05,0~7,03,Screen 1/Line 4: Engine Cooling Temperature
LC,05,0~7,04,Screen 1/Line 4: Outside Temperature
LC,05,0~7,05,Screen 1/Line 4: Engine RPM
LC,05,0~7,06,Screen 1/Line 4: Oil Pressure
LC,05,0~7,07,Screen 1/Line 4: Boost
LC,05,0~7,08,Screen 1/Line 4: Engine Power
LC,05,0~7,09,Screen 1/Line 4: Engine Power Loss
LC,05,0~7,0A,Screen 1/Line 4: Engine Power Wheel
LC,05,0~7,0B,Screen 1/Line 4: Engine Torque
LC,05,0~7,0C,Screen 1/Line 4: Engine Torque Loss
LC,05,0~7,0D,Screen 1/Line 4: Engine Torque Wheel
LC,05,0~7,0E,Screen 1/Line 4: Engine Pedal Position
LC,05,0~7,0F,Screen 1/Line 4: Engine Throttle Position
LC,05,0~7,10,Screen 1/Line 4: Wheel speed Front Left
LC,05,0~7,11,Screen 1/Line 4: Wheel speed Front Right
LC,05,0~7,12,Screen 1/Line 4: Wheel speed Back Left
LC,05,0~7,13,Screen 1/Line 4: Wheel speed Back Right
LC,05,0~7,14,Screen 1/Line 4: Brake Pressure
LC,05,0~7,15,Screen 1/Line 4: G across
LC,05,0~7,16,Screen 1/Line 4: Gierrate
LC,05,0~7,17,Screen 1/Line 4: Steering Angle
LC,05,0~7,18,Screen 1/Line 4: Haldex Clutch Open
LC,05,0~7,19,Screen 1/Line 4: Haldex Overtemp
LC,05,0~7,1A,Screen 1/Line 4: Haldex Transmitted Torque
LC,05,0~7,1B,Screen 1/Line 4: Haldex Oil Temperature
LC,05,0~7,1C,Screen 1/Line 4: Car Speed
LC,05,0~7,1D,Screen 1/Line 4: Fuel Content
LC,05,0~7,1E,Screen 1/Line 4: Voltage
LC,05,0~7,1F,Screen 1/Line 4: DSG Current Gear
; {Screen 1/Line 5}
LC,06,0~7,00,Screen 1/Line 5 (red display only): Off
LC,06,0~7,01,Screen 1/Line 5 (red display only): Engine Oil Temperature
LC,06,0~7,02,Screen 1/Line 5 (red display only): Engine Intake Temperature
LC,06,0~7,03,Screen 1/Line 5 (red display only): Engine Cooling Temperature
LC,06,0~7,04,Screen 1/Line 5 (red display only): Outside Temperature
LC,06,0~7,05,Screen 1/Line 5 (red display only): Engine RPM
LC,06,0~7,06,Screen 1/Line 5 (red display only): Oil Pressure
LC,06,0~7,07,Screen 1/Line 5 (red display only): Boost
LC,06,0~7,08,Screen 1/Line 5 (red display only): Engine Power
LC,06,0~7,09,Screen 1/Line 5 (red display only): Engine Power Loss
LC,06,0~7,0A,Screen 1/Line 5 (red display only): Engine Power Wheel
LC,06,0~7,0B,Screen 1/Line 5 (red display only): Engine Torque
LC,06,0~7,0C,Screen 1/Line 5 (red display only): Engine Torque Loss
LC,06,0~7,0D,Screen 1/Line 5 (red display only): Engine Torque Wheel
LC,06,0~7,0E,Screen 1/Line 5 (red display only): Engine Pedal Position
LC,06,0~7,0F,Screen 1/Line 5 (red display only): Engine Throttle Position
LC,06,0~7,10,Screen 1/Line 5 (red display only): Wheel speed Front Left
LC,06,0~7,11,Screen 1/Line 5 (red display only): Wheel speed Front Right
LC,06,0~7,12,Screen 1/Line 5 (red display only): Wheel speed Back Left
LC,06,0~7,13,Screen 1/Line 5 (red display only): Wheel speed Back Right
LC,06,0~7,14,Screen 1/Line 5 (red display only): Brake Pressure
LC,06,0~7,15,Screen 1/Line 5 (red display only): G across
LC,06,0~7,16,Screen 1/Line 5 (red display only): Gierrate
LC,06,0~7,17,Screen 1/Line 5 (red display only): Steering Angle
LC,06,0~7,18,Screen 1/Line 5 (red display only): Haldex Clutch Open
LC,06,0~7,19,Screen 1/Line 5 (red display only): Haldex Overtemp
LC,06,0~7,1A,Screen 1/Line 5 (red display only): Haldex Transmitted Torque
LC,06,0~7,1B,Screen 1/Line 5 (red display only): Haldex Oil Temperature
LC,06,0~7,1C,Screen 1/Line 5 (red display only): Car Speed
LC,06,0~7,1D,Screen 1/Line 5 (red display only): Fuel Content
LC,06,0~7,1E,Screen 1/Line 5 (red display only): Voltage
LC,06,0~7,1F,Screen 1/Line 5 (red display only): DSG Current Gear
; {Screen 2/Line 1}
LC,07,0~7,00,Screen 2/Line 1: Off
LC,07,0~7,01,Screen 2/Line 1: Engine Oil Temperature
LC,07,0~7,02,Screen 2/Line 1: Engine Intake Temperature
LC,07,0~7,03,Screen 2/Line 1: Engine Cooling Temperature
LC,07,0~7,04,Screen 2/Line 1: Outside Temperature
LC,07,0~7,05,Screen 2/Line 1: Engine RPM
LC,07,0~7,06,Screen 2/Line 1: Oil Pressure
LC,07,0~7,07,Screen 2/Line 1: Boost
LC,07,0~7,08,Screen 2/Line 1: Engine Power
LC,07,0~7,09,Screen 2/Line 1: Engine Power Loss
LC,07,0~7,0A,Screen 2/Line 1: Engine Power Wheel
LC,07,0~7,0B,Screen 2/Line 1: Engine Torque
LC,07,0~7,0C,Screen 2/Line 1: Engine Torque Loss
LC,07,0~7,0D,Screen 2/Line 1: Engine Torque Wheel
LC,07,0~7,0E,Screen 2/Line 1: Engine Pedal Position
LC,07,0~7,0F,Screen 2/Line 1: Engine Throttle Position
LC,07,0~7,10,Screen 2/Line 1: Wheel speed Front Left
LC,07,0~7,11,Screen 2/Line 1: Wheel speed Front Right
LC,07,0~7,12,Screen 2/Line 1: Wheel speed Back Left
LC,07,0~7,13,Screen 2/Line 1: Wheel speed Back Right
LC,07,0~7,14,Screen 2/Line 1: Brake Pressure
LC,07,0~7,15,Screen 2/Line 1: G across
LC,07,0~7,16,Screen 2/Line 1: Gierrate
LC,07,0~7,17,Screen 2/Line 1: Steering Angle
LC,07,0~7,18,Screen 2/Line 1: Haldex Clutch Open
LC,07,0~7,19,Screen 2/Line 1: Haldex Overtemp
LC,07,0~7,1A,Screen 2/Line 1: Haldex Transmitted Torque
LC,07,0~7,1B,Screen 2/Line 1: Haldex Oil Temperature
LC,07,0~7,1C,Screen 2/Line 1: Car Speed
LC,07,0~7,1D,Screen 2/Line 1: Fuel Content
LC,07,0~7,1E,Screen 2/Line 1: Voltage
LC,07,0~7,1F,Screen 2/Line 1: DSG Current Gear
; {Screen 2/Line 2}
LC,08,0~7,00,Screen 2/Line 2: Off
LC,08,0~7,01,Screen 2/Line 2: Engine Oil Temperature
LC,08,0~7,02,Screen 2/Line 2: Engine Intake Temperature
LC,08,0~7,03,Screen 2/Line 2: Engine Cooling Temperature
LC,08,0~7,04,Screen 2/Line 2: Outside Temperature
LC,08,0~7,05,Screen 2/Line 2: Engine RPM
LC,08,0~7,06,Screen 2/Line 2: Oil Pressure
LC,08,0~7,07,Screen 2/Line 2: Boost
LC,08,0~7,08,Screen 2/Line 2: Engine Power
LC,08,0~7,09,Screen 2/Line 2: Engine Power Loss
LC,08,0~7,0A,Screen 2/Line 2: Engine Power Wheel
LC,08,0~7,0B,Screen 2/Line 2: Engine Torque
LC,08,0~7,0C,Screen 2/Line 2: Engine Torque Loss
LC,08,0~7,0D,Screen 2/Line 2: Engine Torque Wheel
LC,08,0~7,0E,Screen 2/Line 2: Engine Pedal Position
LC,08,0~7,0F,Screen 2/Line 2: Engine Throttle Position
LC,08,0~7,10,Screen 2/Line 2: Wheel speed Front Left
LC,08,0~7,11,Screen 2/Line 2: Wheel speed Front Right
LC,08,0~7,12,Screen 2/Line 2: Wheel speed Back Left
LC,08,0~7,13,Screen 2/Line 2: Wheel speed Back Right
LC,08,0~7,14,Screen 2/Line 2: Brake Pressure
LC,08,0~7,15,Screen 2/Line 2: G across
LC,08,0~7,16,Screen 2/Line 2: Gierrate
LC,08,0~7,17,Screen 2/Line 2: Steering Angle
LC,08,0~7,18,Screen 2/Line 2: Haldex Clutch Open
LC,08,0~7,19,Screen 2/Line 2: Haldex Overtemp
LC,08,0~7,1A,Screen 2/Line 2: Haldex Transmitted Torque
LC,08,0~7,1B,Screen 2/Line 2: Haldex Oil Temperature
LC,08,0~7,1C,Screen 2/Line 2: Car Speed
LC,08,0~7,1D,Screen 2/Line 2: Fuel Content
LC,08,0~7,1E,Screen 2/Line 2: Voltage
LC,08,0~7,1F,Screen 2/Line 2: DSG Current Gear
; {Screen 2/Line 3}
LC,09,0~7,00,Screen 2/Line 3: Off
LC,09,0~7,01,Screen 2/Line 3: Engine Oil Temperature
LC,09,0~7,02,Screen 2/Line 3: Engine Intake Temperature
LC,09,0~7,03,Screen 2/Line 3: Engine Cooling Temperature
LC,09,0~7,04,Screen 2/Line 3: Outside Temperature
LC,09,0~7,05,Screen 2/Line 3: Engine RPM
LC,09,0~7,06,Screen 2/Line 3: Oil Pressure
LC,09,0~7,07,Screen 2/Line 3: Boost
LC,09,0~7,08,Screen 2/Line 3: Engine Power
LC,09,0~7,09,Screen 2/Line 3: Engine Power Loss
LC,09,0~7,0A,Screen 2/Line 3: Engine Power Wheel
LC,09,0~7,0B,Screen 2/Line 3: Engine Torque
LC,09,0~7,0C,Screen 2/Line 3: Engine Torque Loss
LC,09,0~7,0D,Screen 2/Line 3: Engine Torque Wheel
LC,09,0~7,0E,Screen 2/Line 3: Engine Pedal Position
LC,09,0~7,0F,Screen 2/Line 3: Engine Throttle Position
LC,09,0~7,10,Screen 2/Line 3: Wheel speed Front Left
LC,09,0~7,11,Screen 2/Line 3: Wheel speed Front Right
LC,09,0~7,12,Screen 2/Line 3: Wheel speed Back Left
LC,09,0~7,13,Screen 2/Line 3: Wheel speed Back Right
LC,09,0~7,14,Screen 2/Line 3: Brake Pressure
LC,09,0~7,15,Screen 2/Line 3: G across
LC,09,0~7,16,Screen 2/Line 3: Gierrate
LC,09,0~7,17,Screen 2/Line 3: Steering Angle
LC,09,0~7,18,Screen 2/Line 3: Haldex Clutch Open
LC,09,0~7,19,Screen 2/Line 3: Haldex Overtemp
LC,09,0~7,1A,Screen 2/Line 3: Haldex Transmitted Torque
LC,09,0~7,1B,Screen 2/Line 3: Haldex Oil Temperature
LC,09,0~7,1C,Screen 2/Line 3: Car Speed
LC,09,0~7,1D,Screen 2/Line 3: Fuel Content
LC,09,0~7,1E,Screen 2/Line 3: Voltage
LC,09,0~7,1F,Screen 2/Line 3: DSG Current Gear
; {Screen 2/Line 4}
LC,10,0~7,00,Screen 2/Line 4: Off
LC,10,0~7,01,Screen 2/Line 4: Engine Oil Temperature
LC,10,0~7,02,Screen 2/Line 4: Engine Intake Temperature
LC,10,0~7,03,Screen 2/Line 4: Engine Cooling Temperature
LC,10,0~7,04,Screen 2/Line 4: Outside Temperature
LC,10,0~7,05,Screen 2/Line 4: Engine RPM
LC,10,0~7,06,Screen 2/Line 4: Oil Pressure
LC,10,0~7,07,Screen 2/Line 4: Boost
LC,10,0~7,08,Screen 2/Line 4: Engine Power
LC,10,0~7,09,Screen 2/Line 4: Engine Power Loss
LC,10,0~7,0A,Screen 2/Line 4: Engine Power Wheel
LC,10,0~7,0B,Screen 2/Line 4: Engine Torque
LC,10,0~7,0C,Screen 2/Line 4: Engine Torque Loss
LC,10,0~7,0D,Screen 2/Line 4: Engine Torque Wheel
LC,10,0~7,0E,Screen 2/Line 4: Engine Pedal Position
LC,10,0~7,0F,Screen 2/Line 4: Engine Throttle Position
LC,10,0~7,10,Screen 2/Line 4: Wheel speed Front Left
LC,10,0~7,11,Screen 2/Line 4: Wheel speed Front Right
LC,10,0~7,12,Screen 2/Line 4: Wheel speed Back Left
LC,10,0~7,13,Screen 2/Line 4: Wheel speed Back Right
LC,10,0~7,14,Screen 2/Line 4: Brake Pressure
LC,10,0~7,15,Screen 2/Line 4: G across
LC,10,0~7,16,Screen 2/Line 4: Gierrate
LC,10,0~7,17,Screen 2/Line 4: Steering Angle
LC,10,0~7,18,Screen 2/Line 4: Haldex Clutch Open
LC,10,0~7,19,Screen 2/Line 4: Haldex Overtemp
LC,10,0~7,1A,Screen 2/Line 4: Haldex Transmitted Torque
LC,10,0~7,1B,Screen 2/Line 4: Haldex Oil Temperature
LC,10,0~7,1C,Screen 2/Line 4: Car Speed
LC,10,0~7,1D,Screen 2/Line 4: Fuel Content
LC,10,0~7,1E,Screen 2/Line 4: Voltage
LC,10,0~7,1F,Screen 2/Line 4: DSG Current Gear
; {Screen 2/Line 5}
LC,11,0~7,00,Screen 2/Line 5 (red display only): Off
LC,11,0~7,01,Screen 2/Line 5 (red display only): Engine Oil Temperature
LC,11,0~7,02,Screen 2/Line 5 (red display only): Engine Intake Temperature
LC,11,0~7,03,Screen 2/Line 5 (red display only): Engine Cooling Temperature
LC,11,0~7,04,Screen 2/Line 5 (red display only): Outside Temperature
LC,11,0~7,05,Screen 2/Line 5 (red display only): Engine RPM
LC,11,0~7,06,Screen 2/Line 5 (red display only): Oil Pressure
LC,11,0~7,07,Screen 2/Line 5 (red display only): Boost
LC,11,0~7,08,Screen 2/Line 5 (red display only): Engine Power
LC,11,0~7,09,Screen 2/Line 5 (red display only): Engine Power Loss
LC,11,0~7,0A,Screen 2/Line 5 (red display only): Engine Power Wheel
LC,11,0~7,0B,Screen 2/Line 5 (red display only): Engine Torque
LC,11,0~7,0C,Screen 2/Line 5 (red display only): Engine Torque Loss
LC,11,0~7,0D,Screen 2/Line 5 (red display only): Engine Torque Wheel
LC,11,0~7,0E,Screen 2/Line 5 (red display only): Engine Pedal Position
LC,11,0~7,0F,Screen 2/Line 5 (red display only): Engine Throttle Position
LC,11,0~7,10,Screen 2/Line 5 (red display only): Wheel speed Front Left
LC,11,0~7,11,Screen 2/Line 5 (red display only): Wheel speed Front Right
LC,11,0~7,12,Screen 2/Line 5 (red display only): Wheel speed Back Left
LC,11,0~7,13,Screen 2/Line 5 (red display only): Wheel speed Back Right
LC,11,0~7,14,Screen 2/Line 5 (red display only): Brake Pressure
LC,11,0~7,15,Screen 2/Line 5 (red display only): G across
LC,11,0~7,16,Screen 2/Line 5 (red display only): Gierrate
LC,11,0~7,17,Screen 2/Line 5 (red display only): Steering Angle
LC,11,0~7,18,Screen 2/Line 5 (red display only): Haldex Clutch Open
LC,11,0~7,19,Screen 2/Line 5 (red display only): Haldex Overtemp
LC,11,0~7,1A,Screen 2/Line 5 (red display only): Haldex Transmitted Torque
LC,11,0~7,1B,Screen 2/Line 5 (red display only): Haldex Oil Temperature
LC,11,0~7,1C,Screen 2/Line 5 (red display only): Car Speed
LC,11,0~7,1D,Screen 2/Line 5 (red display only): Fuel Content
LC,11,0~7,1E,Screen 2/Line 5 (red display only): Voltage
LC,11,0~7,1F,Screen 2/Line 5 (red display only): DSG Current Gear
; {Screen 3/Line 1}
LC,12,0~7,00,Screen 3/Line 1: Off
LC,12,0~7,01,Screen 3/Line 1: Engine Oil Temperature
LC,12,0~7,02,Screen 3/Line 1: Engine Intake Temperature
LC,12,0~7,03,Screen 3/Line 1: Engine Cooling Temperature
LC,12,0~7,04,Screen 3/Line 1: Outside Temperature
LC,12,0~7,05,Screen 3/Line 1: Engine RPM
LC,12,0~7,06,Screen 3/Line 1: Oil Pressure
LC,12,0~7,07,Screen 3/Line 1: Boost
LC,12,0~7,08,Screen 3/Line 1: Engine Power
LC,12,0~7,09,Screen 3/Line 1: Engine Power Loss
LC,12,0~7,0A,Screen 3/Line 1: Engine Power Wheel
LC,12,0~7,0B,Screen 3/Line 1: Engine Torque
LC,12,0~7,0C,Screen 3/Line 1: Engine Torque Loss
LC,12,0~7,0D,Screen 3/Line 1: Engine Torque Wheel
LC,12,0~7,0E,Screen 3/Line 1: Engine Pedal Position
LC,12,0~7,0F,Screen 3/Line 1: Engine Throttle Position
LC,12,0~7,10,Screen 3/Line 1: Wheel speed Front Left
LC,12,0~7,11,Screen 3/Line 1: Wheel speed Front Right
LC,12,0~7,12,Screen 3/Line 1: Wheel speed Back Left
LC,12,0~7,13,Screen 3/Line 1: Wheel speed Back Right
LC,12,0~7,14,Screen 3/Line 1: Brake Pressure
LC,12,0~7,15,Screen 3/Line 1: G across
LC,12,0~7,16,Screen 3/Line 1: Gierrate
LC,12,0~7,17,Screen 3/Line 1: Steering Angle
LC,12,0~7,18,Screen 3/Line 1: Haldex Clutch Open
LC,12,0~7,19,Screen 3/Line 1: Haldex Overtemp
LC,12,0~7,1A,Screen 3/Line 1: Haldex Transmitted Torque
LC,12,0~7,1B,Screen 3/Line 1: Haldex Oil Temperature
LC,12,0~7,1C,Screen 3/Line 1: Car Speed
LC,12,0~7,1D,Screen 3/Line 1: Fuel Content
LC,12,0~7,1E,Screen 3/Line 1: Voltage
LC,12,0~7,1F,Screen 3/Line 1: DSG Current Gear
; {Screen 3/Line 2}
LC,13,0~7,00,Screen 3/Line 2: Off
LC,13,0~7,01,Screen 3/Line 2: Engine Oil Temperature
LC,13,0~7,02,Screen 3/Line 2: Engine Intake Temperature
LC,13,0~7,03,Screen 3/Line 2: Engine Cooling Temperature
LC,13,0~7,04,Screen 3/Line 2: Outside Temperature
LC,13,0~7,05,Screen 3/Line 2: Engine RPM
LC,13,0~7,06,Screen 3/Line 2: Oil Pressure
LC,13,0~7,07,Screen 3/Line 2: Boost
LC,13,0~7,08,Screen 3/Line 2: Engine Power
LC,13,0~7,09,Screen 3/Line 2: Engine Power Loss
LC,13,0~7,0A,Screen 3/Line 2: Engine Power Wheel
LC,13,0~7,0B,Screen 3/Line 2: Engine Torque
LC,13,0~7,0C,Screen 3/Line 2: Engine Torque Loss
LC,13,0~7,0D,Screen 3/Line 2: Engine Torque Wheel
LC,13,0~7,0E,Screen 3/Line 2: Engine Pedal Position
LC,13,0~7,0F,Screen 3/Line 2: Engine Throttle Position
LC,13,0~7,10,Screen 3/Line 2: Wheel speed Front Left
LC,13,0~7,11,Screen 3/Line 2: Wheel speed Front Right
LC,13,0~7,12,Screen 3/Line 2: Wheel speed Back Left
LC,13,0~7,13,Screen 3/Line 2: Wheel speed Back Right
LC,13,0~7,14,Screen 3/Line 2: Brake Pressure
LC,13,0~7,15,Screen 3/Line 2: G across
LC,13,0~7,16,Screen 3/Line 2: Gierrate
LC,13,0~7,17,Screen 3/Line 2: Steering Angle
LC,13,0~7,18,Screen 3/Line 2: Haldex Clutch Open
LC,13,0~7,19,Screen 3/Line 2: Haldex Overtemp
LC,13,0~7,1A,Screen 3/Line 2: Haldex Transmitted Torque
LC,13,0~7,1B,Screen 3/Line 2: Haldex Oil Temperature
LC,13,0~7,1C,Screen 3/Line 2: Car Speed
LC,13,0~7,1D,Screen 3/Line 2: Fuel Content
LC,13,0~7,1E,Screen 3/Line 2: Voltage
LC,13,0~7,1F,Screen 3/Line 2: DSG Current Gear
; {Screen 3/Line 3}
LC,14,0~7,00,Screen 3/Line 3: Off
LC,14,0~7,01,Screen 3/Line 3: Engine Oil Temperature
LC,14,0~7,02,Screen 3/Line 3: Engine Intake Temperature
LC,14,0~7,03,Screen 3/Line 3: Engine Cooling Temperature
LC,14,0~7,04,Screen 3/Line 3: Outside Temperature
LC,14,0~7,05,Screen 3/Line 3: Engine RPM
LC,14,0~7,06,Screen 3/Line 3: Oil Pressure
LC,14,0~7,07,Screen 3/Line 3: Boost
LC,14,0~7,08,Screen 3/Line 3: Engine Power
LC,14,0~7,09,Screen 3/Line 3: Engine Power Loss
LC,14,0~7,0A,Screen 3/Line 3: Engine Power Wheel
LC,14,0~7,0B,Screen 3/Line 3: Engine Torque
LC,14,0~7,0C,Screen 3/Line 3: Engine Torque Loss
LC,14,0~7,0D,Screen 3/Line 3: Engine Torque Wheel
LC,14,0~7,0E,Screen 3/Line 3: Engine Pedal Position
LC,14,0~7,0F,Screen 3/Line 3: Engine Throttle Position
LC,14,0~7,10,Screen 3/Line 3: Wheel speed Front Left
LC,14,0~7,11,Screen 3/Line 3: Wheel speed Front Right
LC,14,0~7,12,Screen 3/Line 3: Wheel speed Back Left
LC,14,0~7,13,Screen 3/Line 3: Wheel speed Back Right
LC,14,0~7,14,Screen 3/Line 3: Brake Pressure
LC,14,0~7,15,Screen 3/Line 3: G across
LC,14,0~7,16,Screen 3/Line 3: Gierrate
LC,14,0~7,17,Screen 3/Line 3: Steering Angle
LC,14,0~7,18,Screen 3/Line 3: Haldex Clutch Open
LC,14,0~7,19,Screen 3/Line 3: Haldex Overtemp
LC,14,0~7,1A,Screen 3/Line 3: Haldex Transmitted Torque
LC,14,0~7,1B,Screen 3/Line 3: Haldex Oil Temperature
LC,14,0~7,1C,Screen 3/Line 3: Car Speed
LC,14,0~7,1D,Screen 3/Line 3: Fuel Content
LC,14,0~7,1E,Screen 3/Line 3: Voltage
LC,14,0~7,1F,Screen 3/Line 3: DSG Current Gear
; {Screen 3/Line 4}
LC,15,0~7,00,Screen 3/Line 4: Off
LC,15,0~7,01,Screen 3/Line 4: Engine Oil Temperature
LC,15,0~7,02,Screen 3/Line 4: Engine Intake Temperature
LC,15,0~7,03,Screen 3/Line 4: Engine Cooling Temperature
LC,15,0~7,04,Screen 3/Line 4: Outside Temperature
LC,15,0~7,05,Screen 3/Line 4: Engine RPM
LC,15,0~7,06,Screen 3/Line 4: Oil Pressure
LC,15,0~7,07,Screen 3/Line 4: Boost
LC,15,0~7,08,Screen 3/Line 4: Engine Power
LC,15,0~7,09,Screen 3/Line 4: Engine Power Loss
LC,15,0~7,0A,Screen 3/Line 4: Engine Power Wheel
LC,15,0~7,0B,Screen 3/Line 4: Engine Torque
LC,15,0~7,0C,Screen 3/Line 4: Engine Torque Loss
LC,15,0~7,0D,Screen 3/Line 4: Engine Torque Wheel
LC,15,0~7,0E,Screen 3/Line 4: Engine Pedal Position
LC,15,0~7,0F,Screen 3/Line 4: Engine Throttle Position
LC,15,0~7,10,Screen 3/Line 4: Wheel speed Front Left
LC,15,0~7,11,Screen 3/Line 4: Wheel speed Front Right
LC,15,0~7,12,Screen 3/Line 4: Wheel speed Back Left
LC,15,0~7,13,Screen 3/Line 4: Wheel speed Back Right
LC,15,0~7,14,Screen 3/Line 4: Brake Pressure
LC,15,0~7,15,Screen 3/Line 4: G across
LC,15,0~7,16,Screen 3/Line 4: Gierrate
LC,15,0~7,17,Screen 3/Line 4: Steering Angle
LC,15,0~7,18,Screen 3/Line 4: Haldex Clutch Open
LC,15,0~7,19,Screen 3/Line 4: Haldex Overtemp
LC,15,0~7,1A,Screen 3/Line 4: Haldex Transmitted Torque
LC,15,0~7,1B,Screen 3/Line 4: Haldex Oil Temperature
LC,15,0~7,1C,Screen 3/Line 4: Car Speed
LC,15,0~7,1D,Screen 3/Line 4: Fuel Content
LC,15,0~7,1E,Screen 3/Line 4: Voltage
LC,15,0~7,1F,Screen 3/Line 4: DSG Current Gear
; {Screen 3/Line 5}
LC,16,0~7,00,Screen 3/Line 5 (red display only): Off
LC,16,0~7,01,Screen 3/Line 5 (red display only): Engine Oil Temperature
LC,16,0~7,02,Screen 3/Line 5 (red display only): Engine Intake Temperature
LC,16,0~7,03,Screen 3/Line 5 (red display only): Engine Cooling Temperature
LC,16,0~7,04,Screen 3/Line 5 (red display only): Outside Temperature
LC,16,0~7,05,Screen 3/Line 5 (red display only): Engine RPM
LC,16,0~7,06,Screen 3/Line 5 (red display only): Oil Pressure
LC,16,0~7,07,Screen 3/Line 5 (red display only): Boost
LC,16,0~7,08,Screen 3/Line 5 (red display only): Engine Power
LC,16,0~7,09,Screen 3/Line 5 (red display only): Engine Power Loss
LC,16,0~7,0A,Screen 3/Line 5 (red display only): Engine Power Wheel
LC,16,0~7,0B,Screen 3/Line 5 (red display only): Engine Torque
LC,16,0~7,0C,Screen 3/Line 5 (red display only): Engine Torque Loss
LC,16,0~7,0D,Screen 3/Line 5 (red display only): Engine Torque Wheel
LC,16,0~7,0E,Screen 3/Line 5 (red display only): Engine Pedal Position
LC,16,0~7,0F,Screen 3/Line 5 (red display only): Engine Throttle Position
LC,16,0~7,10,Screen 3/Line 5 (red display only): Wheel speed Front Left
LC,16,0~7,11,Screen 3/Line 5 (red display only): Wheel speed Front Right
LC,16,0~7,12,Screen 3/Line 5 (red display only): Wheel speed Back Left
LC,16,0~7,13,Screen 3/Line 5 (red display only): Wheel speed Back Right
LC,16,0~7,14,Screen 3/Line 5 (red display only): Brake Pressure
LC,16,0~7,15,Screen 3/Line 5 (red display only): G across
LC,16,0~7,16,Screen 3/Line 5 (red display only): Gierrate
LC,16,0~7,17,Screen 3/Line 5 (red display only): Steering Angle
LC,16,0~7,18,Screen 3/Line 5 (red display only): Haldex Clutch Open
LC,16,0~7,19,Screen 3/Line 5 (red display only): Haldex Overtemp
LC,16,0~7,1A,Screen 3/Line 5 (red display only): Haldex Transmitted Torque
LC,16,0~7,1B,Screen 3/Line 5 (red display only): Haldex Oil Temperature
LC,16,0~7,1C,Screen 3/Line 5 (red display only): Car Speed
LC,16,0~7,1D,Screen 3/Line 5 (red display only): Fuel Content
LC,16,0~7,1E,Screen 3/Line 5 (red display only): Voltage
LC,16,0~7,1F,Screen 3/Line 5 (red display only): DSG Current Gear
;
;End of label files