;
; VCDS Label File
;
; Skoda Fabia/Roomster (5J)
;
; Component: J446 - Parking Aid (#76)
;
; P/N: 5J0-919-283-???
;
; includes measuring blocks, coding and adaptation
;
; created on 14/May/2008 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification: 14/May/2008
;
; requires VCDS 800.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,General
001,1,Resulting,Distance Front,Specification: Not Installed
001,2,Resulting,Distance Rear,Specification: 10...160 cm (255 cm = no obstacle recognized)
001,3,Vehicle Speed,,Range: 0.0...255.0 km/h
001,4,Sensor,Voltage Supply,Specification: 10.0...14.5 V
;
002,0,External Information
002,1,Reverese Gear,engaged,Range: Reverse: Yes/Reverse: No
002,2,Trailer hitched,,Range: YES/NO/Not Installed
002,3,Sound Output,Suppressed (Park),Range: OFF/ON
002,4,Parking Aid,Button (E266),Range: ON/OFF/Not Oper./Not Installed
;
004,0,Distance (Rear)
004,1,Rear Left (G203),Sensor,Specification: 10...60 cm (255 cm = no obstacle recognized)
004,2,Rear Left (G204),Center Sensor,Specification: 10...160 cm (255 cm = no obstacle recognized)
004,3,Rear Right (G205),Center Sensor,Specification: 10...160 cm (255 cm = no obstacle recognized)
004,4,Rear Right (G206),Sensor,Specification: 10...60 cm (255 cm = no obstacle recognized)
;
008,0,Confirmation Sound && Indirect Echo
008,1,Confirm. Sound,(Reverse Gear),Range: ON/OFF
008,2,Indirect Echo,RR to RCR,255cm = no obstacle recognized
008,3,Indirect Echo,RCR zu RCL,255cm = no obstacle recognized
008,4,Indirect Echo,RCL zu RL,255cm = no obstacle recognized
;
010,0,Volume && Frequency
010,1,Rear Buzzer,Volume,Range: 0.0...100.0 %
010,2,Rear Buzzer,Frequency,Range: 0...2000 Hz
;
011,0,Volume && Frequency (Factory Setting)
011,1,Rear Buzzer,Volume,Range: 0.0...100.0 %
011,2,Rear Buzzer,Frequency,Range: 0...2000 Hz
;
080,0,Advanced Control Module Identification I
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Parking Aid (J446) Coding
C01,00?xx20: Confirmation
C02,0 = Confirmation when engaging Reverse Gear active
C03,1 = Confirmation when engaging Reverse Gear inactive
C04,00x?x20: Trailer Hitch
C05,0 = Trailer Hitch not installed
C06,1 = Trailer Hitch installed
C07,00xx?20: Transmission
C08,0 = Manual Transmission
C09,1 = Automatic Transmission
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A001,0,Rear Buzzer Volume
A001,5,Rear Buzzer Volume
A001,6,Adaptation of the rear warning buzzer volume.
A001,7, 
A001,8,Range: 0...94
A001,9,Standard: 50
;
