;
; VCDS Label File
;
; Copyright © 2018+ Ross-Tech, LLC
;
; Audi Q7 (4L)
;
; Component: J197 - Level Control (#34)
;
; P/N: 4L0-910-553-???
;
; Includes measured value blocks, basic setting, adaptation, coding,
; Access authorization and selective actuator diagnostics
;
; created on 23/Nov/2006 by Sebastian Stange (sst@plangarage.de)
; translated on XX/XX/2018 by Richard Lukins/FioranoCars.com (Richard@Fioranocars.com)
; updated on 17/Oct/2018 by Sebastian Stange (sst@plangarage.de)
;
; Last modified on 16.07.2009
;
; Requires VCDS 805.1 or later
;
;
; ------------------------------------------------- -
;
; measuring value blocks & basic settings
;
; ------------------------------------------------- -
;
;
001,0, General
001,1, voltage, (terminal 15), setpoint: 8.5 ... 15.5 V
001,2, voltage, (terminal 30), setpoint: 8.5 ... 15.5 V
001,3,Vehicle Speed
001,4,Status,Terminal 50,Range: Term. 50 OFF/Term. 50 ON
;
002,1, doors ,, range of values: door open / door closed / non-plausible
002,2, tailgate ,, Value range: flap on / flap closed / non-plausible
002,3,Level Sensor Right,Supply Voltage,Range: 0.0...6.375 V\nSpecification: 4.875...5.125 V
002,4,Level Sensor Left,Supply Voltage,Range: 0.0...6.375 V\nSpecification: 4.875...5.125 V
;
003,1, longitudinal fitting, adjustment
003,2, transverse adjustment, adjustment
003,4, compressor relay, value range: Relay ON / Relay OFF
;
004,0, height deviation from normal level
004,1, deviation, front left, value range: -127.0 ... + 128.0 mm
004,2, deviation, front right, value range: -127.0 ... + 128.0 mm
004,3, deviation, rear left, value range: -127.0 ... + 128.0 mm
004,4, deviation, rear right, value range: -127.0 ... + 128.0 mm
;
005,0, vehicle height (wheel center to mudguard)
005,1, vehicle height, front left, value range: 0.0..535.5 mm
005,2, vehicle height, front right, value range: 0.0..535.5 mm
005,3, vehicle height, rear left, value range: 0.0..535.5 mm
005,4, Vehicle height, rear right, value range: 0.0..535.5 mm
;
006,1, compressor, temperature, range of values: -40.0 ... + 140.0 ° C
006,2, pressure sensor ,, value range: 0.0 ... 20.0 bar
006,3, Discharge, solenoid valve, value range: On / Off
006,4, pressure accumulator, solenoid valve, range: On / Off
;
007,0, Status of pneumatic spring valves
007,1, air spring valve, front left, value range: On / Off
007,2, air spring valve, front right, value range: On / Off
007,3, air spring valve, rear left, value range: On / Off
007,4, air spring valve, rear right, value range: On / Off
;
010,0, height deviation of control position
010,1, deviation, front left, value range: -127.0 ... + 128.0 mm
010,2, deviation, front right, value range: -127.0 ... + 128.0 mm
010,3, deviation, rear left, value range: -127.0 ... + 128.0 mm
010,4, deviation, rear right, value range: -127.0 ... + 128.0 mm
;
011,0, damper valve flow
011,1, damper valve flow, front left, value range: 0.000 ... 2.050 A
011,2, damper valve flow, front right, value range: 0.000 ... 2.050 A
011,3, damper valve flow, rear left, value range: 0.000 ... 2.050 A
011,4, damper valve current, rear right, value range: 0.000 ... 2.050 A
;
012,0, build-up acceleration
012,1, set-up address, front left, value range: 0.0 ... 5.1 V \ nPollution value: 2.3 ... 2.6 V
012,2, set-up delay, front right, value range: 0.0 ... 5.1 V \ nRegulation: 2.3 ... 2.6 V
012,3, set-up position, rear, value range: 0.0 ... 5.1 V \ nRegulation: 2.3 ... 2.6 V
012,4, steering angle, sensor (G85)
;
013,0, damper speed
013,1, damper speed, front left
013,2, damper speed, front right
013,3, damper speed, rear left
013,4, damper speed, rear right
;
014,1, damper detection ,, 0 = Comfort \ n1 = Dynamics \ n2 = Automatic
014,2, emergency running status ,, 0 = no emergency run
014,3, Limitation, brake engagement, value range: 0.0 ... 100.0%
014,4, Limitation, longitudinal acceleration, value range: 0.0 ... 100.0%
;
B015,0, approach normal level
B015,1,,,
B015,2,,,
B015,3,,,
B015,4,,,
;
B017,0, Disable system function test
B017,1,,,
B017,2,,,
B017,3,,,
B017,4,,,
;
B020,0, bleed the accumulator
B020,1,,,
B020,2,,,
B020,3,,,
B020,4,,,
;
B021,0, bleed the front axle
B021,1,,,
B021,2,,,
B021,3,,,
B021,4,,,
;
B022,0, ventilate the rear axle
B022,1,,,
B022,2,,,
B022,3,,,
B022,4,,,
;
B023,0, ventilate pressure reservoir
B023,1,,,
B023,2,,,
B023,3,,,
B023,4,,,
;
B024,0, aerate the front axle
B024,1,,,
B024,2,,,
B024,3,,,
B024,4,,,
;
B025,0, aerate the rear axle
B025,1,,,
B025,2,,,
B025,3,,,
B025,4,,,
;
120,0, CAN data bus Time overshoot (drive)
120,1, brake electronics, (J104)
120,2, motor electronics
120,3, steering angle sensor, (G85)
120,4, Optional
;
121,0, CAN data bus Time overshoot (drive)
121,1, CAN gateway, (J533)
;
125,0, CAN data bus Communication (drive)
125,1, brake electronics, (J104)
125,2, engine electronics
125,3, steering angle sensor, (G85)
125,4, Optional
;
126,0, CAN data bus Communication (drive)
126,1, CAN gateway, (J533)
;
;
;---------------------------------------------------
;
; Coding
;
;---------------------------------------------------
;
;
C00, level control (J197) coding
C01,00155?0: Trailer Electronics
C02,1 = Trailer Electronics NOT installed
C03,2 = Trailer Electronics installed
;
;
;---------------------------------------------------
;
; Access authorization
;
;---------------------------------------------------
;
;
S00,Level Control (J197) Security Access
S01,08367 = Unlocking basic setting
S02,30419 = Unlocking pressure accumulator test (self-acting actuator diagnostics)
S03,31564 = Enabling adjustment
S04,
S05,10273 = Activate the loading mode
S06,41172 = Disable loading mode;
;
;---------------------------------------------------
;
; Selective Output Test
;
;---------------------------------------------------
;
;
T142, front damping adjustment valve (N336)
T143, right front damping valve (N337)
T144, rear damping adjustment valve (N338)
T145, rear right damping valve (N339)
T367, front damping valve (N336): soft control (300 mA)
T368, valve for damping adjustment, front left (N336): Control hard (1000 mA)
T369, front right damper valve (N337): soft control (300 mA)
T370, valve for damping adjustment, right front (N337): Control hard (1000 mA)
T371, rear damping valve (N338): soft control (300 mA)
T372, rear damping valve (N338): Actuation hard (1000 mA)
T373, rear right damper control valve (N339): soft control (300 mA)
T374, rear right damper (N339): Actuation hard (1000 mA)
T459, Front display and control unit (J523)
T1399, relay for compressor level control (J403)
T1784, vehicle is lowered in front left
T1785, vehicle is lowered at the front right
T1786, vehicle is lowered at the rear left
T1787, vehicle is lowered rear right
T1825, pressure memory test
;
;
;---------------------------------------------------
;
; Adaptation
;
;---------------------------------------------------
;
;

A001,0, control position front left
A001,5, control position front left
A001,6, Measure the distance between the center of the wheel and the lower edge
A001,7, the wheel house. Enter the value in millimeters (mm)
A001,8, as a new adjustment value. After successful input
A001,9, continue with the front right wheel (channel 002).
;
A002,0, control position front right
A002,5, control position front right
A002,6, Measure the distance between the center of the wheel and the lower edge
A002,7, of the wheel house. Enter the value in millimeters (mm)
A002,8, as a new adjustment value. After successful input
A002,9, continue with the wheel at the rear left (channel 003).
;
A003,0, control position rear left
A003,5, control position rear left
A003,6, Measure the distance between the center of the wheel and the lower edge
A003,7, the wheel house. Enter the value in millimeters (mm)
A003,8, as a new adjustment value. After successful input
A003,9, continue with the rear right wheel (channel 004).
;
A004,0, control position rear right
A004,5, control position rear right
A004,6, Measure the distance between the center of the wheel and the lower edge
A004,7, the wheel house. Enter the value in millimeters (mm)
A004,8, as a new adjustment value. After successful input
A004,9, confirm the new control position (channel 005).
;
A005,0, confirm the control position
A005,5, confirm the control position
A005,6, To confirm the previously entered new control position
A005,7, save the value "1".
A005,8,
A005,9, then check the error memory and proceed to the
A005, 10, to individual levels by means of selector switch. Lastly measure
A005,11, re-check the height of each wheel and check the absolute
A005,12, Vehicle height in MWB 005.
;
A010,0, car lift mode
A010,1, level control
A010,2, Status
A010,5, car lift mode
A010,6, The car lift mode is preferably activated via the MMI.
A010,7, If it is activated via the MMI it can only be activated via the MMI
A010,8, can be deactivated again. Use of this adjustment channel
A010,9, is only permissible in case of an MMI defect.
A010,10,
A010,11,0 = Carriage mode active
A010,12,1 = Carriage mode inactive
;
;
;---------------------------------------------------
;
; misc
;
;---------------------------------------------------
;
;
W,VCR340003
;
