;
; VCDS Label File
;
; Copyright © 2007+ Ross-Tech, LLC
;
; VW Caddy (2K) / VW Golf/Jetta (1K/5M) / VW Passat (3C) / VW Touran (1T)
;
; Component: J412 - Telephone (#77) - UHV-Low
;
; P/N: 3C0-035-729-???
;
; includes measuring blocks, adaptation, coding and selective output test
;
; created on 11/Nov/2007 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 16/Sep/2013
;
; requires VCDS 11.11.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,General
001,1,Voltage,(Terminal 30),Specification: 9.0...15.0 V
001,3,Signal Strength
001,4,Signal Strength,,Range: 0.0...100.0 % / Not Recogn.
;
002,0,Telephone
002,1,Telephone
002,3,Connection,Status,Range: Connected / Not Connected
002,4,Network,Status,Range: Acquired / Not Acquired
;
003,0,Microphone
003,1,Microphone
003,2,Microphone,Status,Specification: OK
003,3,Microphone
003,4,Microphone,Current,Specification: 3.0...9.0 mA
;
004,0,Audio Outputs
004,1,Audio Output,Plus (+),
004,2,Status,Audio Output (+),Specification: OK
004,3,Audio Output,Minus (-)
004,4,Status,Audio Output (-),Specification: OK
;
005,0,Button for Roadside Assistance && Information Service
005,1,Roadside,Assistance Button
005,2,Roadside,Assistance Button,Range: Operated/Not Oper./Not Recogn.
005,3,Information,Service Button
005,4,Information,Service Button,Range: Operated/Not Oper./Not Recogn.
;
015,0,Bluetooth
015,1,Bluetooth
015,2,Bluetooth,Visibility,Range: visible/invisible
015,3,Bluetooth,Status
;
020,0,Cell Phone Cradle
020,1,Cell Phone,Cradle
020,2,Cell Phone,Cradle Status
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Telephone Preparation (J412) Coding
C01,00160?X: Infotainment System
C02,2 = Radio System
C03,4 = Radio/Navigation System
C04,00160X?: Mute (see TPI 2013408)
C05,1 = Mute (via Hardware 'Mute-Wire') OFF
C06,3 = Mute (via Hardware 'Mute-Wire') ON
;
;
;---------------------------------------------------
;
; selektive output test
;
;---------------------------------------------------
;
;
T851,Loudspeaker(s)
T1530,Radio Mute
T2793,Connected Bluetooth Devices
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A001,0,Basis Volume (Telephone)
A001,5,Basis Volume (Telephone)
A001,6,Standard Output Signal Level
A001,7, 
A001,8,0 = -6 dB / 3 = -3 dB / 5 = -1 dB / 6 = ±0 dB
A001,9,7 = +1 dB / 9 = +3 dB / 12 = +6 dB
;
A003,0,Basis Volume (Microphone)
A003,5,Basis Volume (Microphone)
A003,6,Standard Input Signal Level
A003,7, 
A003,8,0 = -6 dB / 3 = -3 dB / 5 = -1 dB / 6 = ±0 dB
A003,9,7 = +1 dB / 9 = +3 dB / 12 = +6 dB
;
A004,0,Afterrun Time
A004,3,Current,Afterrun Time
A004,5,Afterrun Time
A004,6,The time the mobile phone plate is active after "Ignition OFF".
A004,7,Range: 0...60 min
;
A005,0,Bluetooth-PassKey
A005,1,Bluetooth
A005,2,Current PassKey,Digit 1 & 2
A005,3,Current PassKey,Digit 3 & 4
A005,5,Bluetooth-PassKey
A005,6,Range: 0...9999
A005,7,Standard: 0000
;
A006,0,Bluetooth Connection cleanup
A006,5,Bluetooth Connection cleanup
A006,6,To delete old Bluetooth Connections
A006,7,save "1" as new value.
;
A008,0,Mute Delay
;
A009,0,Audio Output Delay
A009,2,Current,Delay Time
A009,5,Audio Output Delay
A009,6,Range: 0...12 ms (milli seconds)
;
A010,0,Bluetooth Visibility
A010,3,Current,Status
A010,5,Bluetooth Visibility
A010,6,0 = invisible
A010,7,1 = visible
;
A011,0,Language
A011,2,Current,Language
A011,5,Language
A011,5,262 = German
;
A020,0,Telephone Number Information Service
;
A021,0,Telephone Number Roadside Assistance
;
