;
; VCDS Label File
;
; Copyright © 2006+ Ross-Tech, LLC
;
; Component: J345 - Trailer (#69)
;
; P/N: 4F0-910-383-???
;
; includes measuring blocks, coding and selective output tests
;
; created on 08/Feb/2006 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 12/Oct/2012
;
; requires VCDS 10.6.3 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Inputs
001,1,Voltage,(Terminal 30)
001,2,Status Term. 30,(switched),Display Range: ON/OFF
001,3,Status Term. 15,(Emergency Run),Display Range: ON/OFF
;
002,0,Inputs
002,1,ECD/ACC,(ESP/ACC Braking),Display Range: ON/OFF
002,2,Brake Light Switch,,Display Range: ON/OFF
002,3,Brake Pressure,Switch,Display Range: ON/OFF
;
003,0,Outputs
003,1,Turn Signal,Rear Left,Display Range: ON/OFF
003,2,Turn Signal,Rear Right,Display Range: ON/OFF
003,3,Tail Light,Left,Display Range: ON/OFF
003,4,Tail Light,Right,Display Range: ON/OFF
;
004,0,Outputs
004,1,Brake Lights,,Display Range: ON/OFF
004,2,Back-Up Lights,,Display Range: ON/OFF
004,3,Rear Fog Lights,,Display Range: ON/OFF
004,4,Status Term. 30,(switched),Display Range: ON/OFF
;
007,0,Trailer Hitch
007,1,Hand Wheel,Contact Switch,Display Range: ON/OFF
007,2,Locking Pin,Contact Switch,Display Range: ON/OFF
007,3,Trailer Hitch,Status,Display Range: Locked/Unlocked
;
008,0,Input Signals
008,1,Status,Terminal 15,Display Range: ON/OFF
008,2,Status,Terminal X,Display Range: ON/OFF
008,3,Battery Managem.,Shut-Off Stage,Display Range: 0...6
008,4,Trailer,attached,Display Range: ON/OFF
;
009,0,Input Signals
009,1,Turn Signal,Left,Display Range: ON/OFF
009,2,Turn Signal,Right,Display Range: ON/OFF
009,3,Emergency Flasher,Warning Lights,Display Range: ON/OFF
;
010,0,Input Signals
010,1,Brake Light Switch,,Display Range: ON/OFF
010,2,Brake Test Switch,,Display Range: ON/OFF
010,3,Brake Pressure,Switch,Display Range: ON/OFF
;
011,0,Input Signals
011,1,Side Marking,Lights,Display Range: ON/OFF
011,2,Parking Light,Left,Display Range: ON/OFF
011,3,Parking Light,Right,Display Range: ON/OFF
;
012,0,Input Signals
012,1,Rear Fog Light,,Display Range: ON/OFF
012,2,Back-Up Light,,Display Range: ON/OFF
;
018,0,LED Status
018,1,LED Status,(green)
018,2,LED Status,(red)
;
019,0,LED Afterrun Time
019,1,LED Run-Time,(green)
019,2,LED Run-Time,(red)
;
080,0,Advanced Control Module Identification I
;
081,0,Advanced Control Module Identification II
;
082,0,Advanced Control Module Identification III
;
130,0,CAN-Databus Communication (Comfort)
130,1,Central Electronics,(J519),Display Range: E.Load.Crtl 1/E.Load.Crtl 0\nSpecification: E.Load.Crtl 1
130,2,Electrical,Ignition Lock,Display Range: El.Ign.Lock 1/El.Ign.Lock 0\nSpecification: El.Ign.Lock 1
130,3,CAN-Gateway,(J533),Display Range: Gateway 1/Gateway 0\nSpecification: Gateway 1
;
131,0,CAN-Databus Communication (Comfort)
131,1,Battery,Management,Display Range: Batt.Mgmt 1/Batt.Mgmt 0\nSpecification: Batt.Mgmt 1
;
;
;---------------------------------------------------
;
; selective output test information
;
;---------------------------------------------------
;
;
T1019,Relay (Terminal 30G)
T2562,Brake Lights (Trailer)
T2564,Tail Lights Left (Trailer - M60)
T2563,Tail Lights Right (Trailer - M61)
T2566,Turn Signals Left (Trailer - M62)
T2565,Turn Signals Right (Trailer - M63)
T2567,Rear Fog Lights (Trailer - M64)
T2568,Back-Up Lights (Trailer)
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Trailer (J345) Coding
C01,0000??x: Trailer Hitch
C02,00 = Trailer Hitch w/o Swivel Function and w/o Operating Button
C03,33 = Trailer Hitch with mechanical Swivel Function and with Hand Wheel
C04, 
C05,0000xx?: Country
C06,1 = Rest of World (RoW)
C07,2 = North America (USA/Canada)
C08,3 = Australia (AUS)
;
