;
; VCDS Label File
;
; Copyright © 2010-2011 Ross-Tech, LLC
;
; VW Transporter (7D)
;
; Component: J285 - Instrument Cluster (#17)
;
; P/N: 7D0-919-???-???
;
; includes measuring blocks, adaptation, coding,
;          login and service reset
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 7D-17.LBL
; 7D0-919-xxx-17.LBL
; 7D0-920-xx0-17.LBL
; 7D0-920-xx1-17.LBL
;
; created on 03/Dec/2010 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 07/Feb/2011
;
; requires VCDS 10.3 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,General
001,1,Vehicle Speed
001,2,Engine Speed
001,3,Oil Pressure,Switch 2,Range: Oil Pr. 2 <min / Oil Pr. 2 OK
001,4,Time
;
002,0,General
002,1,Odometer
002,2,Fuel Level
002,3,Fuel Sender,Resistance
002,4,Ambient,Temperature
;
003,0,General
003,1,Coolant,Temperature
;
050,0,General
050,1,Odometer
050,2,Engine Speed
050,4,Coolant,Temperature
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A02,0,Service Reminder
A02,5,Service Reminder
A02,6,Displayed Values:
A02,7,01 = Oil Service due
A02,8,10 = Inspection due
A02,9,11 = Oil Service & Inspection due
A02,10, 
A02,11,New Values:
A02,12,00 = Reset Oil Service & Inspection
A02,13,10 = Reset Oil Service
A02,14,01 = Reset Inspection
;
A003,0,Consumption Correction
A003,5,Consumption Correction
A003,6,Standard Value: 100 %
A003,7,Display Range: 85...115 %
A003,8,Increments: 1 %
A003,9, 
A003,10,Calculation based on volume per distance (e.g. l/100km):
A003,11,New Adaptation Value = Old Adaptation Value * Calculated Consumption / Old Display Value
A003,12,Calculation based on distance per volume (e.g. MPG):
A003,13,New Adaptation Value = Old Adaptation Value * Old Display Value / Calculated Consumption 
;
A004,0,Language
A004,5,Language
A004,6,1 = German
A004,7,2 = English
A004,8,3 = French
A004,9,4 = Italian
A004,10,5 = Spanish
A004,11,6 = Portuguese
;
A005,0,Service Reminder: Max. Distance to Oil Service "OIL"
A005,5,Service Reminder: Max. Distance to Oil Service "OIL" (in 1000 km)
A005,6,15 = 15.000 km (Standard)
;
A006,0,Service Reminder: Max. Distance to Inspection "INSP 01"
A006,5,Service Reminder: Max. Distance to Inspection "INSP 01" (in 1000 km)
A006,6,30 = 30.000 km (Standard)
;
A007,0,Service Reminder: Max. Time to Inspection "INSP 02"
A007,5,Service Reminder: Max. Time to Inspection "INSP 02" (in 10 Days)
A007,6,37 = 370 Days (Standard)
;
A009,0,Mileage/Odometer
A009,5,Mileage/Odometer
A009,6,Increments: 1 = 10 km or 1 = 10 mi
A009,7, 
A009,8,The distance can only be changed once until
A009,9,the current value is not over 100 km/62 mi.
A009,10, 
A009,11,NOTE: Perform Login first.
;
A010,0,Service Reminder: Distance to Oil Service "OIL"
A010,5,Service Reminder: Distance to Oil Service "OIL" (in 1000 km)
A010,6,15 = 15.000 km (Standard)
;
A011,0,Service Reminder: Distance to Inspection "INSP 01"
A011,5,Service Reminder: Distance to Inspection "INSP 01" (in 1000 km)
A011,6,30 = 30.000 km (Standard)
;
A012,0,Service Reminder: Time to Inspection "INSP 02"
A012,5,Service Reminder: Time to Inspection "INSP 02" (in 10 Days)
A012,6,37 = 370 Days (Standard)
;
A016,0,Distance Impulse Number
;
A030,0,Tank Characteristic (Fuel Level Sensor)
A030,5,Tank Characteristic (Fuel Level Sensor)
A030,6,This channel is used to set the fuel gauge reserve mark
A030,7,therfor fill the tank with 9 l of fuel and correct the
A030,8,needle to hit the reserve mark. This is a parallel shift
A030,9,of the tank characteristic.
A030,10, 
A030,11,Standard: 128
A030,12,Range: 120...136 (-2.0...+2.0 l)
A030,13,Increments: 1 = 1 Ohm = 1/4 l
;
;
;---------------------------------------------------
;
; login
;
;---------------------------------------------------
;
;
L00,Instrument Cluster (J285) Login
L01,13861 = Adaptation Enabling
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Instrument Cluster (J285) Coding
C01,??xxx: Equipment
C02,+01 = Brake Pad Warning installed
C03,+02 = Seatbelt Warning installed
C04,+04 = Washer Fluid Warning installed
C05,+16 = Navigation System installed
C06,xx?xx: Country
C07,1 = Europe (EU) / 2 = USA (US) / 3 = Canada (CDN) / 4 = Great Britain (GB)
C08,5 = Japan (JP) /6 = Saudi Arabia (SA) / 7 = Australia (AUS)

;
;
;---------------------------------------------------
;
; service reset
;
;---------------------------------------------------
;
;
RD,2,Service Reminder Status,1,
RD,5,Max. Distance to Oil Service "OIL",1000,DIST
RD,6,Max. Distance to Inspection "INSP 01",1000,DIST
RD,7,Max. Time to Inspection "INSP 02",1,Day(s)
RD,10,Remaining Distance to Oil Service "OIL",1000,DIST
RD,11,Remaining Distance to Inspection "INSP 01",1000,DIST
RD,12,Remaining Time to Inspection "INSP 02",1,Day(s)
;
RJ,0,0,Service Reset (Oil Service & Inspection),,
RJ,0,1,2,0
;
RJ,1,0,Service Reset (Oil Service),,
RJ,1,1,2,10
;
RJ,2,0,Service Reset (Inspection),,
RJ,2,1,2,1
;
RJ,3,0,Service Reset (Oil Service - Indivdual Channels),,
RJ,3,1,10,15
;
RJ,4,0,Service Reset (Inspection - Indivdual Channels),,
RJ,4,1,10,15
RJ,4,2,11,30
;
RJ,5,0,Service Reset (Oil Service & Inspektion - Indivdual Channels),,
RJ,5,1,10,15
RJ,5,2,11,30
RJ,5,3,12,37
;
