;
; VCDS Label File
;
; Copyright © 2008+ Ross-Tech, LLC
;
; VW Transporter (7H)
;
; Component: J519 - Central Electronics (#09)
;
; P/N: 7H0-937-049-???
;
; includes measuring blocks, (converted) coding and adaptation
;
; created on 23/May/2008 by Sebastian Stange (Sebastian@Ross-Tech.com)
; updated on 29/May/2015 by Sebastian Stange (Sebastian@Ross-Tech.com) // Converted Coding added
;
; last modification on 29/May/2015
;
; requires VCDS 14.10.2 / LCode 1.0.5.6 or newer
;
;
;---------------------------------------------------
;
; measuaring blocks
;
;---------------------------------------------------
;
;
001,0,Voltage Supply
001,1,Terminal S,,Range: ON/OFF
001,2,Terminal 50,,Range: ON/OFF
001,3,Terminal X,,Range: ON/OFF
001,4,Terminal 15,,Range: ON/OFF
;
002,0,Voltage Supply
002,1,Battery Voltage
002,2,Load Managem.,Intervention,Range: active/inactive
002,3,Blinker,,Range: OK/Not OK (9...15 V)
002,4,Wiper,,Range: OK/Not OK (9...15 V)
;
003,0,Voltage Supply
003,1,Rear Window,Heating,Range: OK/Not OK (9...15 V)
003,2,Horn,,Range: OK/Not OK (9...15 V)
003,3,Interior Light,,Range: OK/Not OK (9...15 V)
003,4,Mirror,Heating,Range: OK/Not OK (9...15 V)
;
004,0,Voltage Supply
004,1,Back-Up Light,,Range: OK/Not OK (9...15 V)
;
005,1,Blinker Switch,Left,Range: Operated/Not Oper.
005,2,Blinker Switch,Right,Range: Operated/Not Oper.
005,3,Emergency,Flasher Button,Range: Operated/Not Oper.
;
006,0,Wiper Switch
006,1,Wiper Switch,Interval,Range: Operated/Not Oper.
006,2,Wiper Switch,Stage 1,Range: Operated/Not Oper.
006,3,Wiper Switch,Stage 2,Range: Operated/Not Oper.
006,4,Wiper Switch,Potentiometer,Range (Interval Stage): 1/2/3/4
;
007,1,Windshield,Washer Pump,Range: Operated/Not Oper.
007,2,Horn,,Range: Operated/Not Oper.
007,3,Hood Contact,Switch,Range: Operated/Not Oper.
;
008,0,Door Contact Switch Status
008,1,Driver's Door,Contact Switch,Range: Door open/Door closed
008,2,Passenger Door,Contact Switch,Range: Door open/Door closed
008,3,Rear Left Door,Contact Switchs,Range: Door open/Door closed
008,4,Rear Right Door,Contact Switch,Range: Door open/Door closed
;
009,0,Rear Lid
009,1,Rear Lid,Pre-Latch,Range: Operated/Not Oper.
009,2,Rear Lid,Main-Latch,Range: Operated/Not Oper.
;
010,0,Buttons
010,1,Front Windshield,Heater Button,Range: Operated/Not Oper.
010,2,Front Rear Window,Heater Button,Range: Operated/Not Oper.
010,3,Heated Mirror,Button,Range: Operated/Not Oper.
010,4,Central Button,Interior Light,Range: Operated/Not Oper.
;
011,0,Cruise Control System (CCS)
011,1,CCS Switch,SET/(-),Range: Operated/Not Oper.
011,2,CCS Switch,RES/(+),Range: Operated/Not Oper.
011,3,CCS Main Switch,Cancel,Range: Operated/Not Oper.
011,4,CCS Main Switch,ON/OFF,Range: Operated/Not Oper.
;
012,1,Dimming,Terminal 58d,Range: 0.0...100.0 %
012,2,Windshield Wiper,End Position,Range: Operated/Not Oper.
012,3,Back-Up Light,Switch
;
013,1,Rain Sensor,,Range: OK/Not OK/Not Install.
013,2,P/N-Signal,(Autom. Transm.),Range: PN active/PN inactive
;
014,0,Electronic Load Management I
014,1,Maximum,Shut-Off Priority
;
015,0,Electronic Load Management II
015,1,Shut-Off Priority
015,2,Counter
015,3,Critical,Time Part
;
016,0,Electronic Load Management III
016,1,Load Managem.,Intervention
016,2,Engine Starts
;
080,0,Advanced Control Module Identification I
080,1,Identification
080,2,Revision
080,3,Production,Date
080,4,Manufacturer &,Test Stand Number
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Central Electric (J519) Coding
C01,+00001 = Heated Rear Window installed
C02,+00002 = Trailer Hitch installed
C03,+00004 = Interior Light with Terminal S installed
C04,+00008 = Heated Front Window/Windshield installed
C05,+00016 = Additional Rear Turn Signals (Roof) installed
C06,+00032 = Electronic Load Management active
C07,+00064 = Heated Rear View Mirrors installed
C08,+00128 = Heated Rear View Mirrors switched via Heated Rear Window
C09,+00256 = Rain Sensor installed
C10,+00512 = Headlight Washers installed
C11,+01024 = Electrical Fuel Pump Relay installed
C12, 
C13,Note #1: Coding Value is the Sum of the individual Options!
C14,Note #2: You can also use the Coding Assist/Helper!
;
;
;---------------------------------------------------
;
; converted coding
; (short coding displayed as long coding for easier modifications)
;
;---------------------------------------------------
;
;
LC,02,0,Heated Rear Window installed
LC,02,1,Trailer Hitch installed
LC,02,2,Interior Light with Terminal S installed
LC,02,3,Heated Front Window/Windshield installed
LC,02,4,Additional Rear Turn Signals (Roof) installed
LC,02,5,Electronic Load Management active
LC,02,6,Heated Rear View Mirrors installed
LC,02,7,Heated Rear View Mirrors switched via Heated Rear Window
LC,01,0,Rain Sensor installed
LC,01,1,Headlight Washers installed
LC,01,2,Electrical Fuel Pump Relay installed
LC,01,7=,Additional Coding Options can be found in Byte 02!
LC,00,3=,Coding Details can be found in Byte 01 && Byte 02!
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A001,0,Terminal 30G Deactivation/Reset
A001,5,Terminal 30G Deactivation/Reset
A001,6,Range: 1-253 (0.66...173 Minutes)
A001,7,Standard: 46 (30 Minutes)
;
A002,0,Front Windshield Heating Activation Time
A002,5,Front Windshield Heating Activation Time
A002,6,Range: 1...253 (0.66...173 Minutes)
A002,7,Standard: 15 (10 Minutes)
A002,8,Special: 254 (infinite)
;
A003,0,Mirror Heating Activation Time
A003,5,Mirror Heating Activation Time
A003,6,Range: 1...253 (0.66...173 Minutes)
A003,8,Standard: 254 (infinite)
;
A004,0,Rear Windshield Heating Activation Time
A004,5,Rear Windshield Heating Activation Time
A004,6,Range: 1...253 (0.66...173 Minutes)
A004,7,Standard: 15 (10 Minutes)
A004,8,Special: 254 (infinite)
;
A005,0,
;0
;
