;
; VCDS Label File
;
; Copyright © 2007+ planGarage.de for Ross-Tech, LLC
;
; Audi A4 (8D)
;
; Component: J285 - Instrument Cluster (#17)
;
; P/N: 8D0-920-???-???
;
; includes measuring blocks, adaptation, coding, login and service reset
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 8D-17.LBL
; 8D0-919-0xx-17.LBL  (MY 1995-1997)
; 8D0-919-xxx-17.LBL  (MY 1998-1999)
; 8D0-920-xxx-17.LBL  (MY 2000+)
;
; created on 27/Feb/2007 by Sebastian Stange (sst@plangarage.de)
;
; last modification on 11/Jan/2017
;
; requires VCDS 908.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,General
001,1,Vehicle Speed
001,2,Engine Speed
001,3,Oil Pressure,Switch 2,Range: Oil Pr. 2 <min / Oil Pr. 2 OK
001,4,Time
;
002,0,General
002,1,Odometer
002,2,Fuel Level
002,3,Fuel Sender,Resistance
002,4,Outside,Temperature
;
003,0,General
003,1,Coolant,Temperature
;
010,0,Adaptation Channels 30 && 09
010,1,Adaptation,Channel
010,2,Fuel Gauge,Sender 1,See Adaptation Channel 30
010,3,Adaptation,Channel
010,4,Mileage,,See Adaptation Channel 09
;
011,0,Adaptation Channels 04 && 03
011,1,Adaptation,Channel
011,2,Language,,See Adaptation Channel 04
011,3,Adaptation,Channel
011,4,Consumption,Correction,See Adaptation Channel 03
;
012,0,Adaptation Channels 40 && 41
012,1,Adaptation,Channel
012,2,Mileage,since Service,See Adaptation Channel 40
012,3,Adaptation,Channel
012,4,Time,since Service,See Adaptation Channel 41
;
013,0,Adaptation Channels 42 && 43
013,1,Adaptation,Channel
013,2,Minimum Mileage,to Service,See Adaptation Channel 42
013,3,Adaptation,Channel
013,4,Maximum Mileage,to Service,See Adaptation Channel 43
;
014,0,Adaptation Channel 44
014,1,Adaptation,Channel
014,2,Maximum Time,to Service,See Adaptation Channel 44
;
015,0,Adaptation Channels 45 && 46
015,1,Adaptation,Channel
015,2,Oil Quality,,See Adaptation Channel 45
015,3,Adaptation,Channel
015,4,Total,Consumption,See Adaptation Channel 46
;
016,0,Adaptation Channels 47 && 48
016,1,Adaptation,Channel
016,2,Soot Entry,,See Adaptation Channel 47
016,3,Adaptation,Channel
016,4,Thermal Load,,See Adaptation Channel 48
;
022,0,Immobilizer I
022,1,Engine Start,permitted,Specification: 1 = Yes\nRange: 0 = No / 1 = Yes
022,2,Engine (ECU),responds,Specification: 1 = Yes\nRange: 0 = No / 1 = Yes
022,3,Key Status,,Specification: 1 = Key OK\nRange: 0 = Key not OK / 1 = Key OK
022,4,Number of,adapted Keys,Specification: 1...8
;
023,0,Immobilizer II
023,1,Variable Code,authorized,Specification: 1 = Yes\nRange: 0 = No / 1 = Yes
023,2,Key Status,(Transponder),Range: 0 = not locked / 1 = locked
023,3,Fixed Code,authorized,Specification: 1 = Yes\nRange: 0 = No / 1 = Yes
023,4,Immobilizer,Status,Specification: 6 (Immobilizer adapted)
; 1 = End of Assembly Line: NEW (Delivery Condition of New Instrument Cluster)
; 2 = End of Assembly Line: VIN adapted
; 3 = End of Assembly Line: ECU adapted
; 4 = Customer Service: NEW (Delivery Condition of Replacement Instrument Cluster)
; 5 = Customer Service: Instrument Cluster adapted
; 6 = Customer Service: Keys adapted (Normal Condition)
; 7 = Customer Service: Key Adaptation active
;
024,0,Immobilizer III (Lock Time)
024,1,Lock-Time,Instrument Cluster
024,2,Lock-Time,Engine (ECU)
024,3,Lock-Time,Emergency Unlock
024,4,Lock-Time,Transponder
;
025,0,Immobilizer IV (Communication)
025,1,Immobilizer,Communication,0 = No Communication\n1 = via CAN-Databus\n2 = via W-Line
;
050,0,General
050,1,Odometer
050,2,Engine Speed
050,3,Oil Temperature
050,4,Coolant,Temperature
;
080,0,Advanced Control Module Identification I
;
081,0,Advanced Control Module Identification II
081,1,Vehicle Ident.,Number (VIN)
;
125,0,CAN-Databus Communication (Powertrain)
125,1,Engine,,Specification: Engine 1\nRange: Engine 0/Engine 1
125,2,Transmission,,Range: Transm. 0/Transm. 1
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Instrument Cluster (J285) Coding
C01,??xxx: Options
C02,+00 = No Options or Navigation III
C03,+02 = Seatbelt Warning active
C04,+16 = Navigation I & II
C05,xx?xx: Country
C06,0 = Germany (D) / 1 = Rest of World (Left Hand Drive - RoW)
C07,2 = USA (US) / 3 = Canada (CDN) / 4 = Great Britain (GB)
C08,5 = Japan (Left Hand Drive - JP) / 6 = Saudi Arabia (SA)
C09,7 = Australia (AUS) / 8 = Rest of World (Right Hand Drive - RoW)
C10,9 = Japan (Right Hand Drive - JP)
C11,xxx?x: Cylinder
C12,4 = 4-Cylinder
C13,6 = 6-Cylinder
C14,8 = 8-Cylinder
C15,xxxx?: Engine
C16,0 = TDI-Engine
C17,2 = 4-Cylinder and 6-Cylinder Gasoline-Engine
C18,3 = 8-Cylinder Gasoline-Engine
C19,4 = Turbo-Engine
;
;
;---------------------------------------------------
;
; login
;
;---------------------------------------------------
;
;
L00,Instrument Cluster (J285) Login
L01,13861 = Adaptation Enabling
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A002,0,Service Reminder
A002,5,Service Reminder
A002,6,0 = Service NOT Due
A002,7,1 = Service Due
A002,8, 
A002,9,To reset the service reminder save 0 as new value.
;
A003,0,Consumption Correction
A003,5,Consumption Correction
A003,6,Standard Value: 100 %
A003,7,Display Range: 85...115 %
A003,8,Increments: 1 %
A003,9, 
A003,10,Calculation based on volume per distance (e.g. l/100km):
A003,11,New Adaptation Value = Old Adaptation Value * Calculated Consumption / Old Display Value
A003,12,Calculation based on distance per volume (e.g. MPG):
A003,13,New Adaptation Value = Old Adaptation Value * Old Display Value / Calculated Consumption 
;
A004,0,Display Language
A004,1,Language
A004,5,Display Language for Messages and Navigation
A004,6,1 = German
A004,7,2 = English
A004,8,3 = French
A004,9,4 = Italian
A004,10,5 = Spanish
A004,11,6 = Portuguese
;
A009,0,Mileage/Odometer
A009,5,Mileage/Odometer
A009,6,Increments: 1 = 10 km or 1 = 10 mi
A009,9,The distance can only be changed once until
A009,10,the current value is not over 100 km/62 mi.
A009,11, 
A009,12,NOTE: Perform Login first.
;
A18,0,Auxiliary Heater
A18,5,Auxiliary Heater
A18,6,00 = Auxiliary Heater NOT installed
A18,7,01 = Auxiliary Heater installed (unrelated to Engine State)
A18,8,10 = Auxiliary Heater installed (related to Engine State)
;
A19,0,Additional Features
A19,5,Additional Features
A19,6,?x: Outside Temperature Display
A19,7,0 = Outside Temperature Display inactive
A19,8,1 = Outside Temperature Display active
A19,9,x?: Remote Clock
A19,10,0 = Remote Clock not installed
A19,11,1 = Remote Clock installed
;
A021,0,Immobilizer - Key Adaptation
A021,1,Number of
A021,2,currently
A021,3,adapted Keys
A021,5,Immobilizer - Key Adaptation
;
A030,0,Tank Characteristic (Fuel Level Sensor)
A030,5,Tank Characteristic (Fuel Level Sensor)
A030,6,This channel is used to set the fuel gauge reserve mark
A030,7,therfor fill the tank with x l of fuel and correct the
A030,8,needle to hit the reserve mark. This is a parallel shift
A030,9,of the tank characteristic.
A030,10, 
A030,11,Standard: 128
A030,12,Range: 120...136 (-2.0...+2.0 l)
A030,13,Increments: 1 = 1 Ohm = 1/4 l
;
A035,0,Speed Threshold
A035,5,Speed Threshold
A035,6,This value represents the speed threshold of the
A035,7,dynamic oil pressure system. The threshold can be
A035,8,raised in increments of 250 RPM.
;
A040,0,Mileage since Service
A040,5,Mileage since Service
A040,6,Increments: 1 = 100 km
;
A041,0,Time since Service
A041,5,Time since Service
A041,6,Increments: 1 = 1 day(s)
;
A042,0,Minimum Mileage to Service
A042,5,Minimum Mileage to Service
A042,6,Increments: 1 = 1000 km/mi
A042,7,00015 = Standard (15.000 km)
A042,8,or (if coded to miles)
A042,9,00009 = Rest of World (9.000 mi)
A042,10,00010 = USA (
;
A043,0,Maximum Mileage to Service
A043,5,Maximum Mileage to Service
A043,6,Increments: 1 = 1000 km/mi
A043,7,00015 = fixed Service Intervals (15.000 km - w/o Longlife)
A043,8,00030 = Gasoline Engines with flexible Service Intervals (30.000 km - with Longlife)
A043,9,00035 = 6-Cyl. Diesel Engines with flexible Service Intervals (35.000 km - with Longlife)
A043,10,00050 = 4-Cyl. Diesel Engines with flexible Service Intervals (50.000 km - with Longlife)
A043,11,or (if coded to miles)
A043,12,00009 = fixed Service Intervals (9.000 mi - Great Britain - w/o Longlife)
A043,13,00019 = Gasoline Engines with flexible Service Intervals (19.000 mi - with Longlife)
A043,14,00022 = 6-Cyl. Diesel Engines with flexible Service Intervals (22.000 mi - with Longlife)
A043,15,00031 = 4-Cyl. Diesel Engines with flexible Service Intervals (31.000 mi - with Longlife)
;
A044,0,Maximum Time to Service
A044,5,Maximum Time to Service
A044,6,Increments: 1 = 1 day(s)
A044,7,00365 = fixed Service Intervals (w/o Longlife)
A044,8,00730 = flexible Service Intervals (with Longlife)
;
A045,0,Oil Quality
A045,5,Oil Quality
A045,6,1 = fixed Service Intervals (w/o Longlife)
A045,7,2 = Gasoline Engines with flexible Service Intervals (with Longlife)
A045,8,3 = 6-Cyl. Diesel Engines with flexible Service Intervals (with Longlife)
A045,9,4 = 4-Cyl. Diesel Engines with flexible Service Intervals (with Longlife)
;
A046,0,Total Consumption
A046,5,Total Consumption
A046,6,This value does not represent the actual consumption
A046,7,but is rather an arithmetic value for the service interval display.
;
A047,0,Soot Entry
A047,5,Soot Entry
A047,6,Arithmetic value used to calculate the amount of soot in
A047,7,the engine oil referenced to a distance of 100 km and used
A047,8,as comparison value for the service interval display.
;
A048,0,Thermal Load
A048,5,Thermal Load
A048,6,Arithmetic value used to calculate the thermal stress of
A048,7,the engine oil referenced to a distance of 100 km and used
A048,8,as comparison value for the service interval display.
A048,9, 
A048,10,NOTE: When changing the adaptation channels 042-048 manually the
A048,11,adaptation channels 040-048 must be stored in the following order:
A048,12,45 > 42 > 43 > 44 > 40 > 41 > 46 > 47 > 48
;
A050,0,Immobilizer - Vehicle Data Learning
A050,5,Immobilizer - Vehicle Data Learning
;
A60,0,CAN-Databus Powertrain Participants
A60,5,CAN-Databus Powertrain Participants
A60,6,00000 = Engine and Instrument Cluster with Immobilizer II
A60,7,01025 = Engine and Instrument Cluster with Immobilizer III
A60,8,01027 = Engine/Transmission and Instrument Cluster with Immobilizer III
;
A62,0,CAN-Databus Infotainment Participants
A62,5,CAN-Databus Infotainment Participants
A62,6,+00001 = Radio (Symphony only)
A62,7,+00002 = Telephone OR Telematics (NAR)
A62,8,+00004 = Navigation System
A62,9,+00008 = Telematics (RoW)
;
;
;---------------------------------------------------
;
; service reset
;
;---------------------------------------------------
;
;
RD,2,Service Reminder Status,1,
RD,40,Mileage since Service,100,DIST
RD,41,Time since Service,1,Days
RD,42,Min Mileage to Service,1000,DIST
RD,43,Max Mileage to Service,1000,DIST
RD,44,Max Time to Service,1,Days
RD,45,Oil Quality,1,
RD,47,Soot Quantity,100,DIST
RD,48,Thermal Load,100,DIST
;
RJ,0,0,General Service Reset,,
RJ,0,1,2,0
;
