;
; VCDS Label File
;
; Copyright © 2005-2011 Ross-Tech, LLC
;
; Audi A3 (8PA)
;
; Component: J234 - Airbag 9.41 (#15)
;
; P/N: 8P0-959-655-???
;
; includes measuring blocks, security access and adaptation
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 8P-15.LBL
; 8P0-959-655-84.LBL (Airbag 8.4)
; 8P0-959-655-94.LBL (Airbag 9.41)
;
; created on 01/Aug/2005 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modificationon on 16/Jun/2011
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks & basic setting
;
;---------------------------------------------------
;
;
001,0,Igniter Status (Airbag && Tensioner)
001,1,Driver Airbag,Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
001,2,Passenger Airbag,Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
001,3,Driver Belt,Tensioner Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
001,4,Passenger Belt,Tensioner Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
B001,0,Seat Occupied Recognition Control Module (J706) Basic Setting
B001,1,Status, , 
B001,2, , , 
B001,3, , , 
B001,4, , , 
;
002,0,Igniter Status (Tensioner && Battery Disconnect)
002,1,Rear Left Belt,Tensioner Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
002,2,Rear Right Belt,Tensioner Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
002,3,Rear Center Belt,Tensioner Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
002,4,Battery Disconnect,Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
003,1,Voltage supply,,Display Range: Correct/Signal too Low/Signal too High
003,2,Seat Occupation,Detection Passenger,Display Range: Child Seat/Light Adult/Medium Adult/Heavy Adult/Not Occup./Short to Ground/Short to Plus/Not Installed
003,3,Belt Inquiry,Driver,Display Range: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
003,4,Belt Inquiry,Passenger,Display Range: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
;
004,0,Belt Inquiry (Rear)
004,1,Belt Inquiry,Rear Left,Display Range: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
004,2,Belt Inquiry,Rear Right,Display Range: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
004,3,Belt Inquiry,Rear Center,Display Range: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
;
005,0,Igniter Status (Side Airbag)
005,1,Front Left Side,Airbag Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
005,2,Front Right Side,Airbag Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
005,3,Rear Left Side,Airbag Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
005,4,Rear Right Side,Airbag Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
007,0,Igniter Status (Head Airbag)
007,1,Driver Head,Airbag Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
007,2,Passenger Head,Airbag Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
010,0,Key Switch Status
010,1,Key Switch,Passenger Airbag,Display Range: ON/OFF
010,2,Key Switch,(HW Path),Display Range: ON/OFF/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
010,3,Key Switch,(SW Path),Display Range: ON/OFF/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
011,0,Igniter Status (Airbag Stage 2 && Knee Airbag)
011,1,Driver Airbag,Igniter (Stage 2),Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
011,2,Passenger Airbag,Igniter (Stage 2),Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
011,3,Driver Knee,Airbag Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
011,4,Passenger Knee,Airbag Igniter,Display Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
016,0,Seat Occupation Recognition (J706)
016,1,Control Module,Serial: 1st/2nd digit
016,2,Control Module,Serial: 3rd/4th digit
016,3,Control Module,Serial: 5th digit
016,4,Control Module,Calibration
;
018,0,Seat Occupation Detection
018,1,Pressure Sensor
018,2,Belt Force Sensor
018,3,Acceleration Sensor
;
019,0,Workshop Codes
019,1,Workshop Code,(Last Coding),of seat occupation detection
019,2,Workshop Code,(Last 0 Calibration),of seat occupation detection
;
021,0,Igniter Resistance (Airbag && Tensioner)
021,1,Driver Airbag,Igniter,Specification: 2.1...5.6 Ohm
021,2,Passenger Airbag,Igniter,Specification: 1.6...5.6 Ohm
021,3,Driver Belt,Tensioner Igniter,Specification: 1.6...5.6 Ohm
021,4,Passenger Belt,Tensioner Igniter,Specification: 1.6...5.6 Ohm
;
022,0,Igniter Resistance (Tensioner && Battery)
022,1,Rear Left Belt,Tensioner Igniter,Specification: 1.6...5.6 Ohm
022,2,Rear Right Belt,Tensioner Igniter,Specification: 1.6...5.6 Ohm
022,3,Rear Center Belt,Tensioner Igniter,Specification: 1.6...5.6 Ohm
022,4,Battery Disconnect,Igniter,Specification: 1.6...5.6 Ohm
;
025,0,Igniter Resistance (Side Airbag)
025,1,Front Left Side,Airbag Igniter,Specification: 1.6...5.6 Ohm
025,2,Front Right Side,Airbag Igniter,Specification: 1.6...5.6 Ohm
025,3,Rear Left Side,Airbag Igniter,Specification: 1.6...5.6 Ohm
025,4,Rear Right Side,Airbag Igniter,Specification: 1.6...5.6 Ohm
;
027,0,Igniter Resistance (Head Airbag)
027,1,Driver Head,Airbag Igniter,Specification: 1.6...5.6 Ohm
027,2,Passenger Head,Airbag Igniter,Specification: 1.6...5.6 Ohm
;
031,0,Igniter Resistance (Airbag Stage 2 && Knee Airbag)
031,1,Driver Airbag,Igniter (Stage 2),Specification: 2.1...5.6 Ohm
031,2,Passenger Airbag,Igniter (Stage 2),Specification: 1.6...5.6 Ohm
031,3,Driver Knee,Airbag Igniter,Specification: 1.6...5.6 Ohm
031,4,Passenger Knee,Airbag Igniter,Specification: 1.6...5.6 Ohm
;
080,0,Advanced Control Module Identification I
;
125,0,CAN-Databus Communication (Powertrain)
125,1,Instrument Cluster,,Specification: Instruments 1
125,2,Brake Electronics,,Specification: ABS 1
;
225,0,CAN-Databus Time-Out (Powertrain)
225,1,Instrument Cluster
225,2,Brake Electronics
;
;
;---------------------------------------------------
;
; coding information
;
;---------------------------------------------------
;
;
C00,Airbag 9.41 (J234) Coding
C01,0?xxxxx: Battery Seperating (0 = not installed / 1 = installed [3.2l only])
C02,0x?xxxx: Stages (3 = North America Region (NAR) / 7 = Rest of World (RoW))
C03,0xx?xxx: Options
C04,0 = without Passenger Airbag Shut-Off (PR-4UE+9P0/9P1)
C05,0 = without Passenger Seat Occupation Detection (PR-4UB+9P1)
C06,1 = with Passenger Airbag Deactivation Key Switch with/without Belt Warning Driver Side (PR-4UF+9P0/9P1)
C07,2 = with Passenger Seat Occupation Detection and Airbag Disabled Warning Light (PR-4UB+9P5)
C08,3 = without Passenger Airbag Shut-Off and with Belt Warning Driver & Passenger Side (PR-4UE+9P3)
C09,4 = with Passenger Airbag Deactivation Key Switch and with Belt Warning Driver & Passenger Side (PR-4UF+9P3)
C10,0xxx?xx: Side Airbags
C11,1 = 2-Door: Front Side Airbags (PR-4X1)
C12,4 = 4-Door: Front Side Airbags (PR-4X1)
C13,5 = Front & Rear Side Airbags (PR-4X2)
C14,6 = Front Side Airbags with Head Airbags (PR-4X3)
C15,7 = Front & Rear Side Airbags with Head Airbags (PR-4X4)
C16,0xxxx?x: Belt Inquiry
C17,0 = North American Region (NAR) with Belt Inquiry (PR-9P5)
C18,0 = Rest of World (RoW) 2-Door (8P1) without Belt Inquiry Driver's Side (PR-9P0)
C19,1 = Rest of World (RoW) 4-Door (8PA) without Belt Inquiry Driver's Side (PR-9P0)
C20,1 = Rest of World (RoW) with Belt Inquiry Driver's Side (PR-9P1)
C21,2 = Rest of World (RoW) with Belt Inquiry Driver's & Passenger Side (PR-9P3)
C22,0xxxxx?: Belt Tensioner
C23,2 = Rest of World (RoW) / 5 = North America Region (NAR)
;
;
;---------------------------------------------------
;
; security access information
;
;---------------------------------------------------
;
;
S00,Airbag (J234) Security Access
S01,20324 = Seat Occupied Recognition Basic Setting/Zero Balancing
;
;
;---------------------------------------------------
;
; adaptation information
;
;---------------------------------------------------
;
;
A000,0,Seat Occupied Recognition Reset
A000,5,Seat Occupied Recognition Reset
A000,6,If a repair on the Seat Occupied Recognition
A000,7,has been performed a reset has to be performed too.
A000,8, 
A000,9,Prerequisites:
A000,10,* Seat in normal position.
A000,11,* Seat must NOT be occupied during the whole procedure.
A000,12,* Seatbelt must NOT be plugged in.
A000,13,* No faults in the system.
A000,14,* Interior temperature must be between 0 °C and 37 °C (32 °F and 98 °F).
A000,15, 
A000,16,NOTE: Perform Security Access first.
;
A001,0,Front Passenger Airbag Deactivation
A001,1,Front Passenger,Airbag
A001,2,Current Status
A001,3,Workshop Code
A001,5,Front Passenger Airbag Deactivation
A001,6,0 = Front Passenger Airbag enabled (Standard)
A001,7,1 = Front Passenger Airbag disabled
A001,8, 
A001,9,Note: Refer to Service Manual!
;
A002,0,Front Driver Airbag Deactivation
A002,1,Front Driver,Airbag
A002,2,Current Status
A002,3,Workshop Code
A002,5,Front Driver Airbag Deactivation
A002,6,0 = Front Driver Airbag enabled (Standard)
A002,7,1 = Front Driver Airbag disabled
A002,8, 
A002,9,Note: Refer to Service Manual!
;
A003,0,Front Passenger Side Airbag Deactivation
A003,1,Front Passenger,Side Airbag
A003,2,Current Status
A003,3,Workshop Code
A003,5,Front Passenger Side Airbag Deactivation
A003,6,0 = Front Passenger Side Airbag enabled (Standard)
A003,7,1 = Front Passenger Side Airbag disabled
A003,8, 
A003,9,Note: Refer to Service Manual!
;
A004,0,Front Driver Side Airbag Deactivation
A004,1,Front Driver,Side Airbag
A004,2,Current Status
A004,3,Workshop Code
A004,5,Front Driver Side Airbag Deactivation
A004,6,0 = Front Driver Side Airbag enabled (Standard)
A004,7,1 = Front Driver Side Airbag disabled
A004,8, 
A004,9,Note: Refer to Service Manual!
;
A005,0,Front Passenger Belt Tensioner Deactivation
A005,1,Front Passenger,Belt Tensioner
A005,2,Current Status
A005,3,Workshop Code
A005,5,Front Passenger Belt Tensioner Deactivation
A005,6,0 = Front Passenger Belt Tensioner enabled (Standard)
A005,7,1 = Front Passenger Belt Tensioner disabled
A005,8, 
A005,9,Note: Refer to Service Manual!
;
A006,0,Front Driver Belt Tensioner Deactivation
A006,1,Front Driver,Belt Tensioner
A006,2,Current Status
A006,3,Workshop Code
A006,5,Front Driver Belt Tensioner Deactivation
A006,6,0 = Front Driver Belt Tensioner enabled (Standard)
A006,7,1 = Front Driver Belt Tensioner disabled
A006,8, 
A006,9,Note: Refer to Service Manual!
;
A007,0,Front Passenger Head Airbag Deactivation
A007,1,Front Passenger,Head Airbag
A007,2,Current Status
A007,3,Workshop Code
A007,5,Front Passenger Head Airbag Deactivation
A007,6,0 = Front Passenger Head Airbag enabled (Standard)
A007,7,1 = Front Passenger Head Airbag disabled
A007,8, 
A007,9,Note: Refer to Service Manual!
;
A008,0,Front Driver Head Airbag Deactivation
A008,1,Front Driver,Head Airbag
A008,2,Current Status
A008,3,Workshop Code
A008,5,Front Driver Head Airbag Deactivation
A008,6,0 = Front Driver Head Airbag enabled (Standard)
A008,7,1 = Front Driver Head Airbag disabled
A008,8, 
A008,9,Note: Refer to Service Manual!
;
A011,0,Rear Passenger Belt Tensioner Deactivation
A011,1,Rear Passenger,Belt Tensioner
A011,2,Current Status
A011,3,Workshop Code
A011,5,Rear Passenger Belt Tensioner Deactivation
A011,6,0 = Rear Passenger Belt Tensioner enabled (Standard)
A011,7,1 = Rear Passenger Belt Tensioner disabled
A011,8, 
A011,9,Note: Refer to Service Manual!
;
A012,0,Rear Driver Belt Tensioner Deactivation
A012,1,Rear Driver,Belt Tensioner
A012,2,Current Status
A012,3,Workshop Code
A012,5,Rear Driver Belt Tensioner Deactivation
A012,6,0 = Rear Driver Belt Tensioner enabled (Standard)
A012,7,1 = Rear Driver Belt Tensioner disabled
A012,8, 
A012,9,Note: Refer to Service Manual!
;
A014,0,Pyrotechnic Igniter for Battery Separating Deactivation
A014,1,Pyrotechnic Igniter,Battery Separating
A014,2,Current Status
A014,3,Workshop Code
A014,5,Pyrotechnic Igniter for Battery Separating Deactivation
A014,6,0 = Battery Separating enabled (Standard)
A014,7,1 = Battery Separating disabled
A014,8, 
A014,9,Note: Refer to Service Manual!
;
A050,0,ESP-Data (Powertrain)
A050,1,Powertrain
A050,5,ESP-Data (Powertrain)
A050,6,1 = Front-Wheel-Drive (FWD)
A050,7,2 = All-Wheel-Drive (AWD)
;
