;
; VCDS Label File
;
; Copyright © 2008+ Ross-Tech, LLC
;
; Seat Leon/Toledo (1M) / Skoda Octavia (1U) / VW Bora/Golf (1J)
; VW New Beetle (1C/9C) / VW Passat (3B) / VW Polo Classic (9V)
;
; Component: J379 - Central Locking (#35) - Generation II (> MY 2001)
;
; P/N: 1C0-962-258-???
;
; includes measuring blocks, adaptation and coding
;
; This file is part of a label files package,
; make sure you have all of the following files.
;
; 1C-35.LBL
; 1C0-962-258-II.LBL
; 1C0-962-258-III.LBL
;
; created on 01/Jan/2008 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 15/Nov/2013
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Driver Door
001,1,Key Switch,Driver Door,Range: open/closed/not operated/implausible
001,2,Int. Door Handle,Driver Door,Range: lock/unlock/not operated/implausible
001,3,Lock Feedback,Driver Door,Range: locked/unlocked
001,4,Safe Feedback,Driver Door,Range: safe/not safe
;
002,0,Passenger Door
002,1,Key Switch,Passenger Door,Range: open/closed/not operated/implausible
002,2,Int. Door Handle,Passenger Door,Range: lock/unlock/not operated/implausible
002,3,Lock Feedback,Passenger Door,Range: locked/unlocked
002,4,Safe Feedback,Passenger Door,Range: safe/not safe
;
003,0,Door Rear Left/Right
003,1,Lock Feedback,Rear Right,Range: locked/unlocked
003,2,Safe Feedback,Rear Right,Range: safe/not safe
003,3,Lock Feedback,Rear Left,Range: locked/unlocked
003,4,Safe Feedback,Rear Left,Range: safe/not safe
;
004,0,Door Contact Switches
004,1,Door Contact,Driver Door,Range: Door open/Door Closed
004,2,Door Contact,Passenger Door,Range: Door open/Door Closed
004,3,Door Contact,Rear Left/Right,Range: Door open/Door Closed/Not Installed
;
005,1,Central Locking,Thermal Protection,Range: Yes/No
005,2,Vehicle Speed
005,3,Remote Control,Buttons,Range: 0 = Not Operated / 1 = Operated\n\n?xxx = Open\nx?xx = Close\nxx?x = Rear Lid\nxxx? = Panic
005,4,Interior Monitor.,Sensor,Range: Yes/No/Not Installed
;
006,1,Status,Terminal S,Range: operated/not operated
006,2,Key Number,,Range: 0...4 (0 = not operated)
006,3,Key Switch,Rear Lid,Range: Open/Closed/Not Oper./Implausible
006,4,Status,Terminal 15,Range: Term.15 ON/Term.15 OFF
;
007,1,Contact Switch,Engine Hood,Range: open/closed
007,2,Contact Switch,Rear Lid,Range: open/closed
007,3,Signal,Close Windows
007,4,Signal,Open Windows
;
008,1,Supply Voltage,(Terminal 30)
008,2,Rear Lid,Button/Handle,Range: Operated/Not Oper./Implausible
008,3,Interior Monitor.,Deactivation,Range: ON/OFF/not installed
;
009,1,Permanent code,known,Specification: OK/n.OK
009,2,Code within,effective range,Specification: OK/n.OK
009,3,Algorithm,,Specification: OK/n.OK
;
010,0,Alarm Source
;   2 = Interior Monitoring
;   4 = Engine Hood Contact Switch
;   8 = Ignition (Terminal 15)
;  16 = Rear Lid/Tailgate Contact Switch
;  32 = Door Contact Switch Rear Left/Right Door
;  64 = Door Contact Switch Passenger Door
; 128 = Door Contact Switch Driver Door
; 255 = No Alarm Source recognized
010,1,Last,Alarm Source,2 = Interior Monitoring\n4 = Engine Hood Contact Switch\n8 = Ignition (Terminal 15)\n16 = Rear Lid/Tailgate Contact Switch\n32 = Door Contact Switch Rear Left/Right Door\n64 = Door Contact Switch Passenger Door\n128 = Door Contact Switch Driver Door\n255 = No Alarm Source recognized
010,2,2nd to last,Alarm Source,2 = Interior Monitoring\n4 = Engine Hood Contact Switch\n8 = Ignition (Terminal 15)\n16 = Rear Lid/Tailgate Contact Switch\n32 = Door Contact Switch Rear Left/Right Door\n64 = Door Contact Switch Passenger Door\n128 = Door Contact Switch Driver Door\n255 = No Alarm Source recognized
010,3,3rd to last,Alarm Source,2 = Interior Monitoring\n4 = Engine Hood Contact Switch\n8 = Ignition (Terminal 15)\n16 = Rear Lid/Tailgate Contact Switch\n32 = Door Contact Switch Rear Left/Right Door\n64 = Door Contact Switch Passenger Door\n128 = Door Contact Switch Driver Door\n255 = No Alarm Source recognized
010,4,4th to last,Alarm Source,2 = Interior Monitoring\n4 = Engine Hood Contact Switch\n8 = Ignition (Terminal 15)\n16 = Rear Lid/Tailgate Contact Switch\n32 = Door Contact Switch Rear Left/Right Door\n64 = Door Contact Switch Passenger Door\n128 = Door Contact Switch Driver Door\n255 = No Alarm Source recognized
;
011,1,Immobilizer,key recognition,Specification: yes/no/not installed
011,2,Automatic,lock/unlock switch,Specification: operated/not oper./implausible
011,3,Rear,first detent,Specification: open/closed/not installed
;
;
;---------------------------------------------------
;
; Coding
;
;---------------------------------------------------
;
;
C00,Central Locking (J379) Coding
C01,00256 = 2 Doors with Selective Unlocking
C02,00257 = 2 Doors with Unlocking of all Doors
C03,04096 = 4 Doors with Selective Unlocking
C04,04097 = 4 Doors with Unlocking of all Doors
;
;
;---------------------------------------------------
;
; Adaptation
;
;---------------------------------------------------
;
;
A01,0,Remote control adaptation
A01,5,Remote control adaptation
A01,6,Enter the number of keys that should be adapted. Save.
A01,7, 
A01,8,Now press button 1 or 2 on every remote that
A01,9,should be adapted for at least 1 second.
A01,10, 
A01,11,Note #1: All keys must be adapted in one procedure.
A01,12,Note #2: Adaptation of all keys must not exceed 15 seconds.
;
A003,0,Auto-Lock
A003,5,Auto-Lock
A003,6,The doors will lock automatically when the
A003,7,vehicle reaches a speed of 15 km/h or 10 mph.
A003,8, 
A003,9,Specification: 0 = off/1 = on
;
A004,0,Auto-Unlock
A004,5,Auto-Unlock
A004,6,The doors will unlock automatically when the key
A004,7,is removed from the ignition switch.
A004,8, 
A004,9,Specification: 0 = off/1 = on
;
A005,0,Interior Monitoring
A005,5,Interior Monitoring
A005,6,Activation of interior monitoring system.
A005,7, 
A005,8,Specification: 0 = off/1 = on
;
A006,0,Unlock Horn
A006,5,Unlock Horn
A006,6,Horn beep when unlocking via remote control.
A006,7, 
A006,8,Specification: 0 = off/1 = on
;
A007,0,Lock Horn
A007,5,Lock Horn
A007,6,Horn beep when locking via remote control.
A007,7, 
A007,8,Specification: 0 = off/1 = on
;
A008,0,Unlock Blink
A008,5,Unlock Blink
A008,6,Blink when unlocking via remote control.
A008,7, 
A008,8,Specification: 0 = off/1 = on
;
A009,0,Lock Blink
A009,5,Lock Blink
A009,6,Blink when locking via remote control.
A009,7, 
A009,8,Specification: 0 = off/1 = on
;
A010,0,Country Setting
A010,5,Country Setting
A010,6,Country setting for alarm horn.
A010,7, 
A010,8,1 - Rest of World (RoW)
A010,9,2 - Germany
A010,10,3 - Great Britain
;
