;
; VCDS Label File
;
; Copyright © 2005+ Ross-Tech, LLC
;
; Audi A4 (8E2/8E5)
;
; Component: J519 - Central Electronics (#09)
;
; P/N: 8E0-907-279-???
;
; includes measuring blocks, adaptation and coding
;
; created by Eric Maurier (Eric@Ross-Tech.com // www.vag-com.fr)
; updated on 27/Sep/2004 by Sebastian Stange (Sebastian@Ross-Tech.com)
; updated on 25/Apr/2012 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 25/Apr/2012
;
; requires VCDS 11.11.3 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,(Output Signals)
001,1,Supply Voltage
001,2,Horn,,Range: ON/OFF
001,3,Status,Terminal 75,Range: ON/OFF
001,4,Headlight,Washer,Range: ON/OFF
;
002,0,Turn Signals (Output Signals)
002,1,Turn Signals,Front Left,Range: 0.0...100.0 %
002,2,Turn Signals,Rear Left,Range: 0.0...100.0 %
002,3,Turn Signals,Front Right,Range: 0.0...100.0 %
002,4,Turn Signals,Rear Right,Range: 0.0...100.0 %
;
003,0,Parking Lights (Output Signals)
003,1,Parking Light,Front Left,Range: 0.0...100.0 %
003,2,Parking Light,Rear Left,Range: 0.0...100.0 %
003,3,Parking Light,Front Right,Range: 0.0...100.0 %
003,4,Parking Light,Rear Right,Range: 0.0...100.0 %
;
004,0,(Output Signals)
004,1,High Beam,Left,Display Range: 0.0...100.0 %
004,2,High Beam,Right,Display Range: 0.0...100.0 %
004,3,License Plate,Light,Display Range: 0.0...100.0 %
004,4,Emergency Flasher,Illumination,Display Range: 0.0...100.0 %

5,0,Output signals: wipers,
5,1,Front wiper,
5,2,Front washer,
5,3,Rear wiper,
5,4,Rear washer,

6,0,Input signals,
6,1,Rotary,light switch
6,2,Warning button,activation, 
6,3,Terminal 75,
6,4,Wiper speed


7,0,Input signals on comfort bus,
7,1,High beams,
7,2,Flashing,
7,3,Turn signal L,
7,4,Turn signal R,


8,0,Input signals on comfort bus: wipers,
8,1,Front wiper,
8,2,Front washer,
8,3,Rear wiper,
8,4,Rear washer,

9,0,Input signals on comfort bus,
9,1,Terminal 15,
9,2,S Contact,
9,3,Speed interval,
9,4,Vacant,

10,0,Output signals (highline only),
10,1,Low beam left,
10,2,Low beam right,
10,3,Backup light,left
10,4,Backup light,right

11,0,Output signals (highline only),
11,1,Fog light FL,
11,2,Fog light FR,
11,3,Fog light rear,
11,4,Vacant,

12,0,Output signals (highline only),
12,1,Brake light,left
12,2,Brake light,right
12,3,Brake light,center
12,4,Vacant

13,0,Input signals (highline only),
13,1,Brake switch
13,2,Brake switch,(test)
13,3,Light sensor
13,4,Vacant

14,0,Input signals bus confort(highline only),
14,1,Driver`s door,open
14,2,Speed,
14,3,Outside temp,
14,4,Vacant,

080,0,Advanced Control Module Identification I
080,1,Identification
080,2,Revision
080,3,Production,Date
080,4,Manufacturer &,Test Stand Number
;
081,0,Advanced Control Module Identification II
081,1,Vehicle Ident.,Number (VIN)
081,2,Control Module,Serial Number
;
125,0,CAN-Databus Communication (Comfort)
125,1,Instrument Cluster,,Specification: Instruments 1
125,2,Steering Wheel,Electronics,Specification: St. Wheel 1
125,3,Comfort System,,Specification: Central 1
125,4,Trailer Electronics,,Specification: Trailer 1
;
126,0,CAN-Databus Communication (Comfort)
126,1,Door Electronics,Driver's Door,Specification: Dr. Door 1
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Central Electronics (J519) Coding
C01,0?xxx: Light Sensor
C02,0 = Light Sensor not installed
C03,1 = Light Sensor installed
C04,0x?xx: Trailer Hitch
C05,0 = Trailer Hitch not installed
C06,1 = Trailer Hitch installed
C07,0xx?x: Headlights
C08,0 = Halogen Headlights
C09,1 = Xenon Headlights
C10,0xxx?: Country
C11,1 = Rest of World
C12,2 = Northern Countries (Finland/Sweden/Norway/Denmark)
C13,3 = USA
C14,4 = Canada
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A001,0,Coming Home Activation Time
A001,5,Coming Home Activation Time
A001,6,Standard: 30 Seconds
A001,7,Range: 30...60 Seconds (Increments 1 s)
;
A002,0,Brake Light Dimming
A002,5,Brake Light Dimming
A002,6,Range: 0...100 %
A002,6,Standard (Limousine/Sedan): 24 %
A002,7,Standard (Wagon/Avant): 0 %
;
A081,0,Component Protection (Vehicle Identification Number)
A081,5,Component Protection (Vehicle Identification Number)
A081,6,To Start the Vehicle Identification Number (VIN)
A081,7,Learning Process enter/save 46992 as new Value.
;
