;
; VCDS Label File
;
; Copyright © 2005-2010 Ross-Tech, LLC
;
; Bentley Continental GT (3W) / VW Phaeton (3D) / VW Touareg (7L)
;
; Component: J518 - Access and Start Control Module aka. KESSY (#05)
;
; P/N: 3C0-909-13?-???
;                          
; created by Michael Moore (Moore@ross-tech.com), 'PanEuropean' on the VW Vortex forum.
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 3D-05.LBL
; 3D0-909-13x-05.LBL
;
; includes measured blocks, coding and coding-2
;
; created on 27/Mar/2005 by Michael
; updated on 25/Sep/2005 by Michael (Bentley Information added)
; updated on 11/Oct/2005 by Michael (checked against CSV and PLB, all blocks documented)
; updated on 16/Oct/2005 by Michael (MVB text enhanced and simplified, additional hover balloons added to MVBs)
; updated on 22/Feb/2006 by Michael (minor editorial corrections to improve balloon and MVB presentation, additional p/n added above)
;
; last modification on 05/Dec/2010
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measured blocks
;
;---------------------------------------------------
;
;
001,0,General Vehicle Electrical Status Information
001,1,Term 15 (Ignition),status,Possible Display: - Terminal 15 ON - Terminal 15 OFF
001,2,Terminal 15SV,status,Possible display: On or Off
001,3,Terminal 75X,status,Possible display: On or Off
001,4,Term 50 (Starter),status,Possible display: On or Off
;
002,0,Engine Start-Stop Keyswitch and/or Start-Stop Button Status
002,1,Start 1,switch status,Possible display: On or Off
002,2,Start 2,switch status,Possible display: On or Off
002,3,Stop 1,switch status,Possible display: On or Off
002,4,Stop 2,switch status,Possible display: On or Off
;
003,0,NOTE: Parking Lock (block 2) is not used on the Phaeton.
003,1,El Ign Lock Supply,Diagnosis,Possible display: On or Off
003,2,Parking Lock,status,,Possible display: On or Off
003,3,Emergency,start mode,Possible display: On or Off
;
004,0,Door Handle Touch Sensor Recognition (for Phaetons with keyless access)
004,1,G415,Driver Door,Possible display: Operated or Not Operated
004,2,G416,Passenger Door,Possible display: Operated or Not Operated
004,3,G417,Left Rear Door,Possible display: Operated or Not Operated
004,4,G418,Right Rear Door,Possible display: Operated or Not Operated
;
005,0,Elapsed Time Counter
;
006,0,Vehicle Key Status -  Click on all 4 block of the values to read decoding information.
006,1,Key 1,bit display,Bit 7 = Battery strength. Bit 6 = Key adapted. Bit 5 = Key blocked. 
006,2,Key 2,bit display,Bit 4 = not synchronized. Bit 3 = Trunk button pressed. Bit 2 = Panic button pressed. 
006,3,Key 3,bit display,Bit 1 = Unlock Button pressed. Bit 0 = Lock button pressed.
006,4,Key 4,bit display,Bits read like this - 76543210.
;
007,0,Radio Frequency Information
007,1,Radio amp, phantom powering,Possible display: On or Off
007,2,Radio range,reduction,Possible display: On or Off
;
008,0,Play protection counter capacitive sensor for Door Handle Touch Sensors (G415 = Driver, G416 = Front Passenger)
008,1,G415 rest period,for shut-off,
008,2,G416 rest period,for shut-off,
008,3,Cycle counter,driver door,
008,4,Cycle counter,both pax side doors
;
009,0,Play protection counter capacitive sensor for Door Handle Touch Sensors (see block 004 for locations)
009,1,G415 cycle,protection status,Possible display: On or Off
009,2,G416 cycle,protection status,Possible display: On or Off
009,3,G417 cycle,protection status,Possible display: On or Off
009,4,G418 cycle,protection status,Possible display: On or Off
;
010,0,Unknown value
;Could this report on keys in range? See blocks below from file 1J0-959-799-aj (credit to Mike Sauve) for possible ideas.
;13,0,remotes
;13,1,Permanent code
;13,2,Code in range
;13,3,Algorithm
10,4,Key number,(press remote),This may identify the key
;
022,0,Security Status
022,1,Start procedure,permitted,Yes = car can be driven  No = key is not or matched or incorrectly matched or the Engine Control Module is incorrectly adapted or malfunctioning
022,2,ECM,responding,,Yes = ECU communications OK (whether ECU is matched or not) No = not possible to match the Immo to the ECU at this time.
022,3,Key,condition OK,,Yes = a legitimate transponder code could be read (authorized or not) No = it will not be possible to match this particular key
022,4,Number of,adapted keys,A maximum of 8 adapted keys is permitted.
;
023,0,See Label File text for Block 23-4 decoding
; 0 - End of production original condition 1 - End of production new 20 - End of production programmed 21 - End of production 1.ECM adapted 22 - End of production 2.ECM adapted 23 - End of production 3.ECM adapted 24 - End of production 4.ECM adapted 30 - End of production ESCL adapted 3x - End of production x-th key adapated 4 - Service new 5 - Service programmed 6 - Immobilizer adapted 7 - ID sensor learning active 8 - ESCL adaptation 
023,1,Authentication,OK,Possible display: Yes or No
023,2,Lockbits,set,Possible display: Yes or No
023,3,Key ID,authorized,Possible display: Yes or No
023,4,Immobilizer,status,Please see the label file for decoding information.
;
024,0,Login Lockout times (all are displayed in minutes)
024,1,Immobilizer,minutes,
024,2,A-CAN,minutes
024,3,Scan protection,minutes (key)
024,4,After adaptation,minutes
;
025,0,ESCL Status
025,1,ESCL,authentication,Possible display: Valid or Not Valid
025,2,ESCL,access,Specified value:possible/not possible
;
026,0,Login Lock Status
026,1,ESL login lock,minutes,
026,2,Security access,lock (minutes)
;
027,0,ESCL Additional information (access to view this depends on value of block 25-2 above)
027,1,ESCL mode,,Possible display:0 - end of line mode/1 - normal mode/2 - adaptation mode/3 - analyze mode
027,2,ESCL unlocking bit,status,Possible display: On or Off
027,3,ESCL locking bit,status,Possible display: On or Off
027,4,ESCL error,status,Possible display:0 - no error/1 - system info/ 2 - internal error/3 - fatal error
;
050,0,Anti theft system status rear lid status
050,1,Anti theft,alarm status,Possible display: On or Off
050,3,Rear lid,lock status,Possible display: On or Off
;050,4,Unknown,(Valet Button?)
;
;Remark: This file supports Phaetons, Bentleys, and Touaregs.  'Rear Lid' can thus mean either 
;trunk lid or rear door, as is appropriate to the type of vehicle.
;
051,0,Driver Door Status
051,1,Door,Open,Possible display: On (door open) or Off (door closed)
051,2,Door,Locked,Possible display: On (door locked) or Off (door unlocked)
051,3,Door Safed,(ROW only),Possible display: On or Off (not applicable to NAR)
051,4,Window,regulator position,Possible display: - 0 to 100%  (0 = fully up, 100 = fully down)
;
052,0,Front Passenger Door Status
052,1,Door,Open,Possible display: On (door open) or Off (door closed)
052,2,Door,Locked,Possible display: On (door locked) or Off (door unlocked)
052,3,Door Safed,(ROW only),Possible display: On or Off (not applicable to NAR)
052,4,Window,regulator position,Possible display: - 0 to 100%  (0 = fully up 100 = fully down)
;
053,0,Left Rear Passenger Door Status
053,1,Door,Open,Possible display: On (door open) or Off (door closed)
053,2,Door,Locked,Possible display: On (door locked) or Off (door unlocked)
053,3,Door Safed,(ROW only),Possible display: On or Off (not applicable to NAR)
053,4,Window,regulator position,Possible display: - 0 to 100%  (0 = fully up 100 = fully down)
;
054,0,Right Rear Passenger Door Status
054,1,Door,Open,Possible display: On (door open) or Off (door closed)
054,2,Door,Locked,Possible display: On (door locked) or Off (door unlocked)
054,3,Door Safed,(ROW only),Possible display: On or Off (not applicable to NAR)
054,4,Window,regulator position,Possible display: - 0 to 100%  (0 = fully up 100 = fully down)
;
056,0,Time of Day (from vehicle clock)
056,1,Unknown,,
056,2,Hour,,
056,3,Minute,,
056,4,Second,,
;
057,0,General Vehicle Information
057,1,click block,for more info,The value here relates to whether the ignition circuit is on or off - might be if car is listening for key.
057,3,Vehicle,speed,Possible display:0 to 250 kilometers per hour
057,4,Gear lever,position,
;
058,0,Module Coding Status
058,1,Country,version
058,2,Engine,type
;
059,0,Solar Powered Ventilation (Parking Ventilation) status
059,1,Ventilation,status,Possible display: On or Off
;
060,0,Presumed to refer to Park Heating (stand-heating)
060,1,Park-heating,status
;
061,0,Sunroof Status
061,1,Sliding opening,range,Possible display: 0 = closed 1 - 2 - 3 - 4 - 5 = opened
061,2,Tilting opening,range,Possible display: 0 = closed 1 or 2 = opened
061,3,Function,slider open,Possible display: On or Off
061,4,Function,slider close,Possible display: On or Off
;
062,0,Status of Switches in Seat Belts
062,2,Driver Belt,switch status,Possible display: On or Off
062,3,Front Pax Belt,switch status,Possible display: On or Off
;
063,0,Diagnostic Bus Status
063,2,Diagnostic bus,Powertrain,Possible display: On or Off
063,3,Diagnostic bus,Comfort,Possible display: On or Off
;
080,0,Advanced Control Module Identification I
080,1,Advanced,Identification I
;
081,0,Advanced Control Module Identification II
081,1,Vehicle Ident.,Number (VIN)
;
082,0,Advanced Control Module Identification III
082,1,Advanced,Identification III
;
083,0,Advanced Control Module Identification IV
083,1,Advanced,Identification IV
;
090,1,Clutch switch,,Possible display:on (activated)/off (not activated)
090,2,Brake light,switch,Possible display:on (activated)/off (not activated)
090,4,Starter,enabling,Possible display: On or Off
;
091,1,Engine speed,RPM,Possible display:Between 0 and 7000 RPM
091,2,Gearlever,position
;
;
;---------------------------------------------------
;
; Coding-II
;
;---------------------------------------------------
;
;
L00,Access and Start Control (J518) Coding-II
L01,19795 = Coding Enabling
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Access and Start Control (J518) Coding
C01,
;C01,0133356 = USA + Keyless access + 5 speed transmission, W12 engine
;C02,0137452 = USA + Keyless access + 6 speed transmission, V8 engine
;C03,0002280 = USA + Central locking and remote control but no keyless + 5 speed transmission
;C04,0006376 = USA + Central locking and remote control but no keyless + 6 speed transmission
;C05,  
;C06,0213228 = Rest of World + Keyless access + 5 speed transmission + left hand drive vehicle
;C07,0218348 = Rest of World + Keyless access + 6 speed transmission + left hand drive vehicle
;C08,0004328 = Rest of World + Central locking and remote control but no keyless + 6 speed transmission + left hand drive vehicle
;C09,0000232 = Rest of World + Central locking and remote control but no keyless + 5 speed transmission + left hand drive vehicle
;
;C11,Other coding is possible for right hand drive vehicles or for Japan or for Taiwan. Contact Ross-Tech if you require it.
;C12,Touareg coding will follow a similar pattern, but with different numbers.
;C13,  
;C14,WARNING - Only the 'whole number' combinations shown above are possible. Do NOT attempt to increment or
;C15,decrement individual digits within the number. Make note of the pre-existing coding before you change anything.
;
