;
; VCDS Label File
;
; Copyright © 2005+ Ross-Tech, LLC
;
; Audi A8 (4E)
;
; Component: J234 - Airbag (#15) - 8.4+
;
; P/N: 4E0-910-655-???
;
; includes measuring blocks and coding
;
; created on 10/Oct/2005 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification on 20/Jul/2015
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Ignitiers I (Front Airbags Stage 1 && Front Belt Tensioners)
001,1,Airbag (Stage 1),Driver Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
001,2,Airbag (Stage 1),Passenger Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
001,3,Belt Tensioner,Front Driver Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
001,4,Belt Tensioner,Front Pass. Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
002,0,Ignitiers II (Rear Belt Tensioners)
002,1,Belt Tensioner,Rear Driver Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
002,2,Belt Tensioner,Rear Pass. Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
002,3,Belt Tensioner,Rear Center,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
003,0,Voltage && Belt Inquiry I (Front)
003,1,Voltage Supply,,Specification: Correct
003,3,Belt Inquiry,Front Driver Side,Specification: Not Installed/Belt Yes/Belt No\nDisplay Range: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
003,4,Belt Inquiry,Front Pass. Side,Specification: Not Installed/Belt Yes/Belt No\nDisplay Range: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
;
004,0,Belt Inquiry II (Rear)
004,1,Belt Inquiry,Rear Driver Side,Specification: Not Installed/Belt Yes/Belt No\nDisplay Range: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
004,2,Belt Inquiry,Rear Pass. Side,Specification: Not Installed/Belt Yes/Belt No\nDisplay Range: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
004,3,Belt Inquiry,Rear Center,Specification: Not Installed/Belt Yes/Belt No\nDisplay Range: Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed/Belt Yes/Belt No
;
006,0,Igniters III (Side Airbags)
006,1,Side Airbag,Front Driver Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
006,2,Side Airbag,Front Pass. Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
006,3,Side Airbag,Rear Driver Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
006,4,Side Airbag,Rear Pass. Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
008,0,Ingniters IV (Front Airbags Stage 2 && Head-Level Airbags)
008,1,Airbag (Stage 2),Front Driver Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
008,2,Airbag (Stage 2),Front Pass. Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
008,1,Head-Level Airbag,Driver Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
008,2,Head-Level Airbag,Passenger Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
009,0,Key Switch (Front Passenger Airbag)
009,1,Key Switch,Status,Display Range: ON/OFF
009,2,Key Switch,Software Status,Display Range: ON/OFF/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
009,3,Key Switch,Hardware Status,Display Range: ON/OFF/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
011,0,Ingniters V (Knee Airbags)
011,1,Knee Airbag,Front Driver Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
011,2,Knee Airbag,Front Pass. Side,Specification: Correct\nDisplay Range: Correct/Signal too Low/Signal too High/Short to Ground/Short to Plus/Not Installed
;
080,0,Advanced Control Module Identification I
080,1,Identification
080,2,Revision
080,3,Production,Date
080,4,Manufacturer &,Test Stand Number
;
125,0,CAN-Databus Powertrain (Communication)
125,1,Brake Electronics,,Specification: ABS 1
125,2,Instrument Cluster,,Specification: Instruments 1
;
225,0,CAN-Databus Powertrain (TimeOut)
225,1,Brake Electronics
225,2,Instrument Cluster
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Airbag 8.4 (J234) Coding
C01,0?3x70x: Options I
C02,4 = Knee Airbags NOT installed [PR-4UE/4UF]
C03,5 = Knee Airbags installed [PR-4UH/4UP]
C04,0x3?70x: Options II
C05,0 = Passenger Airbag Shut-Off NOT installed [PR-4UE/4UH+9P0/9P1]
C06,1 = Passenger Airbag Shut-Off via Key Switch installed [PR-4UF/4UP+9P0/9P1]
C07,2 = Passenger Airbag Shut-Off with Seat Occupation Detection installed [PR-4UH+9P5]
C08,0x3x70?: Belt Tensioner
C09,5 = Electrically Adjustable Single Seats installed [4-Seater / PR-5Z1]
C10,7 = Electrically Adjustable Single Seats NOT installed [5-Seater / PR-5Z0]
;
