;
; VAG-COM Label File
;
; Audi A2 (8Z) / Audi A4 (8E/8H) / Audi TT (8N)
;
; Component: J345 - Interior Monitoring (#45)
;
; includes measuring blocks, adaptation and coding
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 8H-45.LBL
; 8N-45.LBL
; 8Z-45.LBL
; 8E0-951-177.LBL
;
; created on 01/Jan/2007 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification: 01/Jan/2008
;
; requires VAG-COM 405.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,General
001,1,Communication,Status,0000 = Communication not OK\n0001 = Communication OK
001,2,Sensor,Sensitivity,Specification: 50.0...100.0 % (see Adaptation Channel 001)
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A001,0,Sensitivity
A001,5,Sensitivity
A001,6,Sensitivity settings of the ultra-sound sensors can
A001,7,be set so that the sensors react with less sensitivity
A001,8, 
A001,9,Standard: 100 (= 100 %)
A001,10,Range: 50...100 %
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Interior Monitoring (J345) Coding
C01,00001 = Standard
;
