;
; VCDS Label File
;
; Copyright © 2005-2010 Ross-Tech, LLC
;
; Seat Altea/Toledo (5P) / Skoda Octavia II (1Z)
; VW Caddy (2K) / VW Fox (5Z) / VW Golf/Jetta (1K) / VW Touran (1T) / VW Scirocco (13)
;
; Component: R - Radio (#56)
;
; includes measuring blocks, adaptation and coding
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 1K-56.LBL
; 1Z-56.LBL
; 5M-56.LBL
; 5P-56.LBL
; 5Z-56.LBL
; 7H-56.LBL
; 1K0-035-1xx-56.LBL
; 7H0-035-1xx-56.LBL
;
; created on 23/Mar/2005 by Sebastian Stange (Sebastian@Ross-Tech.com)
; updated on 30/Sep/2010 by Jille Berends (jjberends@gmail.com)
; updated on 04/Oct/2010 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 04/Oct/2010
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,General
001,1,Supply Voltage,(Terminal 30),Range: 0.0...20.0 V\nSpecification: 9.0...15.0 V
001,2,Amplifier,Output,only if Amplifier installed
001,3,Dimming,Terminal 58d (CAN),Range: 0.0...100.0 %\nSpecification: 29.0...98.0 %
001,4,Status,S-Contact (CAN),Range: ON/OFF
;
002,0,Telephone
002,1,Component
002,2,Mute Status
002,4,Status
;
003,0,Speaker/Line-Out (Front Left)
003,1,Location/Type
003,2,Status
;
004,0,Speaker/Line-Out (Front Right)
004,1,Location/Type
004,2,Status
;
005,0,Speaker/Line-Out (Rear Left)
005,1,Location/Type
005,2,Status
;
006,0,Speaker/Line-Out (Rear Right)
006,1,Location/Type
006,2,Status
;
007,0,Remote Feed Antenna I
007,1,Antenna Type
007,2,Component
007,3,Status
;
008,0,Signal Strength
008,1,Signal Strength
008,2,Signal Strength,Tuner I
008,3,Signal Strength
008,4,Signal Strength,Tuner II
;
010,0,Remote Feed Antenna II
010,1,Type
010,2,Component
010,3,Status
;
011,0,Communication Status CD-Changer (R41)
011,1,Component
011,2,Status
;
016,0,CAN Connection Satelite Radio Receiver (SDARS)
;
025,0,Internal Control Module Malfunctions
025,1,Control Module,Status,\n01 = Button(s) Jam\n02 = Checksum Error ROM/EPROM/Flash-ROM\n03 = Writing Error EEPROM\n04 = CC-Drive (Casette) Error\n05 = CD/DVD-Drive Error\n09 = Malfunction at CD/DVD-Drive\n0A = Internal Communication (BUS)
;
080,0,Advanced Control Module Identification I
;
081,0,Advanced Control Module Identification II
081,1,Serial Number
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A001,0,Reception Optimization
A001,5,Reception Optimization
A001,6,This channel allows optimization of the reception
A001,7,behavior for areas with strong FM interference.
A001,8, 
A001,9,0 = Normal reception
A001,10,1 = Optimized reception
;
A002,0,Driving School Option
A002,5,Driving School Option (Only RCD3XX)
A002,6,0 = Speed Display inactive
A002,7,1 = Speed Display active
A002,8, 
A002,9,This Function is intended for Driving School purposes and is
A002,10,only supported by specific Versions of the RCD3XX. To Activate
A002,11,this Function switch the Radiio OFF. Then hold the MENU Button
A002,12,while pressing and holding the ON/OFF Button for at least 2 Seconds.
;
;A003,0,
;30
;
A010,0,Remote Control
A010,5,Remote Control
A010,6,0 = Playback disabled
A010,7,1 = Playback enabled
A010,8, 
A010,9,Note: After closing the Diagnostic Session/Communication
A010,10,the Standard Value 0 is automatically being restored.
;
A011,0,Remote Control: Source
A011,5,Remote Control: Source
A011,6,0 = FM
A011,7,1 = AM
A011,8, 
A011,9,Note: After closing the Diagnostic Session/Communication
A011,10,the Standard Value 0 is automatically being restored.
;
A012,0,Remote Control: Frequency FM
A012,5,Remote Control: Frequency FM
A012,6,The Frequency Adjustment is being carried out
A012,7,incrementally starting with 0 = 88.3 MHz.
A012,8, 
A012,9,Note: After closing the Diagnostic Session/Communication
A012,10,the Standard Value 0 is automatically being restored.
;
A013,0,Remote Control: Frequency AM
A013,1,Remote Control: Frequency AM
A013,6,The Frequency Adjustment is being carried out
A013,7,incrementally starting with 0 = 540 kHz.
A013,8, 
A013,9,Note: After closing the Diagnostic Session/Communication
A013,10,the Standard Value 0 is automatically being restored.
;
A014,0,Remote Control: Volume
A014,5,Remote Control: Volume
A014,6,Range: 0...100
A014,7,Standard: 40
A014,8, 
A014,9,Note: After closing the Diagnostic Session/Communication
A014,10,the Standard Value 0 is automatically  being restored.
;
A015,0,Remote Control: Balance
A015,5,Remote Control: Balance
A015,6,Note: After closing the Diagnostic Session/Communication
A015,7,the Standard Value 0 is automatically  being restored.
;
A016,0,Remote Control: Fader
A016,1,Remote Control: Fader
A016,6,Note: After closing the Diagnostic Session/Communication
A016,7,the Standard Value 0 is automatically  being restored.
;
;A017,0,
;0
;
;A018,0,
;0
;
;A019,0,
;0
;
;A022,0,
;0
;
A050,0,Development Test Mode
A050,5,Development Test Mode
A050,6,To Enable the Development Test Mode save "1" as new value.
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Radio (R) Coding
C01,00?xxxx: Treble Speaker Monitoring
C02,1 = Front and Rear Monitoring inactive
C03,2 = Front Monitoring active / Rear Monitoring inactive
C04,3 = Front Monitoring inactive / Rear Monitoring active
C05,4 = Front and Rear Monitoring active
C06,00x?xxx: Radio Configuration I
C07,+2 = CAN-Telephone Control
C08,00xx?xx: Speaker Channels
C09,0 = No passive Speakers (Sound System)
C10,2 = 2 passive Speakers Front and 0 passive Speakers Rear
C11,4 = 4 passive Speakers
C12,00xxx?x: Sound System Correction
C13,0 = No Sound System (No Correction)
C14,1 = Sound System with Cloth Interior (with Open Circuit Recognition)
C15,2 = Sound System with Leather Interior (with Open Circuit Recognition)
C16,3 = Sound System with Cloth Interior (without Open Circuit Recognition)
C17,00xxxx?: Radio Configuration II
C18,+1 = Active/Remote Supplied Antenna
C19,+2 = CD-Changer/iPod-Connection
C20,+4 = CAN-Secondary Display (Board Computer/large Display)
;
