;
; VCDS Label File
;
; Copyright © 2002+ Ross-Tech, LLC
;
; Audi TT (8N)
;
; Component: J429 - Central Locking (#35)
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 8N-35.LBL
; 8Nx-962-267.LBL
;
; includes measuring blocks, (converted) coding and adaptation
;
; created on 15/Dec/2002 by Simon Graham (simgr@attbi.com)
; updated on 21/Apr/2011 by Sebastian Stange (Sebastian@Ross-Tech.com)
; updated on 29/May/2015 by Sebastian Stange (Sebastian@Ross-Tech.com) // Converted Coding added
;
; last modification on 29/May/2015
;
; requires VCDS 14.10.2 / LCode 1.0.5.6 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Driver Door
001,1,Drivers Door,Key Switch,Range: open/close/not oper.
001,2,Interior Locking,Switch (E150),Range: lock/unlock/not oper.
001,3,Door Lock,Status/Feedback,Range: locked/unlocked
001,4,Safety Lock,Status/Feedback,Range: safe/not safe
;
002,0,Passenger Door
002,1,Passenger Door,Key Switch,Range: open/close/not oper.
002,3,Door Lock,Status/Feedback,Range: locked/unlocked
002,4,Safety Lock,Status/Feedback,Range: safe/not safe
;
003,0,Door Contact Switches
003,1,Drivers Door,Contact Switch,Range: Door open/Door closed
003,2,Passenger Door,Contact Switch,Range: Door open/Door closed
003,3,Interior Monitor.,Switch,Range: operated/not oper.
;
004,0,Fuel Flap / Trunk Lid
004,1,Remote Switch,Fuel Flap,Range: open/not oper.
004,2,Trunk Lid,Contact Switch,Range: Lid open/Lid closed
004,3,Remote Switch,Trunk Lid,Range: open/not oper.
;
005,1,Interior,Lights,Range: ON/OFF
005,2,Terminal 15,Shut-Off Delay,Range: Relay ON/Relay OFF
005,3,Remote Control,Comfort Operation,Range: open/close/not oper.
005,4,Luggage Comp,Light,Range: ON/OFF
;
006,0,Remote Control
006,1,Remote Control,Key Number,Range: 0.0...4.0 (0 = None operated / 1-4 = Memory Location 1-4)
006,2,Remote Control,Command,0 = inactive / 1 = active\n\nxxx? = Panic (NAR only)\nxx?x = Rear Lid\nx?xx = Lock\n?xxx = Unlock
; 0 = inactive / 1 = active
; xxx? = Panic (NAR only)
; xx?x = Rear Lid
; x?xx = Lock
; ?xxx = Unlock
006,3,Remote Control,Positions,0 = not occupied / 1 = occupied\n\nxxx? = Memory Location 1\nxx?x = Memory Location 2\nx?xx = Memory Location 3\n?xxx = Memory Location 4
; 0 = NOT occupied / 1 = occupied
; xxx? = Memory Location 1
; xx?x = Memory Location 2
; x?xx = Memory Location 3
; ?xxx = Memory Location 4
;
007,1,Vehicle Speed
007,2,Immobilizer,Status,ON = Immobilizer OK\nOFF = Immobilizer NOT OK (Engine Start blocked)
007,3,Status,Terminal 15,Range: active/inactive
007,4,Status,Terminal S,Range: active/inactive
;
008,0,Coding Flags
008,1,Coding I,,?xx = Remote Control\nx?x = Safe Function inactive (NAR only)\nxx? = Remote Control Confirmation (Opening/Blink 2x)
; ?xx = Remote Control
; x?x = Safe Function inactive (NAR only)
; xx? = Remote Control Confirmation (Opening/Blink 2x)
008,2,Coding II,,?xxx = Terminal 87 Door/Window Motor Logic (NAR only)\nx?xx = Anti-Theft Confirmation (Horn)\nxx?x = Remote Control Confirmation (Locking/Blink 1x)\nxxx? = Time Delay for Trunk Unlocking OR Alarm Cycle for Sounder
; ?xxx = Terminal 87 Door/Window Motor Logic (NAR only)
; x?xx = Anti-Theft Confirmation (Horn)
; xx?x = Remote Control Confirmation (Locking/Blink 1x)
; xxx? = Time Delay for Trunk Unlocking OR Alarm Cycle for Sounder
008,3,Coding III,,?xxx = Right-Hand-Drive (RHD)\nx?xx = Comfort Operation via Remote Control\nxx?x = Auto-Lock/Unlock\nxxx? = Automatic Convertible Top
; ?xxx = Right-Hand-Drive (RHD)
; x?xx = Comfort Operation via Remote Control
; xx?x = Auto-Lock/Unlock
; xxx? = Automatic Convertible Top
008,4,Coding IV,,?xxx = Anti-Theft-System\nx?xx = Selective Central Locking\nxx?x = Anti-Theft Confirmation (Blink)\nxxx? = Anti-Theft LED (1 Hz)
; ?xxx = Anti-Theft-System
; x?xx = Selective Central Locking
; xx?x = Anti-Theft Confirmation (Blink)
; xxx? = Anti-Theft LED (1 Hz)
;
009,0,Convertible Top I
009,1,Operation,Switch (E137)
009,3,Canvas Cover,recognized
009,4,Hard Top,recognized
;
010,0,Convertible Top II
010,1,Front Lock,Switch (F172)
010,2,Latch Open,Switch
010,3,Cover Detector,Switch (F171)
010,4,Front Lock,Switch (F202)
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A021,0,Remote Control learning (Memory Location)
A021,5,Remote Control learning (Memory Location)
A021,6,Select the Memory Location (1-4) to which the Remote should be adapted.
A021,7,Save the new Value and press the Open/Lock Button on the Remote Control.
A021,8, 
A021,9,Additional Remote Controls can be learned by selecting different
A021,10,Memory Locations. Continue until all Remotes are learned.
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Central Locking (J429) Coding
C01,+00001 = Rear Lid Opening via Rear Lid Lock Button
C02,+00002 = Anti-Theft Locking Confirmation (Turn Signals)
C03,+00004 = Selective Locking active
C04,+00008 = Anti-Theft-System installed
C05,+00016 = Half-Automatic Convertible Top (Roadster only)
C06,+00032 = Auto-Lock/Unlock (Locking at 15 km/h)
C07,+00064 = Comfort Operation (Windows/Sunroof) via Remote Control
C08,+00128 = Right-Hand-Drive (RHD)
C09,+00256 = Rear Lid Logic (Anti-Theft-System)
C10,+00512 = Remote Control "Close" Confirmation (1x Turn Signals)
C11,+01024 = Anti-Theft Locking Confirmation (Siren/Horn)
C12,+02048 = Door/Window Logic (USA / Terminal 87)
C13,+04096 = Remote Control "Open" Confirmation (2x Turn Signals)
C14,+08192 = Remote Control active
C15, 
C16,Note #1: Coding Value is the Sum of the individual Options!
C17,Note #2: You can also use the Coding Assist/Helper!
;
;
;---------------------------------------------------
;
; converted coding
; (short coding displayed as long coding for easier modifications)
;
;---------------------------------------------------
;
;
LC,02,0,Rear Lid Opening via Rear Lid Lock Button
LC,02,1,Anti-Theft Locking Confirmation (Turn Signals)
LC,02,2,Selective Locking active
LC,02,3,Anti-Theft-System installed
LC,02,4,Half-Automatic Convertible Top (Roadster only)
LC,02,5,Auto-Lock/Unlock (Locking at 15 km/h)
LC,02,6,Comfort Operation (Windows/Sunroof) via Remote Control
LC,02,7,Right-Hand-Drive (RHD)
LC,01,0,Rear Lid Logic (Anti-Theft-System)
LC,01,1,Remote Control "Close" Confirmation (1x Turn Signals)
LC,01,2,Anti-Theft Locking Confirmation (Siren/Horn)
LC,01,3,Door/Window Logic (USA / Terminal 87)
LC,01,4,Remote Control "Open" Confirmation (2x Turn Signals)
LC,01,5,Remote Control active
LC,01,7=,Additional Coding Options can be found in Byte 02!
LC,00,3=,Coding Details can be found in Byte 01 && Byte 02!
;
