;
; VAG-COM Label File
;
; Audi A3 (8L)
;
; Component: J285 - Instrument Cluster (#17)
;
; P/N: 8L0-920-???-???
;
; includes measuring blocks, adaptation, coding, login
;          and service reset
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 8L-17.LBL
; 8L0-919-xxx.LBL
; 8L0-920-xxx.LBL
;
; created on 03/Dec/2006 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification: 20/Feb/2008
;
; requires VAG-COM 610.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;

;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Instrument Cluster (J285) Coding
;
;
;---------------------------------------------------
;
; login
;
;---------------------------------------------------
;
;
L00,Instrument Cluster (J285) Login
L01,13861 = Adaptation Enabling
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A002,0,Service Reminder
A002,5,Service Reminder
A002,6,0 = Service NOT Due
A002,7,1 = Service Due
A002,8, 
A002,9,To reset the service reminder save 00000 as new value.
;
A003,0,Consumption Correction
A003,5,Consumption Correction
A003,6,Standard Value: 100 %
A003,7,Display Range: 85...115 %
A003,8,Increments: 1 %
A003,9, 
A003,10,Calculation based on volume per distance (e.g. l/100km):
A003,11,New Adaptation Value = Old Adaptation Value * Calculated Consumption / Old Display Value
A003,12,Calculation based on distance per volume (e.g. MPG):
A003,13,New Adaptation Value = Old Adaptation Value * Old Display Value / Calculated Consumption 
;
A004,0,Language
A004,5,Language
A004,6,1 = German
A004,7,2 = English
A004,8,3 = French
A004,9,4 = Italian
A004,10,5 = Spanish
A004,11,6 = Portuguese
A004,12,8 = Chinese
;
A009,0,Mileage/Odometer
A009,5,Mileage/Odometer
A009,6,Increments: 1 = 10 km or 1 = 10 mi
A009,9,The distance can only be changed once until
A009,10,the current value is not over 100 km/62 mi.
A009,11, 
A009,12,NOTE: Perform Login first.
;
A018,0,Auxiliary Heating
;
A019,0,Additional Features
A019,5,Additional Features
A019,6,?xxxx: Illumination (MY 2002 and above)
A019,7,0 = Needle and Scale only active at "Light ON"
A019,8,1 = Needle already active at "Ignition ON"
A019,9,2 = Scale already active at "Ignition ON"
A019,10,3 = Scale (2nd Map) and Needle at "Ignition ON" active
A019,11, 
A019,12,x?xxx - Board Computer
A019,13,0 - only Level 2 (Long Time Memory)
A019,14,1 - Level 1 and 2
A019,15, 
A019,16,xx?xx - Driver Information System (DIS)
A019,17,0 - DIS 1 / 1 - Highline without DIS / 2 - DIS 2
A019,18, 
A019,19,xxx?x - Outside Temperature
A019,20,0 - not active / 1 - active
A019,21, 
A019,22,xxxx? - Remote Clock
A019,23,0 - not active / 1 - clock active
;
A021,0,Immobilizer - Key Adaptation
A021,1,Number of
A021,2,currently
A021,3,adapted Keys
A021,5,Immobilizer - Key Adaptation
;
A030,0,Tank Characteristic (Fuel Level Sensor 1)
A030,5,Tank Characteristic (Fuel Level Sensor 1)
A030,6,This is a parallel shift of the tank characteristic.
A030,7, 
A030,8,Standard: 128
A030,9,Range: 96...160 (-8.0...+8.0 l)
A030,10,Increments: 1 = 1 Ohm = 1/4 l
;
A032,0,Tank Characteristic (Not detactable Tank Volume)
A032,5,Tank Characteristic (Not detactable Tank Volume)
A032,6,The tank volume which is not recordable by the fuel gauge sender(s).
;
A033,0,Tank Characteristic (Full Calibration)
A033,5,Tank Characteristic (Full Calibration)
A033,6,Non-parallel shift of the tank characterictic above a readout of 1/2.
A033,7,To start the adaptation enter '65535' as new value.
A033,8, 
A033,9,Standard Value: 128
A033,10,Value Range: 112...144 (-4.0...+4.0 l)
A033,11,Increments: 1 = 1 Ohm = 1/4 l
;
A035,0,Speed Threshold
A035,5,Speed Threshold
A035,6,This value represents the speed threshold of the
A035,7,dynamic oil pressure system. The threshold can be
A035,8,raised in increments of 250 RPM.
;
A040,0,Mileage since Service
A040,5,Mileage since Service
A040,6,Resolution: 1 = 100 km
A040,7, 
A040,8,NOTE: Adaptation channels 40-48 must be
A040,9,entered and stored in the following order:
A040,10,45 > 42 > 43 > 44 > 40 > 41 > 46 > 47 > 48
;
A041,0,Time since Service
A041,5,Time since Service
A041,6,Resolution: 1 = 1 day(s)
A041,7, 
A041,8,NOTE: Adaptation channels 40-48 must be
A041,9,entered and stored in the following order:
A041,10,45 > 42 > 43 > 44 > 40 > 41 > 46 > 47 > 48
;
A042,0,Minimum Mileage to Service
A042,5,Minimum Mileage to Service
A042,6,Increments: 1 = 1000 km/mi
A042,7,00015 = Standard (15.000 km)
;
A043,0,Maximum Mileage to Service
A043,5,Maximum Mileage to Service
A043,6,Increments: 1 = 1000 km/mi
A043,7,00015 = fixed Service Intervals (15.000 km - w/o Longlife)
A043,8,00030 = flexible Service Intervals (30.000 km - with Longlife)
A043,10,00050 = Diesel (ONLY PD-TDI post Week 18/2001) Engines with flexible Service Intervals (50.000 km - with Longlife)
;
A044,0,Maximum Time to Service
A044,5,Maximum Time to Service
A044,6,Increments: 1 = 1 day(s)
A044,7,00365 = fixed Service Intervals (w/o Longlife)
A044,8,00730 = flexible Service Intervals (with Longlife)
A044,9, 
A044,10,NOTE: Adaptation channels 40-48 must be
A044,11,entered and stored in the following order:
A044,12,45 > 42 > 43 > 44 > 40 > 41 > 46 > 47 > 48
;
A045,0,Oil Quality
A045,5,Oil Quality
A045,6,1 = fixed Service Intervals (w/o Longlife)
A045,7,2 = flexible Service Intervals (with Longlife)
A045,8,4 = Diesel (ONLY PD-TDI post Week 18/2001) Engines with flexible Service Intervals (with Longlife)
;
A046,0,Total Consumption
A046,5,Total Consumption
A046,6,This value does not represent the actual consumption
A046,7,but is rather an arithmetic value for the service interval display.
;
A047,0,Soot Entry
A047,5,Soot Entry
A047,6,Arithmetic value used to calculate the amount of soot in
A047,7,the engine oil referenced to a distance of 100 km and used
A047,8,as comparison value for the service interval display.
;
A048,0,Thermal Load
A048,5,Thermal Load
A048,6,Arithmetic value used to calculate the thermal stress of
A048,7,the engine oil referenced to a distance of 100 km and used
A048,8,as comparison value for the service interval display.
;
A050,0,Immobilizer - Vehicle Data Learning
A050,5,Immobilizer - Vehicle Data Learning
;
;
;---------------------------------------------------
;
; service reset
;
;---------------------------------------------------
;
;
RD,2,Service Reminder Status,1,
RD,40,Mileage since Service,100,DIST
RD,41,Time since Service,1,Days
RD,42,Min Mileage to Service,1000,DIST
RD,43,Max Mileage to Service,1000,DIST
RD,44,Max Time to Service,1,Days
RD,45,Oil Quality,1,
;
RJ,0,0,Service Reset,,
RJ,0,1,2,0
;
RJ,1,0,Change to Fixed Intervals (Kilometers)
RJ,1,1,45,1
RJ,1,2,42,15
RJ,1,3,43,15
RJ,1,4,44,365
;
RJ,4,0,Change to Flexible Intervals (Kilometers/Gasoline & Diesel)
RJ,4,1,45,2
RJ,4,2,42,15
RJ,4,3,43,30
RJ,4,4,44,730
;
RJ,5,0,Change to Flexible Intervals (Kilometers/PD-TDI post Week 18/2001)
RJ,5,1,45,4
RJ,5,2,42,15
RJ,5,3,43,50
RJ,5,4,44,730
;
