;
; VCDS Label File
;
; Copyright © 2006+ Ross-Tech, LLC
;
; Component: R - Radio (#56) - DELTA 6/Premium 6/RHAPSODY
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 1U-56.LBL
; 3B-56.LBL
; 3B7-035-1xx-56.LBL
;
; includes measuring blocks, adaptation and coding
;
; created on 02/Jun/2006 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 09/Jul/2013
;
; requires VCDS 11.11.5 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,General
001,1,Supply Voltage,(Terminal 30),Specification: 5...18 V
001,2,Amplifier,Output,only if Amplifier installed
001,3,Telephone-Mute
001,4,Telephone-Mute,Status,Range: ON/OFF
;
002,0,Speaker/Line-Out (Front)
002,1,Location/Type
002,2,Status
002,3,Location/Type
002,4,Status
;
003,0,Speaker/Line-Out (Rear)
003,1,Location/Type
003,2,Status
003,3,Location/Type
003,4,Status
;
004,0,Remote Feed Antenna
004,1,Antenna,Type
004,2,Component
004,3,Antenna,Status
;
005,0,IF-Output
005,1,Component
005,2,IF-Output,Status
;
007,0,Communication Status CD-Changer (R41)
007,1,Component
007,2,CD-Changer,Status
;
008,0,Signal Strength
008,1,Signal Strength
008,2,Signal Strength,Tuner
;
025,0,Internal Control Module Malfunctions
025,1,Control Module,Status,01 = Button(s) Jam\n02 = Checksum Error ROM/EPROM/Flash-ROM\n03 = Writing Error EEPROM\n04 = CC-Drive (Casette) Error\n05 = CD/DVD-Drive Error
; 01 = Button(s) Jam
; 02 = Checksum Error ROM/EPROM/Flash-ROM
; 03 = Writing Error EEPROM
; 04 = CC-Drive (Casette) Error
; 05 = CD/DVD-Drive Error
;
080,0,Advanced Control Module Identification I
080,1,Identification
080,2,Revision
080,3,Production,Date
080,4,Manufacturer &,Test Stand Number
;
081,0,Advanced Control Module Identification II
081,1,Serial Number
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Radio (R) Coding
C01,000?xxx: Radio Configuration I
C02,+1 = IF-Output
C03,+2 = Telephone (via CAN)
C04,+4 = Multi-Function Steering Wheel (via CAN)
C05,000x?xx: Speaker Channels
C06,0 = No passive Speakers (Sound System)
C07,2 = 2 passive Speakers (Front)
C08,4 = 4 passive Speakers (Front & Rear)
C09,000xx?x: Sound System Correction
C10,0 = No Sound System (No Correction)
C11,1 = Sound System with Cloth Interior
C12,2 = Sound System with Leather Interior
C13,3 = Monsoon (USA only)
C14,000xxx?: Radio Configuration II
C15,+1 = Active/Remote Supplied Antenna
C16,+2 = CD-Changer
C17,+4 = CAN-Secondary Display (Board Computer/large Display)
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A001,0,Reception Optimization
A001,5,Reception Optimization
A001,6,This channel allows optimization of the reception
A001,7,behavior for areas with strong FM interference.
A001,8, 
A001,9,0 = Normal reception
A001,10,1 = Optimized reception
;
A010,0,Remote Control
A010,5,Remote Control
A010,6,0 = Playback disabled
A010,7,1 = Playback enabled
A010,8, 
A010,9,Note: After closing the Diagnostic Session/Communication
A010,10,the Standard Value 0 is automatically being restored.
;
A011,0,Remote Control: Source
A011,5,Remote Control: Source
A011,6,0 = FM
A011,7,1 = AM
A011,8, 
A011,9,Note: After closing the Diagnostic Session/Communication
A011,10,the Standard Value 0 is automatically being restored.
;
A012,0,Remote Control: Frequency FM
A012,5,Remote Control: Frequency FM
A012,6,The Frequency Adjustment is being carried out
A012,7,incrementally starting with 0 = 88.3 MHz.
A012,8, 
A012,9,Note: After closing the Diagnostic Session/Communication
A012,10,the Standard Value 0 is automatically being restored.
;
A013,0,Remote Control: Frequency AM
A013,1,Remote Control: Frequency AM
A013,6,The Frequency Adjustment is being carried out
A013,7,incrementally starting with 0 = 540 kHz.
A013,8, 
A013,9,Note: After closing the Diagnostic Session/Communication
A013,10,the Standard Value 0 is automatically being restored.
;
A014,0,Remote Control: Volume
A014,5,Remote Control: Volume
A014,6,Range: 0...100
A014,7,Standard: 40
A014,8, 
A014,9,Note: After closing the Diagnostic Session/Communication
A014,10,the Standard Value 0 is automatically  being restored.
;
A015,0,Remote Control: Balance
A015,5,Remote Control: Balance
A015,6,Note: After closing the Diagnostic Session/Communication
A015,7,the Standard Value 0 is automatically  being restored.
;
A016,0,Remote Control: Fader
A016,1,Remote Control: Fader
A016,6,Note: After closing the Diagnostic Session/Communication
A016,7,the Standard Value 0 is automatically  being restored.
;
A050,0,Development Test Mode
A050,5,Development Test Mode
A050,6,To Enable the Development Test Mode save "1" as new value.
;
