;
; VCDS Label File
;
; Copyright © 2008+ Ross-Tech, LLC
;
; Seat Leon/Toledo (1M) / Skoda Octavia (1U) / VW Bora/Golf (1J)
; VW New Beetle (1C/9C) / VW Passat (3B) / VW Polo Classic (9V)
;
; Component: J379 - Central Locking (#35) - Generation III (> MY 2002)
;
; P/N: 1C0-962-258-???
;
; includes measuring blocks, coding and adaptation
;
; This file is part of a label files package,
; make sure you have all of the following files.
;
; 1C-35.LBL
; 1C0-962-258-II.LBL
; 1C0-962-258-III.LBL
;
; created on 26/Sep/2008 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 15/Nov/2013
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Driver's door
001,1,Electric window,hall signal,E40 (Specification: auto. open/auto. close/man. open/man. close/close not operated/implausible)
001,2,Electric window,thermal protection,Specification: yes/no
001,3,Child safety,switch,E39 (Specification: yes/no/not installed)
;
002,0,Driver's door (driver's switch for electric windows)
002,1,Passenger side,electric window,E81 (Specification: autom. open/autom. close/man. open/man. close/not operated/implausible)
002,2,Rear left,electric window,E53 (Specification: autom. open/autom. close/man. open/man. close/not operated/implausible)
002,3,Rear right,electric window,E55 (Specification: autom. open/autom. close/man. open/man. close/not operated/implausible)
;
003,0,Driver's door
003,1,Mirror adjustment,switch driver,E43 (Specification: Pos X+/Pos X-/Pos Y+/Pos Y-/not operated)
003,2,Mirror selection,switch driver,E48 (Specification: left/right/fold/not operated)
003,3,Mirror folding,switch,E263 (Specification: released/engaged/not installed)
003,4,Mirror heating,,E231 (Specification: on/off/not installed)
;
004,0,Passenger's door (electric window)
004,1,Switch passenger,(E107),Specification: autom. open/autom. close/man. open/man. close/not operated/implausible
004,2,Thermal protection,passenger,Specification: yes/no
;
005,0,Rear door's (electric windows)
005,1,Switch rear left,(E52),Specification: autom. open/autom. close/man. open/man. close/not operated/implausible
005,2,Thermal protection,rear left,Specification: yes/no
005,3,Switch rear right,(E54),Specification: autom. open/autom. close/man. open/man. close/not operated/implausible
005,4,Thermal protection,rear right,Specification: yes/no
;
006,1,Supply Voltage,(terminal 30)
006,2,Ignition,,Specification: Terminal 15 on/Terminal 15 off
006,3,S-Terminal,,Specification: operated/not operated
006,4,Speed signal,,Steps: 2 km/h
;
007,1,Central locking,key switch driver,Specification: open/closed/not operated/implausible
007,2,Central locking,key switch pass.,Specification: open/closed/not operated/implausible
007,3,Interior locking,driver switch,E150 (Specification: lock/unlock/not operated/implausible)
007,4,Interior locking,passenger switch,E198 - USA only (Specification: lock/unlock/not operated/implausible)
;
008,1,Hood contact,switch (F120),Specification: operated/not operated/not installed
008,2,Rear lid/tailgate,key switch,E165 (Specification: open/closed/not operated/implausible)
008,3,Rear lid/tailgate,contact switch,F124 (Specification: open/closed)
008,4,Central locking,thermal protection,Specification: yes/no
;
009,0,Central locking feedback
009,1,Driver's side,,Specification: safe/not safe/locked/unlocked
009,2,Passenger's side,,Specification: safe/not safe/locked/unlocked
009,3,Rear left,,Specification: safe/not safe/locked/unlocked
009,4,Rear right,,Specification: safe/not safe/locked/unlocked
;
010,0,Rotary latch switches
010,1,Driver's side,,Specification: 1 = dr. open / 2 = dr. closed
010,2,Passenger's side,,Specification: 1 = dr. open / 2 = dr. closed
010,3,Rear left,,Specification: 1 = dr. open / 2 = dr. closed
010,4,Rear right,,Specification: 1 = dr. open / 2 = dr. closed
;
011,1,Immobilizer,key recognition,Specification: yes/no/not installed
011,3,Sliding/tilting,sunroof released,Specification: yes/no
011,4,Status,CAN-Databus,Specification: 2-wire
;
013,1,Rear lid button,rear lid handle,E188/E234 (Specification: not operated/remote switch/lid lever/implausible)
013,2,Rear,first detent,Specification: open/closed/not installed
013,3,Instrument,illumination,Specification: 0...100 %
013,4,Sliding/tilting,sunroof
;
014,1,Permanent code,known,Specification: OK/n.OK
014,2,Code within,effective range,Specification: OK/n.OK
014,3,Algorithm,,Specification: OK/n.OK
014,4,Key number,,Specification: 0...4 (0 = not operated)
;
015,1,Remote control,button,Specification: open/closed/RLR/panic (RLR = rear lid release)
015,2,Interior monitor,sensor (G273),Specification: yes/no/not installed
015,3,Interior monitoring,switch-off (E267),Specification: on/off/not installed
;
016,0,Alarm Source
;   1 = Door Contact Switch Driver Door
;   2 = Door Contact Switch Passenger Door
;   4 = Door Contact Switch Rear Left Door
;   8 = Door Contact Switch Rear Right Door
;  16 = Door Contact Switch Rear Lid/Tailgate
;  17 = Immobilizer
;  18 = Anti-Theft System Power Supply
;  32 = Engine Hood Contact Switch
;  64 = Ignition (Terminal 15)
; 128 = Interior Monitoring
; 255 = No Alarm Source recognized
016,1,Last source,,1 = Door Contact Switch Driver Door\n2 = Door Contact Switch Passenger Door\n4 = Door Contact Switch Rear Left Door\n8 = Door Contact Switch Rear Right Door\n16 = Door Contact Switch Rear Lid/Tailgate\n17 = Immobilizer\n18 = Anti-Theft System Power Supply\n32 = Engine hood contact switch\n64 = Ignition (Terminal 15)\n128 = Interior Monitoring\n255 = No Alarm Source recognized
016,2,2nd last source,,1 = Door Contact Switch Driver Door\n2 = Door Contact Switch Passenger Door\n4 = Door Contact Switch Rear Left Door\n8 = Door Contact Switch Rear Right Door\n16 = Door Contact Switch Rear Lid/Tailgate\n17 = Immobilizer\n18 = Anti-Theft System Power Supply\n32 = Engine hood contact switch\n64 = Ignition (Terminal 15)\n128 = Interior Monitoring\n255 = No Alarm Source recognized
016,3,3rd last source,,1 = Door Contact Switch Driver Door\n2 = Door Contact Switch Passenger Door\n4 = Door Contact Switch Rear Left Door\n8 = Door Contact Switch Rear Right Door\n16 = Door Contact Switch Rear Lid/Tailgate\n17 = Immobilizer\n18 = Anti-Theft System Power Supply\n32 = Engine hood contact switch\n64 = Ignition (Terminal 15)\n128 = Interior Monitoring\n255 = No Alarm Source recognized
016,4,4th last source,,1 = Door Contact Switch Driver Door\n2 = Door Contact Switch Passenger Door\n4 = Door Contact Switch Rear Left Door\n8 = Door Contact Switch Rear Right Door\n16 = Door Contact Switch Rear Lid/Tailgate\n17 = Immobilizer\n18 = Anti-Theft System Power Supply\n32 = Engine hood contact switch\n64 = Ignition (Terminal 15)\n128 = Interior Monitoring\n255 = No Alarm Source recognized
;
080,0,Advanced Control Module Identification I
080,1,Identification
080,2,Revision
080,3,Production,Date
080,4,Manufacturer &,Test Stand Number
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Central Locking (J379) Coding
C01,00016 = 2 Doors with Selective Unlocking
C02,00017 = 2 Doors with Unlocking of all Doors
C03,00018 = 4 Doors with Selective Unlocking
C04,00019 = 4 Doors with Unlocking of all Doors
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A01,0,Remote control adaptation
A01,5,Remote control adaptation
A01,6,Enter the number of keys that should be adapted. Save.
A01,7, 
A01,8,Now press button 1 or 2 on every remote that
A01,9,should be adapted for at least 1 second.
A01,10, 
A01,11,Note #1: All keys must be adapted in one procedure.
A01,12,Note #2: Adaptation of all keys must not exceed 15 seconds.
;
A003,0,Auto-Lock
A003,5,Auto-Lock
A003,6,The doors will lock automatically when the
A003,7,vehicle reaches a speed of 15 km/h or 10 mph.
A003,8, 
A003,9,Specification: 0 = off/1 = on
;
A004,0,Auto-Unlock
A004,5,Auto-Unlock
A004,6,The doors will unlock automatically when the key
A004,7,is removed from the ignition switch.
A004,8, 
A004,9,Specification: 0 = off/1 = on
;
A005,0,Interior Monitoring
A005,5,Interior Monitoring
A005,6,Activation of interior monitoring system.
A005,7, 
A005,8,Specification: 0 = off/1 = on
;
A006,0,Unlock Horn
A006,5,Unlock Horn
A006,6,Horn beep when unlocking via remote control.
A006,7, 
A006,8,Specification: 0 = off/1 = on
;
A007,0,Lock Horn
A007,5,Lock Horn
A007,6,Horn beep when locking via remote control.
A007,7, 
A007,8,Specification: 0 = off/1 = on
;
A008,0,Unlock Blink
A008,5,Unlock Blink
A008,6,Blink when unlocking via remote control.
A008,7, 
A008,8,Specification: 0 = off/1 = on
;
A009,0,Lock Blink
A009,5,Lock Blink
A009,6,Blink when locking via remote control.
A009,7, 
A009,8,Specification: 0 = off/1 = on
;
A010,0,Country Setting
A010,5,Country Setting
A010,6,Country setting for alarm horn.
A010,7, 
A010,8,1 - Rest of World (RoW)
A010,9,2 - Germany
A010,10,3 - Great Britain
;
