;
; VAG-COM Label File
;
; Audi A4 (8E2/8E5) / Audi A6 (4B)
;
; Component: J446 - Parking Aid (#76)
;
; P/N: 8E0-919-283-??
;
; includes measuring blocks, adaptation and coding
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 8E-76.LBL
; 8E0-919-283-8E2.LBL
; 8E0-919-283-8ED.LBL
;
; created on 09/Apr/2006 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification: 14/Oct/2007
;
; requires VAG-COM 405.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Distance (Front)
001,1,Front Left,Sensor (G255),Specification: 10...60 cm (255 cm = no obstacle recognized)
001,2,Front Left Center,Sensor (G254),Specification: 10...160 cm (255 cm = no obstacle recognized)
001,3,Front Right Center,Sensor (G253),Specification: 10...160 cm (255 cm = no obstacle recognized)
001,4,Front Right,Sensor (G252),Specification: 10...60 cm (255 cm = no obstacle recognized)
;
002,0,Distance (Rear)
002,1,Rear Left,Sensor (G203),Specification: 10...60 cm (255 cm = no obstacle recognized)
002,2,Rear Left Center,Sensor (G204),Specification: 10...160 cm (255 cm = no obstacle recognized)
002,3,Rear Right Center,Sensor (G205),Specification: 10...160 cm (255 cm = no obstacle recognized)
002,4,Rear Right,Sensor (G206),Specification: 10...60 cm (255 cm = no obstacle recognized)
;
003,0,Resulting Distance / Vehicle Speed && Voltage
003,1,Resulting,Distance Front,Specification: 0...120 cm (255 cm = no obstacle recognized)
003,2,Resulting,Distance Rear,Specification: 0...160 cm (255 cm = no obstacle recognized)
003,3,Vehicle Speed,,Range: 0.0...255.0 km/h
003,4,Sensor,Voltage Supply
;
004,0,External Information
004,1,Confirmation,Sound,Range: Sound ON/Sound OFF
004,2,Reverese Gear,engaged,Range: Reverse: Yes/Reverse: No
004,3,Trailer hitched,,Range: Trailer: Yes/Trailer: No
004,4,Rear Lid,,Range: Lid Open/Lid Closed
;
005,0,External Information
005,1,Function Light,,Range: LED ON/LED OFF
005,2,Function Button,,Range: Button ON/Button OFF
;
006,0,Oscillation Time (Rear)
006,1,Rear Left,Sensor (G203),Specification: max. 4.00 ms
006,2,Rear Left Center,Sensor (G204),Specification: max. 4.00 ms
006,3,Rear Right Center,Sensor (G205),Specification: max. 4.00 ms
006,4,Rear Right,Sensor (G206),Specification: max. 4.00 ms
;
007,0,Oscillation Time (Front)
007,1,Front Left,Sensor (G255),Specification: max. 4.00 ms
007,2,Front Left Center,Sensor (G254),Specification: max. 4.00 ms
007,3,Front Right Center,Sensor (G253),Specification: max. 4.00 ms
007,4,Front Right,Sensor (G252),Specification: max. 4.00 ms
;
080,0,Advanced Control Module Identification I
;
125,0,CAN-Databus Communication (Comfort)
125,1,Instrument Cluster,(J285)
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Parking Aid (J446) Coding
C01,?xxxx: Trailer Hitch (0 = No / 1 = Yes)
C02,x?xxx: Transmission
C03,0 = Manual Transmission
C04,1 = Automatic Transmission
C05,xx?xx: Confirmation Sound (0 = No / 1 = Yes)
C06,xxx?x: Chassis
C07,0 = Limousine (Sedan) Rest of World
C08,1 = Avant (Wagon) Rest of World
C09,2 = Limousine (Sedan) North America
C10,3 = Avant (Wagon) North America
C11,4 = S-Variant Limousine (Sedan) Rest of World
C12,5 = S-Variant Avant (Wagon) Rest of World
C13,6 = S-Variant Limousine (Sedan) North America
C14,7 = S-Variant Avant (Wagon) North America
C15,8 = allroad
C16,xxxx?: Model
C17,4 - Audi A4 (8E)
C18,5 = Audi A4 Cabrio (8H)
C19,6 = Audi A6 (4B)
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A01,0,Rear Buzzer Volume
A01,5,Rear Buzzer Volume
A01,6,Adaptation of the rear warning buzzer volume.
A01,7, 
A01,8,Display Range: 2...6
;
A02,0,Rear Buzzer Frequency
A02,5,Rear Buzzer Frequency
A02,6,Adaptation of the rear warning buzzer frequency.
A02,7, 
A02,8,Display Range: 0...4
;
A03,0,Front Buzzer Volume
A03,5,Front Buzzer Volume
A03,6,Adaptation of the front warning buzzer volume.
A03,7, 
A03,8,Display Range: 2...6
;
A04,0,Front Buzzer Frequency
A04,5,Front Buzzer Frequency
A04,6,Adaptation of the front warning buzzer frequency.
A04,7, 
A04,8,Display Range: 0...4
;
