;
; VCDS Label File
;
; Copyright © 2007+ Ross-Tech, LLC
;
; Audi TT (8J)
;
; Component: J525 - Sound System (#47)
;
; P/N: 8J0-035-223-???
;
; includes measuring blocks, coding and selective output test
;
; created on 31/Jul/2007 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 06/Mar/2015
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Supply Voltage
001,1,Supply Voltage,(Terminal 30)
001,2,Voltage Status,,x---xxx1 = Terminal  S active\nx---xx1x = Terminal 15 active\nx---x1xx = Terminal  X active\nx---1xxx = Terminal 50 active\n1---xxxx = Error
; x---xxx1 = Terminal  S active
; x---xx1x = Terminal 15 active
; x---x1xx = Terminal  X active
; x---1xxx = Terminal 50 active
; 1---xxxx = Error
;
002,0,Temperatures
002,1,Temperature,Analog Part
002,2,Temperature,Digital Part
002,4,Status,Remote Wire,0 = Remote Wire OFF\n1 = Remote Wire ON
;
004,1,Voltage,Microphone Input
004,2,Vehicle Speed
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Sound System (J525) Coding
C01,0?xxxxx: Options II (P/N Index B and above ONLY)
C02,0 = Cell Phone Preparation & Voice Control not installed
C03,2 = Cell Phone Preparation installed
C04,3 = Voice Control installed
C05,4 = Cell Phone Preparation & Voice Control installed
C06,0x?xxxx: Noise Compensation
C07,1 = GALA
C08,3 = GALA/Bose Audipilot (switchable)
C09,4 = Bose Audiopilot
C10,0xx?xxx: Volume Adjustment
C11,0 = No Increase/Decrease | 1 = 1 db Increase | 2 = 2 db Increase
C12,3 = 3 db Increase | 4 = 4 db Increase | 5 = 5 db Increase | 6 = 6 db Increase (Standard)
C13,7 = 1 db Decrease | 8 = 2 db Decrease | 9 = 3 db Decrease
C14,0xxx?xx: Activation
C15,1 = via Remote Wire
C16,2 = via Signal Level
C17,0xxxx?x: Model
C18,1 = Audi TT (8J) Coupé
C19,2 = Audi TT (8J) Roadster (Manual Roof)
C20,3 = Audi TT (8J) Roadster (Automatic Roof)
C21,0xxxxx?: Options II
C22,1 = Right-Hand-Drive/Cloth/Diesel | 2 = Left-Hand-Drive/Leather/Diesel
C23,3 = Right-Hand-Drive/Leather/Diesel | 4 = Left-Hand-Drive/Cloth/Gasoline
C24,5 = Right-Hand-Drive/Cloth/Gasoline | 6 = Left-Hand-Drive/Leather/Gasoline
C25,7 = Right-Hand-Drive/Leather/Gasoline | 8 = Left-Hand-Drive/Cloth/Diesel
;
;
;---------------------------------------------------
;
; selective output test
;
;---------------------------------------------------
;
;
T420,Front Midrange Speaker (R103/R104)
T870,Front Bass Speaker (R21/R23)
T874,Front Treble Speaker (R20/R22)
T876,Rear Treble Speaker (R14/R16)
T2246,Center Speaker
T2558,Rear Mid-Range/Woofer Loudspeaker (R159/R160)
;
