;
; VCDS Label File
;
; Copyright © 2008+ Ross-Tech, LLC
;
; Audi A3 (8P) / Audi A4 (8E) / Audi TT (8J)
;
; Component: Radio/Navigation System (#37/#56) - RNS-E
;
; P/N: 8J0-035-192-???
;
; includes measuring blocks, adaptation and coding
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 8E-37.LBL
; 8E-56.LBL
; 8J-37.LBL
; 8J-56.LBL
; 8P-37.LBL
; 8P-56.LBL
; 8J0-035-192-RNSL.LBL
;
; created on 06/Jun/2008 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 12/Jul/2012
;
; requires VCDS 800.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;

;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C01,00?xxxx: Configuration III
C02,1 = Treble Speaker Monitoring inactive & Analog Input (AUX) not installed
C03,2 = Treble Speaker Monitoring active
C04,3 = Analog Input (AUX) installed
C05,4 = Treble Speaker Monitoring active & Analog Input (AUX) installed
C06,00x?xxx: Configuration II
C07,+1 = GALA iactive
C08,+2 = Telephone/Cell Phone Preparation installed
C09,+4 = Diagnosis of Front Speakers inactive
C10,00xx?xx: Speakers
C11,0 = Sound System (active Speakers)
C12,2 = passive Front Speakers
C13,00xxx?x: Sound Correction
C14,0 = Linear (No Sound System/No Correction)
C15,1 = Audi A4 Limousine/Avant (8E)
C16,2 = Audi A4 Cabrio without high-pass (8H)
C17,3 = Audi A4 Cabrio with high-pass (8H)
C18,4 = Audi TT (8J)
C19,5 = Audi A3 (8P)
C20,9 = Sound System (Bose)
C21,00xxxx?: Configuration I
C22,+1 = Multifunction Steering Wheel
C23,+2 = CD-Changer
C24,+4 = Destination input while driving
;
;
;---------------------------------------------------
;
; selective output test
;
;---------------------------------------------------
;
;
T854,Display Test
T2875,CD/DVD-Drive Read Test: Short Test
T2876,CD/DVD-Drive Read Test: Random Test
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A002,0,Wheel Impulse
A002,5,Wheel Impulse
A002,6,The Distance Impulse describes the amount of ABS Pulses per Wheel Revolution.
A002,7, 
A002,8,43 = Audi A3 (8P)/ Audi TT (8J) / Audi R8 (42)
A002,9,45 = Audi A4 (8E) OR Seat Exeo (3R)
A002,10, 
A002,11,NOTE: If "0" is entered as new Value the System calibrates
A002,12,itself automatically after a short distance and inputs a proper Value.
;
A003,0,Language (Screen)
A003,5,Language (Screen)
A003,6,0 = German
A003,7,1 = English (UK only)
A003,8,2 = English (USA only)
A003,9,3 = Spanish
A003,10, 
A003,11,Additional Options can be found in
A003,12,the RADIO/SETUP Menu for this Device.
;
A004,0,Tire Circumference
A004,5,Tire Circumference
A004,6,The Tire Circumference is beeing adapted in "mm".
;
A007,0,Settings
A007,5,Settings
A007,6,+01 = Distance in Miles
A007,7,+02 = Speed in mph
A007,8,+04 = Time in am/pm
A007,9,+08 = Date in MM:TT:JJJJ
A007,10,+16 = Repeat Voice Commands
;
