;
; VCDS Label File
;
; Copyright © 2012 Ross-Tech, LLC
;
; Audi A8 (4E)
;
; Component: J431 - Automatic Headlight Aim Control (#55)
;
; P/N: 4E0-910-357-???
;
; includes measuring blocks, basic setting, coding and adaptation
;
; created on 28/Mar/2012 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 28/Mar/2012
;
; requires VCDS 11.11.2 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,General
001,1,Voltage,(Terminal 15)
001,2,Light,(Terminal 56b),Specification: ON/OFF
001,3,Vehicle Speed
001,4,Acceleration
;
B001,0,Adjustment Position && Adjustment Learning
B001,1,Status, , 
B001,2, , , 
B001,3, , , 
B001,4, , , 
;
002,0,Sensor Values
002,1,Front Sensor (G78),(actual)
002,2,Rear Sensor (G76),(actual)
002,3,Actuator Motor,Activation
002,4,Time Constant
;
003,0,Input Signals (CAN)
003,1,Turn Signal,Left,Range: ON/OFF
003,2,Turn Signal,Right,Range: ON/OFF
003,3,Brake Lights,,Range: ON/OFF
003,4,Engine,,Range: ON/OFF
;
004,0,Cornering Light
004,1,Cornering Light,Right,Range: ON/OFF
004,2,Cornering Light,Left,Range: ON/OFF
004,3,Cornering Light,Right Flash,Range: ON/OFF
004,4,Cornering Light,Left Flash,Range: ON/OFF
;
005,0,Steering Angle Sensor (G85)
005,1,Steering Angle,Sensor (G85)
;
125,0,CAN-Databus Powertrain (Communication)
125,1,Brake Electronics,(J104),Display Range: ABS 1/ABS 0\nSpecification: ABS 1
125,2,CAN-Gateway,(J533)
125,3,Steering Angle,Sensor (G85),Display Range: Steer. ang. 1/Steer. ang. 0\nSpecification: Steer. ang. 1
125,4,Engine,,Display Range: Engine 1\Engine 0\nSpecification: Engine 1
;
126,0,CAN-Databus Powertrain (Communication)
126,1,Level Control,(J197)
126,2,Ignition Lock
126,3,Immobilizer
;
225,0,CAN-Databus Powertrain (Time-Out)
225,1,Brake Electronics,(J104)
225,2,CAN-Gateway,(J533)
225,3,Steering Angle,Sensor (G85)
225,4,Engine
;
226,0,CAN-Databus Powertrain (Time-Out)
226,1,Level Control,(J197)
226,2,Ignition Lock
226,3,Immobilizer
;
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Automatic Headlight Aim Control (J745) Coding
C01,0000000 = Halogen Headlights
C02,0000001 = Bi-Xenon Headlights
C03,0000002 = Cornering Light (old Front/Dual Frame )
C04,0000003 = Cornering Light (new Front/Single Frame - Rest of World)
C05,0000004 = Cornering Light (new Front/Single Frame - North American Region)
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;

;
