;
; VCDS Label File
;
; Copyright © 2008-2010 Ross-Tech, LLC
;
; VW Tiguan (5N)
;
; Component: J104 - Brake Electronics (#03) - TRW 450
;
; P/N: 5N0-614-517-???
;
; includes measuring blocks, basic setting, coding, adaptation 
;          and security access
;
; created on 18/Jul/2008 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 27/Jun/2010
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks & basic setting
;
;---------------------------------------------------
;
;
001,0,Current Wheel Speed
001,1,Speed Sensor,Front Left (G47),Range: 0.0...255.0 km/h
001,2,Speed Sensor,Front Right (G45),Range: 0.0...255.0 km/h
001,3,Speed Sensor,Rear Left (G46),Range: 0.0...255.0 km/h
001,4,Speed Sensor,Rear Right (G44),Range: 0.0...255.0 km/h
;
B001,0,Brake System Bleeding
B001,1,Status, , 
B001,2, , , 
B001,3, , , 
B001,4, , , 
;
;002,1,,,
;       1,Bin. Bits,
002,2,All-Wheel-Drive,Status
;   000100,Bin. Bits,
;002,3,,,
;0x0080,Hex Value,
;
003,0,Switches and Warning Lights
003,1,Clutch (F36),& Interlock (N110),1x = Clutch Pedal Switch operated\nx1 = Interlock Switch active (P/N)
003,2,Brake System,Warning L. (K118)
003,3,ABS,Warning L. (K47)
003,4,ASR/ESP,Warning L. (K155)
;
004,0,Steering Angle / Lateral Acceleration / Rotation Rate
004,1,Steering Angle,Sensor (G85),Range: -720.0...+720.0 °\nTolerance (when straight): ±2.5 °
004,2,Lateral Acc.,Sensor (G200),Specification (Standing): ± 1.5 m/s²
004,3,Rotation Rate,Sensor (G202),Range: -69.0...+69.0 °/s\nSpecification: ± 1.5 °/s
004,4,Longitudinal,Acc. Sensor (G251),Specification: ± 1.5 m/s²
;
005,0,Brake Pressure && Steering Angle Sensor Status
005,1,Brake Pressure,Sensor (G201),Specification: ± 3.0 bar
005,2,Steering Angle,Sensor (G85) Status,Range: Initialised/N. Initialised/Implausible
005,3,ASR/ESP-Button,(E256),Range: ON/OFF
005,4,Brake Light,Switch (F)
;
006,0,Voltage Supply
006,1,Voltage,Terminal 15
006,2,Voltage,Term.30 (Valves),Range: 0.0...20.5 V
006,3,Voltage,Term.30 (Logic),Range: 0.0...20.5 V
006,4,Voltage,Pump Motor,Range: 0.0...20.5 V
;
007,1,EDS Shut-Off,(Overtemp.),1xxx = Front Left\nx1xx = Front Right\nxx1x = Rear Left\nxxx1 = Rear Right
;007,2,,,
;40.0°C,Temperature,
;
008,0,Adaptation Status
008,1,Adaptation,Überlastbetrieb
;008,2,
;0,Count,
008,3,Adaptation,Vacuum Level
;
009,1,Vacuum Reserv.,Pressure
009,2,Brake Pressure,Sensor (G201),Specification: ± 3.0 bar
009,3,Vacuum Level,Control
;009,4,,,
;not installed, ,
;
010,1,Trailer,Stabilization
010,2,Input,Signals,1xx = Wipers ON\nx1x = Drivers Door OPEN\nxx1 = Reverse Gear ENGAGED
;
011,0,Speed Encoder Errors (Front Left)
011,1,Encoder Errors,(G47) Minimum
011,2,Encoder Errors,(G47) Maximum
011,3,Encoder Errors,(G47) Average
;
012,0,Speed Encoder Errors (Front Right)
012,1,Encoder Errors,(G45) Minimum
012,2,Encoder Errors,(G45) Maximum
012,3,Encoder Errors,(G45) Average
;
013,0,Speed Encoder Errors (Rear Left)
013,1,Encoder Errors,(G46) Minimum
013,2,Encoder Errors,(G46) Maximum
013,3,Encoder Errors,(G46) Average
;
014,0,Speed Encoder Errors (Rear Right)
014,1,Encoder Errors,(G44) Minimum
014,2,Encoder Errors,(G44) Maximum
014,3,Encoder Errors,(G44) Average
;
015,1,Hill Descend,Assist Status,0 = inactive\n1 = active (> 15% Downhill Grade)
015,2,Hill Descend,Assist Lamp,Range: ON/OFF
;015,3,,,
;Not Active, ,
;15,4,,,
;0.0 %,Lambda,
;
016,0,Tire Pressure Monitoring (TPMS) I
016,1,Mileage at,last Warning,Mileage (KM) = Field 1 x 65535 + Field 2
016,2,Mileage at,last Warning,Mileage (KM) = Field 1 x 65535 + Field 2
;
017,0,Tire Pressure Monitoring (TPMS) II
017,1,Mileage at,last Warning,Mileage (KM) = Field 1 x 65535 + Field 2
017,2,Mileage at,last Warning,Mileage (KM) = Field 1 x 65535 + Field 2
;
018,0,Tire Pressure Monitoring (TPMS) III
018,1,TPMS-Button,(E492),Range: Operated/Not Oper.
;
B040,0,Deactivation of Longitudinal Acceleration Sensor (G251)
;
B060,0,Adjustment of Steering Angle Sensor (G85)
B060,1,Adjustment
B060,2,Adjustment,Status,Specification: OK
B060,3,Steering Angle,Sensor (G85)
;
B061,0,Adjustment of Rotation Rate & Lateral/Longit. Acc. Sensor (G200/G202/G251)
B061,1,Adjustment
B061,2,Adjustment,Status,Specification: OK
;
B066,0,Adjustment of Brake Pressure Sensor (G201)
B066,1,Adjustment
B066,2,Adjustment,Status,Specification: OK
B066,3,Brake Pressure,Sensor (G201)
;
070,1,ESP-Status,,Range: Activated/Not Activated
070,2,ASR-Status,,Range: Activated/Not Activated
070,3,EDS-Status,,Range: Activated/Not Activated
070,4,Auto-Hold,Status,Range: Activated/Not Activated
;
071,1,Parking Brake,Status,Range: Activated/Not Activated
;71,2,,,
;Disabled, ,
;
125,0,CAN-Databus Powertrain (Communication)
125,1,Engine,,Specification: Engine 1\nRange: Engine 1/Engine 0
125,3,Instrument Cluster,(J285),Specification: Instruments 1\nRange: Instruments 1/Instruments 0
125,4,Steering Angle,Sensor (G85),Specification: Steer. ang. 1\nRange: Steer. ang. 1/Steer. ang. 0
;
126,0,CAN-Databus Powertrain (Communication)
126,1,CAN-Gateway,(J533),Specification: Gateway 1\nRange: Gateway 1/Gateway 0
126,2,Airbag,(J234),Range: Airbag 1/Airbag 0\nSpecification: Airbag 1
126,3,All-Wheel,Drive (J492)
126,4,Parking Brake,(J540)
;
127,0,CAN-Databus Powertrain (Communication)
127,2,Immobilizer,,Specification: Immobilizer 1\nRange: Immobilizer 1/Immobilizer 0
;
231,0,Tire Pressure Monitoring (TPMS)
; 0 = Nothing Learned
; 1 = Only 1st Threshold powered
; 2 = Only 2nd Threshold powered
; 3 = Only 1st Threshold rolling
; 4 = Only 2nd Threshold rolling
; 5 = 1st Threshold powered and rolling
; 6 = 1st Threshold powered and 2nd Threshold rolling
; 7 = 2nd Threshold powered and 1st Threshold rolling
; 8 = 2nd Threshold powered and rolling (Optimal)
231,1,Speed Range I
; 5?xxx = Speed Range 1 ( 15 -  70 km/h)
; 5x?xx = Speed Range 2 ( 70 - 100 km/h)
; 5xx?x = Speed Range 3 (100 - 130 km/h)
; 5xxx? = Speed Range 4 (130 - 160 km/h)
231,2,Speed Range II
; 5?xxx = Speed Range 5 (160 - 190 km/h)
; 5x?xx = Speed Range 6 (190 - 220 km/h)
; 5xx?x = Speed Range 7 (220 - 250 km/h)
231,3,Curve/Wheel,Recognition
; 5?x00 = Curve Recognition (0 = No Curve / 1 = Left or Right Curve learned / 2 = Complete Curve learned)
; 5x?00 = Wheel Recognition (0 = inactive / 1 = activ)
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
;A001,0,
;1
;
;A021,0,
;ERROR: Security Acess required
;
;A023,0,
;2
;A023,1,
;2.0 km/h
;
;A031,0,
;0
;A031,1,
;Enabled
;
;A033,0,
;ERROR: Security Access required
;
;A044,0,
;0
;A044,1,
;Enabled
;
;A051,0,
;0
;A051,1,
;Enabled
;
;A053,0,
;0
;A053,1,
;Rear Axle
;A053,2,
;Full
;A053,3,
;Delay
;A053,4,
;Enabled
;
;A055,0,
;0
;A055,1,
;Brake discs
;A055,2,
;wiper
;A055,3,
;Enabled
;
;A056,0,
;1
;A56,1,
;Trailer
;A056,2,
;Function
;A056,3,
;Deactivated
;
;A057,0,
;ERROR: Security Access required
;
;A061,0,
;0
;A061,1,
;Brake Booster
;A061,2,
;Deactivated
;
;A063,0,
;0
;A063,1,
;Test
;A063,2,
;Enabled
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
;
;
C00,Brake Electronics (J104) Coding
C01,To request a proper Coding Value for this Control Module please
C02,Email Ross-Tech or your local Distrubutor. Make sure to include
C03,a complete Auto-Scan (full VIN as well) of the Vehicle as well
C04,as a short Description of what happened to the Car.
C05, 
C06,http://www.Ross-Tech.com/contact.html
;
;
;---------------------------------------------------
;
; security access
;
;---------------------------------------------------
;
;
S00,Brake Electronics (J104) Security Access
S01,40168 = Basic Setting Enabling
S02,50403 = Adaptation Enabling
;
