;
; VCDS Label File
;
; Volkswagen Sharon (7M)
;
; Component: J***- Multifunction unit (electronic central electrics) 08.97 ? (#09)
;
; P/N: 7M3-962-258-???
;
; includes measuring blocks, (converted) coding and adaptation
;
; created on 29/Nov/2017 by Seamus Mallon
; updated on 01/Dec/2017 by Seamus Mallon
;
; requires VCDS 14.10.2 / LCode 1.0.5.6 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Door Key Switch Status
001,1,Key Switch,Driver Door,Range: Closed
001,2,Key Switch,Driver Door,Range: OPEN
001,3,Key Switch,Pass Door,Range: OPEN
001,4,Key Switch,Rear Lid,Range: OPEN
;
002,0,Door Switches Status
002,1,Interior locking Switch,E150,Range: Lock/Unlock/implausible
002,2,Rear lid release switch,E165 unlock signal,Range: unlock
002,3,Door contact switch, driver door -F2-,Range: Door Closed/Door Open
002,4,Door contact switch, Passenger doors,Range: Door Closed/Door Open
;
003,0,Ignition Key Status
003,1,Vehicle system voltage, terminal 30,Range: 11.5v – 14.5v
003,2,Terminal 15,,Range: OFF/ON
003,3,Terminal X,,Range: OFF/ON
003,4,S-contact (buzzer),,Range: OFF/ON
;
004,1,Consumer deactivation,Fuse -S157,Range: OK/Not OK
004,2,Consumer deactivation,signal,Range: OFF/ON
004,3,Interior light,signal,Range: OFF/ON
004,4,Window heater output, Reduction,Range: Yes/No
;
005,1,Speed signal,Km/Hour,Range: Speed in km/Hour
005,2,Alternator,terminal 61,Range: Turn/Still
005,4,Crash sensor signal,,Range: Off/On
;
007,0,Heated Window Status
007,1,Heated Windscreen,Switch -E180-,Range: Off/On
007,2,Heated Rear Window,Switch -E15-,Range: Off/On
007,3,Heated Rear Window,Fuse -S41-,Range: ok/Not OK
007,4,Heated Rear Window,Status,Range: Off/On;
;
008,1,Turn signal switch -E2-,Indicate left position, Range: Off/On
008,2,Turn signal switch -E2-,Indicate right position, Range: Off/On
008,3,Turn signal,Left,Range: Off/On
008,4,Turn signal,Right,Range: Off/On
;
009,2,Light switch,-E4- (main & dipped beam),Range: Off/On
009,3,Dipped beam light,Left, Range: OK/not OK
009,4,Dipped beam light, Right,Range: OK/not OK

;
010,1,Brake light Switch,,Range:OFF/ON
010,2,Brake light,Left,Range:OK/not OK
010,3,Brake light,Right,Range:OK/not OK
;
013,0,Side Lights Status
013,1,Side light Left,Switch Status,Range:OFF/ON
013,2,Side light Right,Switch Status,Range:OFF/ON
013,3,Side-Tail light,Left bulb status,Range:OK / not OK
013,4,Side-Tail light,Right bulb status,Range: OK / not OK
;
014,0,Remote Control Status
014,1,Radio Remote Control,buttons press,Range: Open/Closed
014,2,Permanent code known,,Range: OK/not OK 
014,3,Code within effective,range,Range: OK/not OK
014,4,Transfer,,Range: OK/not OK
;
015,2,Bonnet switch,, Range: Closed/OPEN 
015,3,Tailgate switch,,Range: Closed/OPEN
;
;

;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Multifunction unit (electronic central electrics) 08.97 ? Coding
C01,00004 = Central locking  - - - - - - - - - - - Single door opening
C02,00005 = Central locking  - - - - - - - - - - - All doors opening 
C03,00256 = CL  Anti-theft alarm - - - - - - - - Selective Central Locking (SCL)
C04,00257 = CL  Anti-theft alarm - - - - - - - - All door opening
C05,16384 = CL Radio RC - - - - - - - - - - - - Single door opening
C06,16385 = CL Radio RC - - - - - - - - - - - - All doors opening	
C07,4096 = CL Radio RC Anti-theft Alarm - Single door opening
C08,4097 = CL Radio RC Anti-theft Alarm - All doors opening
;
;
;---------------------------------------------------
;
