;
; VCDS Label File
;
; Copyright © 2006-2011 Ross-Tech, LLC
;
; VW New Beetle Cabriolet (1Y)
;
; Component: J256 - Convertible Top (#26)
;
; P/N: 1Y0-959-255-???
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 1Y-26.LBL
; 1Y0-959-255-HYD.LBL
; 1Y0-959-255-MEC.LBL
;
; includes measuring blocks
;
; created on 12/Feb/2006 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 20/Jun/2011
;
; requires VCDS 10.6.4 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,1,Conv. Top Oper.,Switch (E137),Range: Not Operated/Open/Closed/Not OK
001,2,Central Window,Regul. Sw. (E189),Range: Not Operated/Open/Closed/Not OK
001,3,Convertible Top,Switches I,01---xxx = Tonneau Cover Switch (F328)   (1 = Tonneau installed)\n0x---1xx = Closed Position Switch (F202) (1 = Convertible Top locked)\n0x---x1x = Open Position Switch (F171)   (1 = Convertible Top closed)\n0x---xx1 = Open Position Switch (F171)   (1 = Convertible Top open)
; 01---xxx = Tonneau Cover Switch (F328)   (1 = Tonneau installed)
; 0x---1xx = Closed Position Switch (F202) (1 = Convertible Top locked)
; 0x---x1x = Open Position Switch (F171)   (1 = Convertible Top closed)
; 0x---xx1 = Open Position Switch (F171)   (1 = Convertible Top open)
001,4,Convertible Top,Switches II,--01x0xx = Right Convertible Top Closed Lock Switch (F326) (1 = Right Lock closed)\n--0x10xx = Right Convertible Top Open Lock Switch (F325)   (1 = Right Lock open)\n--0xx01x = Left Convertible Top Closed Lock Switch (F324)  (1 = Left Lock closed)\n--0xx0x1 = Left Convertible Top Open Lock Switch (F323)    (1 = Left Lock open)
; --01x0xx = Right Convertible Top Closed Lock Switch (F326) (1 = Right Lock closed)
; --0x10xx = Right Convertible Top Open Lock Switch (F325)   (1 = Right Lock open)
; --0xx01x = Left Convertible Top Closed Lock Switch (F324)  (1 = Left Lock closed)
; --0xx0x1 = Left Convertible Top Open Lock Switch (F323)    (1 = Left Lock open)
;
002,1,Vehicle Speed,from Cluster (J285)
002,2,Vehicle Speed,from ABS (J104)
002,3,Supply Voltage,(Terminal 30)
002,4,Window Regulator,Status,1xxxxxxx = Right Rear Window Regulator     (1 = Open)\nx1xxxxxx = Right Rear Window Regulator     (1 = Closed)\nxx1xxxxx = Left Rear Window Regulator      (1 = Open)\nxxx1xxxx = Left Rear Window Regulator      (1 = Closed)\nxxxx1xxx = Passenger Side Window Regulator (1 = Open)\nxxxxx1xx = Passenger Side Window Regulator (1 = Closed)\nxxxxxx1x = Driver Side Window Regulator    (1 = Open)\nxxxxxxx1 = Driver Side Window Regulator    (1 = Closed)
; 1xxxxxxx = Right Rear Window Regulator     (1 = Open)
; x1xxxxxx = Right Rear Window Regulator     (1 = Closed)
; xx1xxxxx = Left Rear Window Regulator      (1 = Open)
; xxx1xxxx = Left Rear Window Regulator      (1 = Closed)
; xxxx1xxx = Passenger Side Window Regulator (1 = Open)
; xxxxx1xx = Passenger Side Window Regulator (1 = Closed)
; xxxxxx1x = Driver Side Window Regulator    (1 = Open)
; xxxxxxx1 = Driver Side Window Regulator    (1 = Closed)
;
003,0,Window Regulator Position
003,1,Window Regulator,Front Left,Range: 0...100 %\n\n0 % = Window Closed\n100 % = Window Open
003,2,Window Regulator,Front Right,Range: 0...100 %\n\n0 % = Window Closed\n100 % = Window Open
003,3,Window Regulator,Rear Left,Range: 0...100 %\n\n0 % = Window Closed\n100 % = Window Open
003,4,Window Regulator,Rear Right,Range: 0...100 %\n\n0 % = Window Closed\n100 % = Window Open
;
004,1,Left Linkage Flap,Position (G442),Range: 0.0...255.0\n\n    0.0...55.0 = Flap closed\n205.0...255.0 = Flap open
004,2,Right Linkage Flap,Position (G443),Range: 0.0...255.0\n\n    0.0...55.0 = Flap closed\n205.0...255.0 = Flap open
004,3,Status,Terminal 15,Range: Term. 15 ON/Term. 15 OFF
004,4,Thermal Protection,Circuit Break. (S68),Yes = Convertible Top Operation allowed\nNo = Convertible Top Operation blocked
; Yes = Convertible Top Operation allowed
;  No = Convertible Top Operation blocked
;
005,1,Linkage Flap,Motor Status,----1xxx = Left Linkage Flap Motor (V289)  (1 = Open)\n----x1xx = Left Linkage Flap Motor (V289)  (1 = Closed)\n----xx1x = Right Linkage Flap Motor (V290) (1 = Open)\n----xxx1 = Right Linkage Flap Motor (V290) (1 = Closed)
; ----1xxx = Left Linkage Flap Motor (V289)  (1 = Open)
; ----x1xx = Left Linkage Flap Motor (V289)  (1 = Closed)
; ----xx1x = Right Linkage Flap Motor (V290) (1 = Open)
; ----xxx1 = Right Linkage Flap Motor (V290) (1 = Closed)
005,2,Hydraulic Pumps,&& Locking Motors,1x--xxxx = Hydraulic Pump Relay (J321)    (1 = Opening Convertible Top)\nx1--xxxx = Hydraulic Pump Relay 2 (J588)  (1 = Closing Convertible Top)\nxx--1xxx = Left Top Locking Motor (V291)  (1 = Open)\nxx--x1xx = Left Top Locking Motor (V291)  (1 = Closed)\nxx--xx1x = Right Top Locking Motor (V292) (1 = Open)\nxx--xxx1 = Right Top Locking Motor (V292) (1 = Closed)
; 1x--xxxx = Hydraulic Pump Relay (J321)    (1 = Opening Convertible Top)
; x1--xxxx = Hydraulic Pump Relay 2 (J588)  (1 = Closing Convertible Top)
; xx--1xxx = Left Top Locking Motor (V291)  (1 = Open)
; xx--x1xx = Left Top Locking Motor (V291)  (1 = Closed)
; xx--xx1x = Right Top Locking Motor (V292) (1 = Open)
; xx--xxx1 = Right Top Locking Motor (V292) (1 = Closed)
005,3,Autom. Day/Night,Interior Mirror (Y7),Range: Lamp OFF/Lamp ON/Blinking
005,4,Warning Buzzer
;
080,0,Advanced Control Module Identification I
;
