;
; VCDS Label File
;
; Copyright © 2005-2012 Ross-Tech, LLC
;
; Audi A6 (4F) / Audi Q7 (4L)
;
; Component: J519 - Central Electronics (#09)
;
; P/N: 4F0-910-279-???
;
; includes measuring blocks, basic setting, adaptation, coding,
;          security access and selective output tests
;
; created on 10/Jul/2005 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 02/Feb/2012
;
; requires VCDS 805.1 or newer
;
;
;---------------------------------------------------
;
; measuring blocks & basic setting
;
;---------------------------------------------------
;
;
001,1,Voltage Supply,(Terminal 30 left)
001,2,Voltage Supply,(Terminal 30 right)
001,3,Rotary,Light Switch,Step 1 = Automatic Driving Light\nStep 2 = Parking Light\nStep 3 = Low Beam\nStep 4 = Fog Light\nStep 5 = Rear Fog Light
001,4,Emergency,Flasher Button,Display Range: operated/not operated
;
B001,0,Steering Column Basic Setting
; After replacing the Steering Column or the Central Electronics Control Module (J519)
; Make sure to approach all 4 end positions (up, down, forward, back) before performing the basic setting.
;
002,0,Steering Column Adjustment
002,1,Adjustment,(Axial)
002,2,Adjustment,(Vertical)
002,3,Adjustment,(Memory)
002,4,Adjustment,(Status),1xxxxxxx - Storage Mode\nx1xxxxxx - Memory Mode\nxx1xxxxx - Manual Adjustment\nxxx1xxxx - Rest Mode\nxxxx1xxx - Extracting\nxxxxx1xx - In\nxxxxxx1x - Lowering\nxxxxxxx1 - Up
;
004,0,Hood Contact && Backup Light
004,1,Hood Contact,Switch,Display Range: ON/OFF
004,2,Back-Up Light,Switch,Display Range: ON/OFF
;
005,0,Parking Lights && Low Beams
005,1,Left,Parking Light,Display Range: ON/OFF/%
005,2,Right,Parking Light,Display Range: ON/OFF/%
005,3,Left,Low Beam,Display Range: ON/OFF/%
005,4,Right,Low Beam,Display Range: ON/OFF/%
;
006,0,High Beams && Fog Lights
006,1,Left,High Beam,Display Range: ON/OFF/%
006,2,Right,High Beam,Display Range: ON/OFF/%
006,3,Left,Fog Light,Display Range: ON/OFF/%
006,4,Right,Fog Light,Display Range: ON/OFF/%
;
007,0,Front && Side Turn Signals
007,1,Left Front,Turn Signal,Display Range: ON/OFF/%
007,2,Right Front,Turn Signal,Display Range: ON/OFF/%
007,3,Left Side,Turn Signal,Display Range: ON/OFF/%
007,4,Right Side,Turn Signal,Display Range: ON/OFF/%
;
008,0,Footwell Lights && Xenon Shutters
008,1,Left Front,Footwell Light,Display Range: ON/OFF/%
008,2,Right Front,Footwell Light,Display Range: ON/OFF/%
008,3,Left,Xenon Shutter,Display Range: ON/OFF/%
008,4,Right,Xenon Shutter,Display Range: ON/OFF/%
;
009,0,Daytime Running Lights
009,1,Left DRL Lamp,(L174),Display Range: ON/OFF/%
009,2,Right DRL Lamp,(L175),Display Range: ON/OFF/%
;
010,1,Terminal 58,,Display Range: ON/OFF
010,2,Emergency Flasher,Button LED,Display Range: ON/OFF/%
010,3,Horn Relay (J4),,Display Range: ON/OFF
010,4,Headlamp Sys.,Clean. Relay (J39),Display Range: ON/OFF
;
011,0,Wash 'n Wipe
011,1,Front Washer,,Display Range: ON/OFF
011,2,Front Washer,,Display Range: ON/OFF
011,3,Rear Wiping,,Display Range: ON/OFF
;
012,0,CAN-Messages from Steering Column Control Module (J527)
012,1,High Beam,,Display Range: ON/OFF
012,2,High Beam Flash,,Display Range: ON/OFF
012,3,Left Signal,,Display Range: ON/OFF
012,4,Right Signal,,Display Range: ON/OFF
;
013,1,Vehicle Speed
013,2,Collective Bit,(Doors)
;
014,0,CAN-Messages from Steering Column Control Module (J527) && MMI
014,1,Wipe Message,from J527,Display Range: OFF/Tip Mode/Stage Int./Stage 1/Stage 2
014,2,Wash Message,from J527,Display Range: ON/OFF
014,3,Interval Stage,,01 = Stage 1\n05 = Stage 2\n09 = Stage 3\n13 = Stage 4
014,4,Service Position,from MMI,Display Range: ON/OFF
;
015,0,Terminal Status
015,1,Terminal 15,,Display Range: ON/OFF
015,2,Terminal X,,Display Range: ON/OFF
015,3,Terminal 50,,Display Range: ON/OFF
;
016,0,Coming/Leaving Home
016,1,Coming Home
016,2,Leaving Home,,Diesplay Range: enabled/disabled
;
017,0,LIN Slave Status
017,1,LIN Slave 1,(Wiper Control),Specification: Slave-A 1
017,2,LIN Slave 2,(Rain/Light Sensor),Specification: Slave-B 1
;
018,0,Communication Error Bit's
018,1,Wipe Angle Control,,Specification: OFF
018,2,Rain/Light Sensor,,Specification: OFF
;
019,0,Rain/Light Sensor
019,1,Light,,Display Range: ON/OFF
019,2,Brightness,,Specification: 0...7
019,3,Rain Sensor,Stream,Display Range: ON/OFF
019,4,Rain Rate,,Specification: 0...7
;
020,0,Front Wiper
020,1,Front Wiper,,Display Range: ON/OFF
020,2,Park Position,,Display Range: ON/OFF
020,3,Lower Return,Position,Display Range: ON/OFF
020,4,Upper Return,Position,Display Range: ON/OFF
;
125,0,CAN-Databus Communication (Comfort)
125,1,CAN-Gateway,,Specification: Gateway 1
125,2,Electrical,Ignition Lock,Specification: El.Ign.Lock 1
;
126,0,CAN-Databus Communication (Comfort)
126,1,Central,Convenience (J393),Specification: Central 1
126,2,Driver's Door,Control Module,Specification: Dr. Door 1
126,3,Steering Wheel,,Specification: St. Wheel 1
;
127,0,CAN-Databus Communication (Comfort)
127,1,Seat Memory,,Specification: Memory 1
127,2,Battery Manager,,Specification: Batt.Mgmt 1
127,3,Databus,Status,Display Range: 1-Wire/2-Wire/No Communication
;
;
;---------------------------------------------------
;
; selective output test
;
;---------------------------------------------------
;
;
T61,Footwell Lights
T910,Indicator Lamp for Emergency Flashers (K6)
T1759,Relay for Horn
T897,Windshield Washer Pump (V5)
T924,Relay for Headlamp Cleaning System (J39)
T967,Left Turn Signals
T968,Right Turn Signals
T978,Lamp for Low Beam: Left (M29)
T979,Lamp for Low Beam: Right (M31)
T1494,Bulb for Parking Lamps: Left (M1) 
T1498,Bulb for Parking Lamps: Right (M3)
T1496,Bulb for Fog-Lamps: Left (L22)
T1500,Bulb for Fog-Lamps: Right (L23)
T1834,Bulb for Side-Blinkers: Left (M18)
T1835,Bulb for Side-Blinkers: Right (M19)
T2377,Wiper: Upper Reverse Point
T2378,Wiper: Lower Reverse Point
T2449,Terminal 58
T2450,Bi-Xenon Shutter Solenoid (F320)
T2745,Bulb for Daytime Running Light: Left
T2746,Bulb for Daytime Running Light: Right
;
;
;---------------------------------------------------
;
; security access
;
;---------------------------------------------------
;
;
S00,Central Electronics I (J519) Security Access
S01,12151 = Adaptation Enabling
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
;A14,0,Daytime Running Lights
;
A16,0,Rear Wiper Comfort Function
A16,5,Rear Wiper Comfort Function
A16,6,If set to 1 the rear wiper will get activated if the
A16,7,front wipers are active and the reverse gear is beeing engaged.
;
A019,0,Halogen Headlights
A019,5,Halogen Headlights
A019,6,0 = Halogen Headlights at 13.5 V (Life Time Extension)
A019,7,7 = Halogen Headlights at 15.0 V
;
A026,0,Front Fog Lights
A026,5,Front Fog Lights
A026,6,0 = Front Fog Lights installed
A026,7,1 = Front Fog Lights NOT installed (Fault Code suppressed)
;
A027,0,Turn Signals in Side Rear View Mirror
A027,5,Turn Signals in Side Rear View Mirror
A027,6,0 = Turn Signals in Side Rear View Mirror active (via Central Electronics)
A027,7,1 = Turn Signals in Side Rear View Mirror inactive (via Door Control Module)
;
A028,0,Side Marker Lights
A028,5,Side Marker Lights (requires SW 0360)
A028,6,0 = Side Marker Lights installed
A028,7,1 = Side Marker Lights NOT installed (Fault Code suppressed)
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Central Electronics (J519) Coding
C01,0?xxxxx: Steering Column Memory (0 = w/o Memory OR Manual / 1 = with Memory)
C02,0x?xxxx: Footwell Lights (0 = Halogen / 1 = LED)
C03,0xx?xxx: Headlight Type
C04,0 = Halogen Headlights w/o Headlight Washer System
C05,1 = Halogen Headlights with Headlight Washer System
C06,2 = Bi-Xenon Headlights
C07,3 = Bi-Xenon Headlights with Advanced Front-Lighting System (AFS)
C08,4 = Bi-Xenon Headlights w/o Headlight Washer System
C09,5 = LED Daytime Running Lights with Headlight Washer System
C10,6 = LED Daytime Running Lights w/o Headlight Washer System
C11,7 = Halogen Headlights with separate Daytime Running Lights and with Headlight Washer System
C12,8 = Halogen Headlights with separate Daytime Running Lights and w/o Headlight Washer System
C13,9 = Bi-Xenon Headlights with LED-DRL and AFS but w/o Headlight Washer System
;9 = Bi-Xenon Headlights with LED-Daytime Running Lights and Adaptive Front Lighting System (AFS) but w/o Headlight Washer System
C14,0xxx?xx: Automatic Driving Light
C15,0 = w/o Automatic Driving Light (Auto)
C16,1 = with Automatic Driving Light (Auto) with Rain/Light Sensor (G397)
C17,2 = with High Beam Assist
C18,0xxxx?x: Daytime Running Lights (DRL)
C19,0 = w/o Daytime Running Lights
C20,1 = with Daytime Running Lights (not selectable via MMI)
C21,2 = with Daytime Running Lights (selectable via MMI)
C22,0xxxxx?: Coutry
C23,1 = Rest of World (RoW) / 2 = Northern European Countries
C24,3 = United States of America (USA) / 4 = Canada
;
