[Version]
Signature="$Windows NT$"
DriverPackageType=PlugAndPlay
DriverPackageDisplayName=%DESC%
Class=USB
ClassGUID={36fc9e60-c465-11cf-8056-444553540000}
Provider=%RossTech%
CatalogFile=RT-USB.CAT
DriverVer=05/12/2014,2.10.00

[SourceDisksNames]
1=%DriversDisk%,,,

[SourceDisksFiles]
RT-USB.SYS = 1
RT-USB.DLL = 1

[DestinationDirs]
RT-USB.NT.Copy = 10,system32\drivers
RT-USB.NT.Copy2 = 10,system32

[Manufacturer]
%RossTech%=RossTechHw

[RossTechHw]
%USB\VID_0403&PID_FA20.DeviceDesc%=RT-USB,USB\VID_0403&PID_FA20
%USB\VID_0403&PID_FA23.DeviceDesc%=RT-USB,USB\VID_0403&PID_FA23
%USB\VID_0403&PID_FA24.DeviceDesc%=RT-USB,USB\VID_0403&PID_FA24
%USB\VID_0403&PID_FA25.DeviceDesc%=RT-USB,USB\VID_0403&PID_FA25

[ControlFlags]
ExcludeFromSelect=*

[RT-USB.NT]
CopyFiles=RT-USB.NT.Copy,RT-USB.NT.Copy2
AddReg=RT-USB.NT.AddReg

[RT-USB.NT.HW]
AddReg=RT-USB.NT.HW.AddReg

[RT-USB.NT.HW.AddReg]
HKR,,"ConfigData",0x00010001,0

[RT-USB.NT.Services]
AddService = RT-USB, 0x00000002, RT-USB.NT.AddService


[RT-USB.NT.AddService]
DisplayName = %SvcDesc%
ServiceType = 1 ; SERVICE_KERNEL_DRIVER
StartType = 3 ; SERVICE_DEMAND_START
ErrorControl = 1 ; SERVICE_ERROR_NORMAL
ServiceBinary = %10%\system32\drivers\RT-USB.SYS
LoadOrderGroup = Base
AddReg = RT-USB.NT.AddService.AddReg

[RT-USB.NT.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,RT-USB.SYS

[RT-USB.NT.AddService.AddReg]
;HKR,Parameters,"LocIds",1,31,00,00,00,32,00,00,00,00
;HKR,Parameters,"RetryResetCount",0x10001,50


[RT-USB.NT.Copy]
RT-USB.SYS

[RT-USB.NT.Copy2]
RT-USB.DLL

[Strings]
RossTech="Ross-Tech"
DESC="USB Driver Package"
DriversDisk="The folder where you installed the Ross-Tech software"
USB\VID_0403&PID_FA20.DeviceDesc="Ross-Tech HEX or KEY USB Interface"
USB\VID_0403&PID_FA23.DeviceDesc="Ross-Tech Micro-CAN Interface"
USB\VID_0403&PID_FA24.DeviceDesc="Ross-Tech Direct USB Interface"
USB\VID_0403&PID_FA25.DeviceDesc="Ross-Tech USB Converter"
SvcDesc="Ross-Tech USB driver"
ClassName="USB"

