;
; VCDS Label File
;
; Copyright © 2005+ Ross-Tech, LLC
;
; Audi A4 (8EC/8ED)
;
; Component: J519 - Central Clectronic (#09)
;
; P/N: 8E0-907-279-???
;
; includes measuring blocks, adaptation and coding
;
; created on 14/Apr/2005 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 07/Oct/2014
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,(Output Signals)
001,1,Supply Voltage
001,2,Horn,,Display Range: ON/OFF
001,3,Status,Terminal 75,Display Range: ON/OFF
001,4,Rotary Light Switch,Supply,Display Range: ON/OFF
;
002,0,Turn Signals (Output Signals)
002,1,Turn Signals,Front Left,Display Range: 0.0...100.0 %
002,2,Turn Signals,Rear Left,Display Range: 0.0...100.0 %
002,3,Turn Signals,Front Right,Display Range: 0.0...100.0 %
002,4,Turn Signals,Rear Right,Display Range: 0.0...100.0 %
;
003,0,Parking Lights (Output Signals)
003,1,Parking Light,Front Left,Display Range: 0.0...100.0 %
003,2,Parking Light,Rear Left,Display Range: 0.0...100.0 %
003,3,Parking Light,Front Right,Display Range: 0.0...100.0 %
003,4,Parking Light,Rear Right,Display Range: 0.0...100.0 %
;
004,0,(Output Signals)
004,1,High Beam,Left,Display Range: 0.0...100.0 %
004,2,High Beam,Right,Display Range: 0.0...100.0 %
004,3,License Plate,Light,Display Range: 0.0...100.0 %
004,4,Emergency Flasher,Illumination,Display Range: 0.0...100.0 %
;
005,0,Brake Lights (Output Signals)
005,1,Brake Light,Left,Display Range: 0.0...100.0 %
005,2,Brake Light,Right,Display Range: 0.0...100.0 %
005,3,Brake Light,Center,Display Range: 0.0...100.0 %
;
006,0,Back-Up && Fog Lights (Output Signals)
006,1,Back-Up Light,Rear Left,Display Range: 0.0...100.0 %
006,2,Back-Up Light,Rear Right,Display Range: 0.0...100.0 %
006,3,Fog Light,Rear Left,Display Range: 0.0...100.0 %
006,4,Fog Light,Rear Right,Display Range: 0.0...100.0 %
;
007,0,Wiping && Washing (Output Signals)
007,1,Front Wiping,Display Range: ON/OFF
007,2,Rear Washing,Display Range: ON/OFF
007,3,Rear Wiping,Display Range: ON/OFF
007,4,Rear Washing,Display Range: ON/OFF
;
008,0,(Input Signals)
008,1,Rotary Light Switch
008,2,Emergency,Flasher Button,Display Range: Not Oper./Activated
008,3,Status,Terminal 75,Display Range: ON/OFF
008,4,Wiper Zero,Position,Display Range: ON/OFF
;
009,0,(Input Signals)
009,1,Brake Light Switch,(from J519),Display Range: Not Oper./Activated
009,2,Brake Light Switch,(via CAN),Display Range: Not Oper./Activated
009,3,Brake Test Switch,(via CAN),Display Range: Not Oper./Activated
009,4,Reverse Gear,(via CAN),Display Range: Not Oper./Activated
;
010,0,High Beam && Turn Signals (Input Signals)
010,1,High Beam,,Display Range: Not Oper./Activated
010,2,High Beam Flash,,Display Range: Not Oper./Activated
010,3,Turn Signal Left,,Display Range: Not Oper./Activated
010,4,Turn Signal Right,,Display Range: Not Oper./Activated
;
011,0,Wiping && Washing (Input Signals)
011,1,Front Wiping,Display Range: ON/OFF
011,2,Rear Washing,Display Range: ON/OFF
011,3,Rear Wiping,Display Range: ON/OFF
011,4,Rear Washing,Display Range: ON/OFF
;
012,0,(Input Signals)
012,1,Status,Terminal 15
012,2,Status,S-Contact
012,3,Interval Steps
;
013,0,Low Beam && Fog Light (Output Signals)
013,1,Low Beam Left,,Display Range: 0.0...100.0 %
013,2,Low Beam Right,,Display Range: 0.0...100.0 %
013,3,Fog Light Left,,Display Range: 0.0...100.0 %
013,4,Fog Light Right,,Display Range: 0.0...100.0 %
;
014,0,High Beam Shutter & Headlight Washer (Output Signals)
014,1,High Beam Shutter,,Display Range: ON/OFF
014,2,Headlight Washer,System,Display Range: ON/OFF
;
015,0,Daytime Running Light && Coming Home Switch (Input Signals)
015,1,Daytime Running,Light Switch,Display Range: Not Oper./Activated
015,2,Coming-Home,Switch,Display Range: Not Oper./Activated
;
016,0,(Input Signals)
016,1,Status,Driver'S Door,Display Range: Door Open/Door Closed
016,2,Vehicle Speed
016,3,Outside,Temperature
;
017,0,Rain/Light Sensor (LIN Signals)
017,1,Rain/Light Sensor,Meas. Malfunction
017,2,Rain/Light Sensor,Comm. Malfunction
017,3,Rain/Light Sensor,Low Voltage
017,4,Rain/Light Sensor,Excessive Voltage
;
018,0,Rain/Light Sensor (LIN Signals)
018,1,Rain/Light Sensor,ADP Malfunction
018,2,Rain/Light Sensor,ADP Malfunction
018,3,Rain Sensor,Malfunction,Display Range: ON/OFF
018,4,Light Sensor,Malfunction,Display Range: ON/OFF
;
019,0,Rain Sensor (LIN Signals)
019,1,Wiper Speed
019,2,Rain Rate
;
020,0,Light Sensor (LIN Signals)
020,1,Light,,Display Range: ON/OFF
020,2,Light (inverse),,Display Range: ON/OFF
020,3,Dark/Bright,,Display Range: ON/OFF
020,4,Brightness
;
050,0,LIN-Databus (LIN Signals)
050,1,LIN-Sensor,Identification
;
080,0,Advanced Control Module Identification I
080,1,Identification
080,2,Revision
080,3,Production,Date
080,4,Manufacturer &,Test Stand Number
;
081,0,Advanced Control Module Identification II
081,1,Vehicle Ident.,Number (VIN)
;
125,0,CAN-Databus Communication (Comfort)
125,1,Instrument Cluster,,Specification: Instruments 1
125,2,Steering Wheel,Electronics,Specification: St. Wheel 1
125,3,Comfort System,,Specification: Central 1
125,4,Trailer Electronics,,Specification: Trailer 1
;
126,0,CAN-Databus Communication (Comfort)
126,1,Door Electronics,Driver's Door,Specification: Dr. Door 1
;
127,0,LIN-Databus Communication
127,1,Rain/Light Sensor,,Specification: Slave-A 1
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Central Electronics (J519) Coding
C01,?xxxx: Chassis
C02,0 = Limousine (PR-K8B)
C03,1 = Avant (PR-K8D)
C04,2 = Cabriolet (PR-K8K)
C05,x?xxx: Driving Light Switch
C06,0 = Rain/Light Sensor (G397) not installed (PR-8K0/8K1/9C6/8K4)
C07,1 - Rain/Light Sensor (G397) installed (PR-8K3/8K7/9C7/8K9)
C08,xx?xx: Trailer Hitch
C09,0 = Trailer Hitch not installed (PR-1D0)
C10,1 = Trailer Hitch installed (PR-1D2)
C11,xxx?x: Headlights
C12,0 = Halogen Headlights w/o Daytime Running Lights (PR-8Q0/8Q1+8K0/8K7)
C13,1 = Halogen Headlights with Daytime Running Lights (PR-8Q0/8Q1+8K1/8K3/9C6/9C7)
C14,2 = Bi-Xenon Headlights with Daytime Running Lights (PR-8Q3/8Q5+8K9/8K4)
C15,3 = Bi-Xenon Headlights w/o Daytime Running Lights (PR-8Q3/8Q5+8K0/8K7)
C16,4 = Bi-Xenon Headlights with Daytime Running/Tail/License Plate Lights (PR-8Q3/8Q5+8K1/8K3)
C17,xxxx?: Country
C18,1 = Rest of World/Nordic Countries/Denmark/Croatia/Baltic Countries with Bi-Xenon
C19,2 = Nordic Countries/Denmark/Croatia/Baltic Countries without Bi-Xenon
C20,3 = USA/Canada with Bi-Xenon
C21,4 = Canada without Bi-Xenon
C22,5 = Special Vehicles
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A001,0,Coming Home Time
A001,5,Coming Home Time
A001,6,Activation Time of the Coming Home Lighting.
A001,7,Standard: 30 Seconds
A001,8,Range: 0...60
A001,9,Increments: 1 Second
;
A002,0,Brake Light Dimming
A002,5,Brake Light Dimming
A002,6,Standard: 30 %
A002,7,Range: 13...40 %
;
A003,0,Tail Light Dimming
A003,5,Tail Light Dimming
A003,6,Standard: 32 %
A003,7,Range: 13...40 %
;
A004,0,Rear Fog Light Dimming
A004,5,Rear Fog Light Dimming
A004,6,Standard: 28 %
A004,7,Range: 13...40 %
;
A005,0,Daytime Running Lights Dimming (Low Beam)
A005,5,Daytime Running Lights Dimming (Low Beam)
A005,6,Affective with Halogen only.
A005,7, 
A005,8,Standard: 92 %
A005,9,Range: 51...100 %
;
A006,0,Daytime Running Lights Dimming (High Beam)
A006,5,Daytime Running Lights Dimming (High Beam)
A006,6,Affective with Bi-Xenon only.
A006,7, 
A006,8,Standard: 70 %
A006,9,Range: 51...100 %
;
A007,0,Daytime Running Lights Dimming (Fog Lights)
A007,5,Daytime Running Lights Dimming (Fog Lights)
A007,6,Affective for Canada only.
A007,7, 
A007,8,Standard: 92 %
A007,9,Range: 51...100 %
;
A008,0,Daytime Running Lights
A008,5,Daytime Running Lights
A008,6,Standard: 1 (ON)
A008,7, 
A008,8,0 = Daytime Running Lights OFF
A008,9,1 = Daytime Running Lights ON
;
A009,0,Switch-Off Delay (Low Beam)
A009,5,Switch-Off Delay (Low Beam)
A009,6,Low Beam Switch-Off Delay with Light Switch in AUTO Position.
A009,7, 
A009,8,Standard: 51
A009,9,Range: 0...64
;
A010,0,Low Beam Response
A010,5,Low Beam Response
A010,6,0 = Parking Lights OFF after Terminal S OFF
A010,7,1 = Parking Lights Remain ON after Terminal 15 OFF
;
A011,0,Low Beam Response (Terminal 15)
A011,5,Low Beam Response (Terminal 15)
A011,6,0 = No Parking Lights
A011,7,1 = Alarm at Door Open
A011,8,2 = Parking Lights OFF at Door Open
;
A012,0,Highway/Comfort Blinking
A012,5,Highway/Comfort Blinking
A012,6,0 = Highway/Comfort Blinking OFF
A012,7,1 = Highway/Comfort Blinking ON
;
A013,0,Wiper Setup
A013,5,Wiper Setup
A013,6,Standard: 115
A013,7, 
A013,8,+001 = Speed Reset
A013,9,+002 = Short to Plus Monitoring
A013,10,+004 = Rain Sensor active
A013,11,+008 = Long Post Wiping after Washing (Drop/Tear Wiping)
A013,12,+016 = Speed dependent Wiper interval active
A013,13,+032 = Headlight Washer System active
A013,14,+064 = Reverse Gear Wiping active
;
A014,0,NAR Parking Light Deactivation
A014,5,NAR Parking Light Deactivation
A014,6,0 = Parking Lights inactive
A014,7,1 = Parking Lights active
;
A016,0,Fog Light Cold Diagnosis
A016,5,Fog Light Cold Diagnosis
A016,6,0 = Fog Light Cold Lamp Diagnosis active
A016,7,1 = Fog Light Cold Lamp Diagnosis inactive (i.e. for DTM Edition)
;
A020,0,Rain-/Light Sensor Setup
A020,5,Rain-/Light Sensor Setup
A020,6,Standard: 2
A020,7, 
A020,8,+01 = Highway Light
A020,9,+02 = Rain Light
;+04 = Rain Closing (Sunroof & Windows)
;Not Supported by Audi/Seat Models
;
A021,0,Assistance Light Sensor Correction
A021,5,Assistance Light Sensor Correction
A021,6,Standard: 59 %
;
A022,0,Transmission Grade (Front Window)
A022,5,Transmission Grade (Front Window)
A022,6,Rain Sensor Transmission Grade at 880 nm.
A022,7, 
A022,8,Standard: 45 %
;
A081,0,Component Protection (Vehicle Identification Number)
A081,5,Component Protection (Vehicle Identification Number)
A081,6,To Start the Vehicle Identification Number (VIN)
A081,7,Learning Process enter/save 46992 as new Value.
;
