;
; VCDS Label File
;
; Copyright © 2006+ Ross-Tech, LLC
;
; Audi A4 (8D) / Audi A6 (4B)
;
; Component: Engine (#01) - AGB/AJK/APB/ARE/AZA/AZB/BEL/BES
;
; P/N: 4B0-907-551-??? / 4Z7-907-551-??? / 8D0-907-551-???
;
; includes measuring blocks, coding, login, adaptation and misc
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 4B-01.LBL
; 4Z-01.LBL
; 8D-01.LBL
; 078-907-551-AZA.LBL  (2.7l T   @ 230-265 HP - AGB/AJK/APB/ARE/AZA/AZB/BEL/BES)
;
; created on 10/Mar/2006 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modificationon on 11/May/2012
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
000,0,General
000,1,Coolant Temperature (G62),Specification: 177...203 (85.0...105.0 °C)
000,2,Engine Load,Specification: 21...34 (15.0...26.0 %)
000,3,Engine Speed (G28),Specification: 67...73 (650...750 RPM)
000,4,Throttle Valve Angle,1...7 (0.40...2.75 %)
000,5,Idle Torque,Specification: 126...135 (-1.5...+1.5 %)
000,6,Torque Loss at Idle,Specification: 124...140 (-3.0...+5.0 %)
000,7,Mixture Adaptation Bank 1 Control Value (Idle),Specification: 122...136 (-4.0...+4.0 %)
000,8,Mixture Adaptation Bank 2 Control Value (Partial),Specification: 122...136 (-4.0...+4.0 %)
000,9,Mixture Adaptation Bank 1 Learned Value (Idle),Specification: 108...148 (-4.0...+4.0 %)
000,10,Mixture Adaptation Bank 2 Learned Value (Partial),Specification: 108...148 (-4.0...+4.0 %)
;
001,0,General
001,1,Engine Speed,(G28),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
001,2,Coolant,Temperature (G62),Specification: 80.0...110.0 °C
001,3,Lambda Control,Bank 1,Range: -25.0...+25.0 %\nSpecification: -10.0...+10.0 %
001,4,Lambda Control,Bank 2,Range: -25.0...+25.0 %\nSpecification: -10.0...+10.0 %
;
002,0,General
002,1,Engine Speed,(G28),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
002,2,Engine Load,,Specification (Idle): 15.0...25.0 %\nRange: 15.0...175.0 %
002,3,Injection Timing,,Specification (Idle): 2.0...4.0 ms
002,4,Mass Air Flow,(G70),Specification (Load): min. 180.0 g/s
;
003,0,General
003,1,Engine Speed,(G28),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
003,2,Mass Air Flow,(G70),Specification (Load): min. 180.0 g/s
003,3,Throttle Valve Angle
003,4,Ignition,Timing Angle
;
004,0,General
004,1,Engine Speed,(G28),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
004,2,Battery Voltage,(Terminal 30),Specification: 11.0...15.0 V
004,3,Coolant,Temperature (G62),Specification: 80.0...110.0 °C
004,4,Intake Air,Temperature (G42)
;
005,0,General
005,1,Engine Speed,(G28),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
005,2,Engine Load,,Specification (Idle): 15.0...25.0 %\nRange: 15.0...175.0 %
005,3,Vehicle Speed
005,4,Load Status,,Display Range: Idle/Partial Throttle/Wide Open Throttle (WOT)/Enrichment/Deceleration
;
006,0,General
006,1,Engine Speed,(G28),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
006,2,Engine Load,,Specification (Idle): 15.0...25.0 %\nRange: 15.0...175.0 %
006,3,Intake Air,Temperature (G42)
006,4,Altitude,Correction Factor
;
010,0,Ignition
010,1,Engine Speed,(G28),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
010,2,Engine Load,,Specification (Idle): 15.0...25.0 %\nRange: 15.0...175.0 %
010,3,Throttle Valve Angle
010,4,Ignition,Timing Angle
;
011,0,Ignition
011,1,Engine Speed,(G28),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
011,2,Coolant,Temperature (G62),Specification: 80.0...110.0 °C
011,3,Intake Air,Temperature (G42)
011,4,Ignition,Timing Angle
;
014,0,Ignition (Misfire Recognition - Total)
014,1,Engine Speed,(G28),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
014,2,Engine Load,,Specification (Idle): 15.0...25.0 %\nRange: 15.0...175.0 %
014,3,Misfire,(total),Specification: 0...15
014,4,Misfire,Recognition,Range: Disabled/Enabled
;
015,0,Ignition (Misfire Recognition - Cylinder 1-3)
015,1,Misfire Counter,Cylinder 1,Specification: 0...15
015,2,Misfire Counter,Cylinder 2,Specification: 0...15
015,3,Misfire Counter,Cylinder 3,Specification: 0...15
015,4,Misfire,Recognition,Range: Disabled/Enabled
;
016,0,Ignition (Misfire Recognition - Cylinder 4-6)
016,1,Misfire Counter,Cylinder 4,Specification: 0...15
016,2,Misfire Counter,Cylinder 5,Specification: 0...15
016,3,Misfire Counter,Cylinder 6,Specification: 0...15
016,4,Misfire,Recognition,Range: Disabled/Enabled
;
018,0,RPM/Load Barriers
018,1,Lower,RPM Barrier
018,2,Upper,RPM Barrier
018,3,Lower,Load Barrier
018,4,Upper,Load Barrier
;
020,0,Ignition (Timing Retardation Cylinder 1-4)
020,1,Timing Retardation,Cylinder 1,Specification: 0.0...12.0 CF
020,2,Timing Retardation,Cylinder 2,Specification: 0.0...12.0 CF
020,3,Timing Retardation,Cylinder 3,Specification: 0.0...12.0 CF
020,4,Timing Retardation,Cylinder 4,Specification: 0.0...12.0 CF
;
021,0,Ignition (Timing Retardation Cylinder 5-8)
021,1,Timing Retardation,Cylinder 5,Specification: 0.0...12.0 CF
021,2,Timing Retardation,Cylinder 6,Specification: 0.0...12.0 CF
;
022,0,Ignition (Timing Retardation Cylinder 1 && 2)
022,1,Engine Speed,(G28),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
022,2,Engine Load,,Specification (Idle): 15.0...25.0 %\nRange: 15.0...175.0 %
022,3,Timing Retardation,Cylinder 1,Specification: 0.0...12.0 CF
022,4,Timing Retardation,Cylinder 2,Specification: 0.0...12.0 CF
;
023,0,Ignition (Timing Retardation Cylinder 3 && 4)
023,1,Engine Speed,(G28),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
023,2,Engine Load,,Specification (Idle): 15.0...25.0 %\nRange: 15.0...175.0 %
023,3,Timing Retardation,Cylinder 3,Specification: 0.0...12.0 CF
023,4,Timing Retardation,Cylinder 4,Specification: 0.0...12.0 CF
;
024,0,Ignition (Timing Retardation Cylinder 5 && 6)
024,1,Engine Speed,(G28),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
024,2,Engine Load,,Specification (Idle): 15.0...25.0 %\nRange: 15.0...175.0 %
024,3,Timing Retardation,Cylinder 5,Specification: 0.0...12.0 CF
024,4,Timing Retardation,Cylinder 6,Specification: 0.0...12.0 CF
;
026,0,Ignition (Knock Control Cylinder 1-4)
026,1,Voltage,Cylinder 1
026,2,Voltage,Cylinder 2
026,3,Voltage,Cylinder 3
026,4,Voltage,Cylinder 4
;
027,0,Ignition (Knock Control Cylinder 5-6)
027,1,Voltage,Cylinder 5
027,2,Voltage,Cylinder 6
;
028,0,Ignition (Knock Sensor Test - Short Trip)
028,1,Engine Speed,(G28),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
028,2,Engine Load,,Specification (Idle): 15.0...25.0 %\nRange: 15.0...175.0 %
028,3,Coolant,Temperature (G62),Specification: 80.0...110.0 °C
028,4,Result,,Range: Test ON/Test OFF/Syst. OK/Syst. not OK\nSpecification: Syst. OK
;
030,0,Lambda Control (Sensor Status)
030,1,Bank 1,Sensor 1,Specification: 111\n\n1xx - Lambda Sensor Heating ON\nx1x - Lambda Sensor ready\nxx1 - Lambda Control active
030,2,Bank 1,Sensor 2,Specification: 110\n\n1xx - Lambda Sensor Heating ON\nx1x - Lambda Sensor ready\nxx1 - Lambda Control active
030,3,Bank 2,Sensor 1,Specification: 111\n\n1xx - Lambda Sensor Heating ON\nx1x - Lambda Sensor ready\nxx1 - Lambda Control active
030,4,Bank 2,Sensor 2,Specification: 110\n\n1xx - Lambda Sensor Heating ON\nx1x - Lambda Sensor ready\nxx1 - Lambda Control active
;
031,0,Lambda Control
031,1,Bank 1 Sensor 1,(actual),Range: 0.000...1.000 V
031,2,Bank 1 Sensor 1,(specified),Range: 0.000...1.000 V
031,3,Bank 2 Sensor 1,(actual),Range: 0.000...1.000 V
031,4,Bank 2 Sensor 1,(specified),Range: 0.000...1.000 V
;
032,0,Lambda Control (Mixture Adaptation)
032,1,Adaptation (Idle),Bank 1 Sensor 1,Range: -25.0...+25.0 %\nSpecification: -4.0...+4.0 %
032,2,Adaptation (Partial),Bank 1 Sensor 1,Range: -25.0...+25.0 %\nSpecification: -4.0...+4.0 %
032,3,Adaptation (Idle),Bank 2 Sensor 1,Range: -25.0...+25.0 %\nSpecification: -4.0...+4.0 %
032,4,Adaptation (Partial),Bank 2 Sensor 1,Range: -25.0...+25.0 %\nSpecification: -4.0...+4.0 %
;
033,0,Lambda Control
033,1,Lambda Control,Bank 1 Sensor 1,Range: -25.0...+25.0 %\nSpecification: -4.0...+4.0 %
033,2,Sensor Voltage,Bank 1 Sensor 1,Range: 0.000...1.000 V
033,3,Lambda Control,Bank 2 Sensor 1,Range: -25.0...+25.0 %\nSpecification: -4.0...+4.0 %
033,4,Sensor Voltage,Bank 2 Sensor 1,Range: 0.000...1.000 V
;
034,0,Lambda Control (Lambda Sensor Aging - Bank 1 Sensor 1)
034,1,Engine Speed,(G28),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
034,2,Catalytic Converter,Bank 1 Temp.,Range: 70.0...850.0 °C\nSpecification: min. 260.0 °C
034,3,Dynamic Factor,Bank 1 Sensor 1,Range: 0.0...3.0 s\nSpecification: 0.1...1.0 s
034,4,Result,Lambda Aging,Range: Test ON/Test OFF/B1-S1 not OK/B1-S1 OK\nSpecification: B1-S1 OK
;
035,0,Lambda Control (Lambda Sensor Aging - Bank 2 Sensor 1)
035,1,Engine Speed,(G28),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
035,2,Catalytic Converter,Bank 2 Temp.,Range: 70.0...850.0 °C\nSpecification: min. 260.0 °C
035,3,Dynamic Factor,Bank 2 Sensor 1,Range: 0.0...3.0 s\nSpecification: 0.1...1.0 s
035,4,Result,Lambda Aging,Range: Test ON/Test OFF/B2-S1 not OK/B2-S1 OK\nSpecification: B2-S1 OK
;
036,0,Lambda Control (Sensor Readiness - After Catalyst)
036,1,Sensor Voltage,Bank 1 Sensor 2,Range: 0.000...1.000 V
036,2,Result,Lambda Availability,Range: Test ON/Test OFF/B1-S2 not OK/B1-S2 OK\nSpecification: B1-S2 OK
036,3,Sensor Voltage,Bank 2 Sensor 2,Range: 0.000...1.000 V
036,4,Result,Lambda Availability,Range: Test ON/Test OFF/B2-S2 not OK/B2-S2 OK\nSpecification: B2-S2 OK
;
037,0,Lambda Control (Correction Bank 1)
037,1,Engine Load,,Specification (Idle): 15.0...25.0 %\nRange: 15.0...175.0 %
037,2,Sensor Voltage,Bank 1 Sensor 2,Range: 0.000...1.000 V
037,3,Correction Value,Bank 2,Specification: -500.0...+500.0 ms\nRange: -1200.0...+1200.0 ms
037,4,Result,,Range: Test ON/Test OFF/Syst. OK/Syst. n.OK\nSpecification: Syst. OK
;
038,0,Lambda Control (Correction Bank 2)
038,1,Engine Load,,Specification (Idle): 15.0...25.0 %\nRange: 15.0...175.0 %
038,2,Sensor Voltage,Bank 2 Sensor 2,Range: 0.000...1.000 V
038,3,Correction Value,Bank 2,Specification: -500.0...+500.0 ms\nRange: -1200.0...+1200.0 ms
038,4,Result,,Range: Test ON/Test OFF/Syst. OK/Syst. n.OK\nSpecification: Syst. OK
;
041,0,Lambda Control (Lambda Sensor Heating Bank 1)
041,1,Resistance,Bank 1 Sensor 1,Specification: 0.0...0.5 kOhm
041,2,Heater Condition,Bank 1 Sensor 1,Range: Htg. S1 OFF/Htg. S1 ON
041,3,Resistance,Bank 1 Sensor 2,Specification: 0.0...0.5 kOhm
041,4,Heater Condition,Bank 1 Sensor 2,Range: Htg. S2 OFF/Htg. S2 ON
;
042,0,Lambda Control (Lambda Sensor Heating Bank 2)
042,1,Resistance,Bank 2 Sensor 1,Specification: 0.0...0.5 kOhm
042,2,Heater Condition,Bank 2 Sensor 1,Range: Htg. S1 OFF/Htg. S1 ON
042,3,Resistance,Bank 2 Sensor 2,Specification: 0.0...0.5 kOhm
042,4,Heater Condition,Bank 2 Sensor 2,Range: Htg. S2 OFF/Htg. S2 ON
;
043,0,Lambda Control (Lambda Sensor Aging - Bank 1 Sensor 2)
043,1,Engine Speed,(G28),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
043,2,Catalytic Converter,Bank 1 Temp.,Range: 70.0...850.0 °C\nSpecification: min. 320.0 °C
043,3,Sensor Voltage,Bank 1 Sensor 2,Range: 0.000...1.000 V
043,4,Result,Aging Check,Display Range: Test ON/Test OFF/B1-S2 OK/B1-S2 n.OK\nSpecification: B1-S2 OK
;
044,0,Lambda Control (Lambda Sensor Aging - Bank 2 Sensor 2)
044,1,Engine Speed,(G28),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
044,2,Catalytic Converter,Bank 2 Temp.,Range: 70.0...850.0 °C\nSpecification: min. 320.0 °C
044,3,Sensor Voltage,Bank 2 Sensor 2,Range: 0.000...1.000 V
044,4,Result,Aging Check,Display Range: Test ON/Test OFF/B2-S2 OK/B2-S2 n.OK\nSpecification: B2-S2 OK
;
046,0,Lambda Control (Catalytic Conversion Test Bank 1)
046,1,Engine Speed,(G28),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
046,2,Catalytic Converter,Bank 1 Temp.,Range: 70.0...850.0 °C\nSpecification: min. 350.0 °C
046,3,Catalytic,Conversion Bank 1,Range: 0.00...0.99\nSpecification: 0.00...0.80
046,4,Result,Cat. Conversion,Display Range: Test ON/Test OFF/CatB1 OK/CatB1 n.OK\nSpecification: CatB1 OK
;
047,0,Lambda Control (Catalytic Conversion Test Bank 2)
047,1,Engine Speed,(G28),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
047,2,Catalytic Converter,Bank 2 Temp.,Range: 70.0...850.0 °C\nSpecification: min. 350.0 °C
047,3,Catalytic,Conversion Bank 2,Range: 0.00...0.99\nSpecification: 0.00...0.80
047,4,Result,Cat. Conversion,Display Range: Test ON/Test OFF/CatB2 OK/CatB2 n.OK\nSpecification: CatB2 OK
;
050,0,Engine Speed Increase
050,1,Engine Speed,(actual),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
050,2,Engine Speed,(specified)
050,3,A/C Readiness,,Range: A/C-Low / A/C-High
050,4,A/C Compressor,,Range: Compr.OFF/Compr.ON
;
051,0,Engine Speed Increase (Gear Shifts)
051,1,Engine Speed,(actual),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
051,2,Engine Speed,(specified)
051,3,Selected Gear,,Range: P or N = 0/Gear = 1 - 6/R = 7
051,4,Battery Voltage,(Terminal 30),Specification: 11.0...15.0 V
;
053,0,Engine Speed Increase (Generator Load)
053,1,Engine Speed,(actual),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
053,2,Engine Speed,(specified)
053,3,Battery Voltage,(Terminal 30),Specification: 11.0...15.0 V
053,4,Generator Load,,Range: 0.0...100.0 %
;
054,0,Idle Speed Stabilization
054,1,Engine Speed,(G28),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
054,2,Load Status,,Range: Idle/Partial Throttle/Wide Open Throttle (WOT)/Enrichment/Deceleration
054,3,Accel. Pedal Pos.,Sensor 1 (G79),Specification: 12.0...97.0 %
054,4,Throttle Valve Angle
;
055,0,Idle Speed Stabilization
055,1,Engine Speed,(G28),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
055,2,Idle Regulator
055,3,Idle Stabilization,Self-Adaptation
055,4,Operating,Condition
; --?xx = A/C Readiness (0 = Minimum Output / 1 = Maximum Output)
; --x?x = Gear Status (0 = P/N / 1 = 2/3/4/R/D)
; --xx? = A/C Compressor (0 = OFF / 1 = ON)
;
056,0,Idle Speed Stabilization
056,1,Engine Speed,(actual),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
056,2,Engine Speed,(specified)
056,3,Idle Regulator
056,4,Operating,Condition
; --?xx = A/C Readiness (0 = Minimum Output / 1 = Maximum Output)
; --x?x = Gear Status (0 = P/N / 1 = 2/3/4/R/D)
; --xx? = A/C Compressor (0 = OFF / 1 = ON)
;
060,0,Electronic Throttle Adaptation
060,1,Throttle Valve,Sensor 1 (G187),Specification: 3.0...93.0 %
060,2,Throttle Valve,Sensor 2 (G188),Specification: 97.0...3.0 %
060,3,Throttle Adaptation,Steps Counter,Specification: 0\nRange: 0...8
060,4,Result,Throttle Valve Adp.,Range: ADP RUN/ADP OK/ADP ERROR\nSpecification: ADP OK
;
061,0,Electronic Throttle
061,1,Engine Speed,(G28),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
061,2,Battery Voltage,(Terminal 30),Specification: 11.0...15.0 V
061,3,Throttle Valve Angle
061,4,Operating,Condition
; --?xx = A/C Readiness (0 = Minimum Output / 1 = Maximum Output)
; --x?x = Gear Status (0 = P/N / 1 = 2/3/4/R/D)
; --xx? = A/C Compressor (0 = OFF / 1 = ON)
;
062,0,Electronic Throttle
062,1,Throttle Valve,Sensor 1 (G187),Specification: 3.0...93.0 %
062,2,Throttle Valve,Sensor 2 (G188),Specification: 97.0...3.0 %
062,3,Accel. Pedal Pos.,Sensor 1 (G79),Specification: 12.0...97.0 %
062,4,Accel. Pedal Pos.,Sensor 2 (G185),Specification: 4.0...49.0 %
;
063,0,Electronic Throttle (Kick-Down Adaptation)
063,1,Accel. Pedal Pos.,Sensor 1 (G79),Specification: 12.0...97.0 %
063,2,Accel. Pedal Pos.,Sensor 2 (G185),Specification: 4.0...49.0 %
063,3,Kick-Down,Switch,Range: Kick Down/Not Oper.
063,4,Kick-Down,Adaptation,Range: ADP RUN/ADP OK/ADP ERROR\nSpecification: ADP OK
;
064,0,Throttle Valve Sensor Adaption Values
064,1,Lower Adaptation,Sensor 1 (G187)
064,2,Lower Adaptation,Sensor 2 (G188)
064,3,Emergency Air Gap,Sensor 1 (G187)
064,4,Emergency Air Gap,Sensor 2 (G188)
;
066,0,Cruise Control System
066,1,Vehicle Speed,(current)
066,2,Switch Positions I
; 1xxx = Cruise Control System active
; x1xx = Clutch operated (always 1 with Automatic Transmission)
; xx1x = Brake operated (Brake Pedal Switch)
; xxx1 = Brake operated (Brake Light Switch)
066,3,Vehicle Speed,(specified)
066,4,Switch Positions II
;
070,0,Emission Reduction (TEV - Basic Setting)
070,1,Evap. Emissions,Sol. Valve,Range: 0.0...100.0 %
070,2,Lambda Control,(During Diagnosis),Range: -25.0...+25.0 %\nSpecification: -5.0...+4.0 %
070,4,Result,,Range: Test ON/Test OFF/TEV OK/TEV not OK
;
071,0,Emission Reduction (Basic Setting: Leak Diagnostic System)
071,1,Reed Contact,Condition,Range: Reed Open/Reed Closed
071,4,Result,Leak Test,Range: Test ON/Test OFF/Syst. OK/Syst. not OK
;
077,0,Emission Reduction (Secondary Air Injection System Bank 1)
077,1,Engine Speed,(G28),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
077,2,Mass Air Flow,(G70),Specification (Load): min. 180.0 g/s
077,3,Secondary Air,System Air Mass,Range: -100.0...+10.0 %
077,4,Result,,Range: Test ON/Test OFF/Syst. OK/Syst. not OK
;
078,0,Emission Reduction (Secondary Air Injection System Bank 2)
078,1,Engine Speed,(G28),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
078,2,Mass Air Flow,(G70),Specification (Load): min. 180.0 g/s
078,3,Secondary Air,System Air Mass,Range: -100.0...+10.0 %
078,4,Result,,Range: Test ON/Test OFF/Syst. OK/Syst. not OK
;
081,0,Advanced Control Module Identification II
;
082,0,Advanced Control Module Identification III
;
089,0,On-Board-Diagnostics (OBD)
089,1,Distance Driven,with MIL on
089,2,Tank Condition,,Display Range: OK/too low
;
090,0,Continuous Camshaft Adjustment (Intake)
090,1,Engine Speed,(G28),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
090,2,Adjustment,Status,Range: Cam Ctrl. ON/Cam Ctrl. OFF
090,3,Adjustment,Bank 1
090,4,Adjustment,Bank 2
;
091,0,Continuous Camshaft Adjustment (Intake - Bank 1)
091,1,Engine Speed,(G28),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
091,2,Engine Load,,Specification (Idle): 15.0...25.0 %\nRange: 15.0...175.0 %´
091,3,Adjustment,Status,Range: Cam Ctrl. ON/Cam Ctrl. OFF
091,4,Adjustment,Bank 1
;
092,0,Continuous Camshaft Adjustment (Intake - Bank 2)
092,1,Engine Speed,(G28),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
092,2,Engine Load,,Specification (Idle): 15.0...25.0 %\nRange: 15.0...175.0 %
092,3,Adjustment,Status,Range: Cam Ctrl. ON/Cam Ctrl. OFF
092,4,Adjustment,Bank 2
;
093,0,Continuous Camshaft Adjustment (Phase Position - Bank 1 && 2)
093,1,Engine Speed,(G28),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
093,2,Engine Load,,Specification (Idle): 15.0...25.0 %\nRange: 15.0...175.0 %
093,3,Phase Position,Bank 1,Range: -20.3...+14.8 CF\nSpecification (Idle): 0 CF (± 6 CF)
093,4,Phase Position,Bank 2,Range: -20.3...+14.8 CF\nSpecification (Idle): 0 CF (± 6 CF)
;
094,0,Continuous Camshaft Adjustment (Intake)
094,1,Engine Speed,(G28),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
094,2,Adjustment,Status,Range: Cam Ctrl. ON/Cam Ctrl. OFF
094,3,Result,Bank 1,Range: Test ON/Test OFF/Syst. OK/Syst. not OK\nSpecification: Syst. not OK
094,4,Result,Bank 2,Range: Test ON/Test OFF/Syst. OK/Syst. not OK\nSpecification: Syst. not OK
;
099,0,Lambda Control Shut-Off (Basic Setting)
099,1,Engine Speed,(G28),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
099,2,Coolant,Temperature (G62),Specification: 80.0...110.0 °C
099,3,Lambda Control
099,4,Lambda Control,Status,Display Range: O2-Reg.OFF/O2-Reg.ON
;
100,0,Readiness Code
100,1,Readiness Bits
; 1xxxxxxx - Exhaust Gas Recirculation (EGR)
; x1xxxxxx - Sensor Heater
; xx1xxxxx - Oxygen Sensors
; xxx1xxxx - A/C System
; xxxx1xxx - Secondary Air Injection (AIR) System
; xxxxx1xx - Activated Charcoal System
; xxxxxx1x - Catalytic Converter Heater
; xxxxxxx1 - Catalytic Converter
100,2,Coolant,Temperature (G62),Specification: 80.0...110.0 °C
100,3,Time since,Engine Start
100,4,OBD-Status
; 1xxx--xx - MIL Warning Lamp ON
; x1xx--xx - Driving Cycle detected
; xx1x--xx - Trip complete
; xxx1--xx - Malfunction detected (1+)
; xxxx--1x - Heating cycle ended
; xxxx--x1 - Heating cycle not possible
;
101,0,Fuel Injection
101,1,Engine Speed,(G28),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
101,2,Engine Load,,Specification (Idle): 15.0...25.0 %\nRange: 15.0...175.0 %
101,3,Injection Timing,,Specification (Idle): 2.0...4.0 ms
101,4,Mass Air Flow,(G70),Specification (Load): min. 180.0 g/s
;
102,0,Fuel Injection
102,1,Engine Speed,(G28),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
102,2,Coolant,Temperature (G62),Specification: 80.0...110.0 °C
102,3,Intake Air,Temperature (G42)
102,4,Injection Timing,,Specification (Idle): 2.0...4.0 ms
;
104,0,Start Adaption Values
104,1,Start Engine,Temperature
104,2,Temperature,Adaptation Factor 1
104,3,Temperature,Adaptation Factor 2
104,4,Temperature,Adaptation Factor 3
;
107,0,Lambda Control
107,1,Engine Speed,(G28),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
107,2,Lambda Control,Bank 1 (Average),Range: -25.0...+25.0 %\nSpecification: -18.0...+12.0 %
107,3,Lambda Control,Bank 2 (Average),Range: -25.0...+25.0 %\nSpecification: -18.0...+12.0 %
107,4,Result,Lambda Control,Display Range: Test ON/Test OFF/Syst. OK/Syst. n.OK\nSpecification: Syst. OK
;
110,0,Load/Full Throttle Enrichment
110,1,Engine Speed,(G28),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
110,2,Coolant,Temperature (G62),Specification: 80.0...110.0 °C
110,3,Injection Timing,,Specification (Idle): 2.0...4.0 ms
110,4,Throttle Valve Angle
;
111,0,Boost Pressure Control
111,1,RPM Range 1
111,2,RPM Range 2
111,3,RPM Range 3
111,4,RPM Range 4
;
112,0,Exhaust Gas Temperature
112,1,Exhaust Gas,Temperature Bank 1,Range: 945.0...1100.0 °C\nSpecification: ~980.0 °C (max. 1025 °C)
112,2,Enrichment Factor,Bank 1,Range: 0.0...100.0 %\nSpecification: 15.0...25.0 %\n\n> 30.0 % indicates Low Fuel Pressure or a bad Mass Air Flow Sensor (MAF/G70)
112,3,Exhaust Gas,Temperature Bank 2,Range: 945.0...1100.0 °C\nSpecification: ~980.0 °C (max. 1025 °C)
112,4,Enrichment Factor,Bank 2,Range: 0.0...100.0 %\nSpecification: 15.0...25.0 %\n\n> 30.0 % indicates Low Fuel Pressure or a bad Mass Air Flow Sensor (MAF/G70)
;
113,0,Load/Full Throttle Enrichment
113,1,Engine Speed,(G28),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
113,2,Engine Load,,Specification (Idle): 15.0...25.0 %\nRange: 15.0...175.0 %
113,3,Throttle Valve Angle
113,4,Athmospheric,Pressure
;
114,0,Boost Pressure Control
114,1,Engine Load,(specified),Tolerance (to Field 2 & 3): max. ±5.0 %
114,2,Engine Load,(spec. corrected),Tolerance (to Field 1 & 3): max. ±5.0 %
114,3,Engine Load,(actual),Tolerance (to Field 1 & 2): max. ±5.0 %
114,4,Wastegate (N75),Duty Cycle
;
115,0,Boost Pressure Control
115,1,Engine Speed,(G28),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
115,2,Engine Load,,Specification (Idle): 15.0...25.0 %\nRange: 15.0...175.0 %
115,3,Boost Pressure,(specified)
115,4,Boost Pressure,(actual),Tolerance (to Spec.): max. ±20 mbar
;
116,0,Boost Pressure Control
116,1,Engine Speed,(G28),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
116,2,Fuel Temp.,Correction Factor,Specification: min. 0.0 %
116,3,Coolant Temp.,Correction Factor,Specification: min. 0.0 %
116,4,Intake Air Temp.,Correction Factor,Specification: min. 0.0 %
;
117,0,Boost Pressure Control
117,1,Engine Speed,(G28),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
117,2,Accel. Pedal Pos.,Sensor 1 (G79),Specification: 12.0...97.0 %
117,3,Throttle Valve Angle
117,4,Boost Pressure,(specified)
;
118,0,Boost Pressure Control
118,1,Engine Speed,(G28),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
118,2,Intake Air,Temperature (G42)
118,3,Wastegate (N75),Duty Cycle
118,4,Boost Pressure,(actual)
;
119,0,Boost Pressure Control
119,1,Engine Speed,(G28),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
119,2,Charge Limit
119,3,Wastegate (N75),Duty Cycle
119,4,Boost Pressure,(actual)
;
120,0,Traction Control (ASR)
120,1,Engine Speed,(G28),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
120,2,Torque specified,by ASR
120,3,Engine Torque,(actual)
120,4,Status,,Specification: ASR OFF/ASR ON
;
122,0,Transmission
122,1,Engine Speed,(G28),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
122,2,Torque specified,by Transmission
122,3,Engine Torque,(actual)
122,4,Status,,Display Range: No Torq Red/Torq. Reduc.
;
125,0,CAN-Databus Communication (Powertrain)
125,1,Transmission
125,2,Brake Electronics,(J104),Range: ABS 1/ABS 0\nSpecification: ABS 1
125,3,Instrument Cluster,(J285),Range: Instruments 1/Instruments 0\nSpecification: Instruments 1
;
220,0,Exhaust Gas Temerature (EGT) Regulation (Bank 1)
220,1,Engine Speed,(G28),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
220,2,Engine Load,,Specification (Idle): 15.0...25.0 %\nRange: 15.0...175.0 %
220,3,Exhaust Gas Temp.,Sensor B1 (G235),Range: 0.0...100.0 %\nSpecification: 32.0...52.0 %
220,4,Operating Status,Bank 1 (EGTR),Range: ON/OFF\nSpecification: ON
;
221,0,Exhaust Gas Temerature (EGT) Regulation (Bank 2)
221,1,Engine Speed,(G28),Specification (Idle): 650...750 RPM\nSpecification (Load): 1900...2200 RPM\nRange: 0...6800 RPM
221,2,Engine Load,,Specification (Idle): 15.0...25.0 %\nRange: 15.0...175.0 %
221,3,Exhaust Gas Temp.,Sensor B2 (G236),Range: 0.0...100.0 %\nSpecification: 32.0...52.0 %
221,4,Operating Status,Bank 2 (EGTR),Range: ON/OFF\nSpecification: ON
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Engine Control Module (J220) Coding
C01,??xxx: Emissions
C02,05 = Euro II/D3 / 06 = TLEV (USA) / 07 = LEV (USA)
C03,08 = GUS/China / 10 = Euro III / 11 = Euro IV/Japan
C04,25 = South Africa / 26 = Mexico/Taiwan / 27 = Brasil
C05,xx?xx: Powertrain
C06,5 = Front-Wheel-Drive
C07,6 = All-Wheel-Drive without ASR/ESP (with CAN-Bus)
C08,7 = All-Wheel-Drive with ASR/ESP (with CAN-Bus)
C09,8 = All-Wheel-Drive with Post-Switch Stage (Low Range - A6 Allroad only)
C10,xxx?x: Transmission
C11,1 = 6-Speed Manual Transmission
C12,5 = 5-Speed Automatic Transmission (01V/5HP19)
C13,xxxx?: Vehicle
C14,1 = Audi A4 (8D)
C15,2 = Audi A6 (4B) & Audi A6 allroad (4BH / only Engine Code APB)
C16,5 = Audi A6 allroad (4BH / excl. Engine Code APB)
;
;
;---------------------------------------------------
;
; login
;
;---------------------------------------------------
;
;
L00,Engine Control Module (J220) Login
L01,11463 = Cruise Control System (CCS) Activation
L02,16167 = Cruise Control System (CCS) Deactivation
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A000,0,Reset Learned Values
A000,5,Reset Learned Values
A000,6,To Reset the learned Values Save this Adaptation Channel.
;
A001,0,Idle Speed Adjustment
A001,1,Engine Speed,(actual)
A001,2,Engine Speed,(specified)
A001,3,A/C Readiness,,Range: A/C-Low / A/C-High
A001,4,A/C Compressor,,Range: Compr.OFF/Compr.ON
;
A050,0,Immobilizer (Vehicle Data learning)
A050,1,Status
A050,5,Immobilizer (Vehicle Data learning)
A050,6,Please enter the Immobilizer PIN/SKC of the Instrument Cluster (OLD PIN/SKC).
A050,7,After that the Learning Process is being initiated the new Engine Control
A050,8,Module adopts the Vehicle-Identification-Number (VIN) and Immobilizer
A050,9,Identification (IMMO-ID) of the Vehicle (from the OLD Instrument Cluster).
A050,10,Once the Adaptation is done switch the Ignition OFF for about 2 Minutes.
;
A091,0,Immobilizer Status
A091,5,Immobilizer Status (Read Only)
A091,6,0 = Immobilizer not matched (NEW)
A091,7,1 = Immobilizer disabled
A091,8,4 = Immobilizer matched (System OK)
;
;
;---------------------------------------------------
;
; readiness
;
;---------------------------------------------------
;
;
O,078-907-551-AZA
;
