;
; VCDS Label File
;
; Audi A4 (8D) / Audi A6 (4B)
;
; Component: Engine (#01) - ACK/ALG/APR
;
; P/N: 4D0-907-551-???
;
; includes coding and adaptation
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 4D-01.LBL
; 078-907-551-ACK.LBL  (2.8l E   @ 193 HP - ACK/ALG/APR)
;
; created on 26/Mar/2008 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification: 26/Mar/2008
;
; requires VCDS 803.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks & basic setting
;
;---------------------------------------------------
;
;

;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Engine (J220) Coding
C01,??xxx: Emissions
C02,02 = MVEG I (non-EU Members)
C03,04 = MVEG II (EU Members)
C04,05 = MVEG III (with Sec. Air Injection)
C05,08 = China and Russia/GUS
C06,xx?xx: Powertrain
C07,0 = Front-Wheel-Drive without ASR
C08,1 = Front-Wheel-Drive with ASR
C09,2 = All-Wheel-Drive without ASR
C10,3 = All-Wheel-Drive with ASR
C11,xxx?x: Transmission
C12,0 = 5-Speed Manual Transmission
C13,5 = 5-Speed Automatic Transmission (01V)
C14,xxxx?: Model
C15,1 = Audi A4 (8D)
C16,2 = Audi A6 (4B)
C17,3 = Audi A8 (4D)
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A001,0,Idle Speed
A001,1,Engine Speed,(actual)
A001,2,Engine Speed,(specified)
A001,3,A/C Readiness,,Range: A/C-Low / A/C-High
A001,4,A/C Compressor,,Range: Compr.OFF/Compr.ON
; 
A091,0,Immobilizer Status
A091,5,Immobilizer Status (Read Only)
A091,6,0 = Immobilizer not matched (NEW)
A091,7,1 = Immobilizer disabled
A091,8,4 = Immobilizer matched (System OK)
;
