;
; VCDS Label File
;
; Copyright © 2006+ Ross-Tech, LLC
;
; Audi Q7 (4L)
;
; Component: J773 - Comfort System II (#6F)
;
; P/N: 4L0-910-290-???
;
; includes measuring blocks, coding and selective output test
;
; created on 29/May/2006 by Sebastian Stange (Sebastian@Ross-Tech.com)
; updated on 29/May/2015 by Sebastian Stange (Sebastian@Ross-Tech.com) // Converted Coding added
;
; last modification on 29/May/2015
;
; requires VCDS 14.10.2 / LCode 1.0.5.6 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,General
001,1,Voltage,(Terminal 30)
001,3,Rear Lid,Detection 1,Range: 0...153
001,4,Rear Lid,Detection 2,Range: 0...153
;
002,0,Rear Left Lights
002,1,Rear Left,Fog Light,Range: 0.0...100.0 %
002,2,Rear Left,Back-Up Light,Range: 0.0...100.0 %
002,3,Rear Left,Side Marker Light,Range: 0.0...100.0 %
;
003,0,Rear Right Lights
003,1,Rear Right,Fog Light,Range: 0.0...100.0 %
003,2,Rear Right,Back-Up Light,Range: 0.0...100.0 %
003,3,Rear Right,Side Marker Light,Range: 0.0...100.0 %
;
004,0,Luggage Compartment Illumination
004,1,Luggage Comp.,Illumination (High),Range: 0.0...100.0 %
004,2,Luggage Comp.,Illumination (Low),Range: 0.0...100.0 %
;
005,0,Front Sunroof
005,1,Front Sunroof,Position,Range: 0.0...100.0 %
005,2,Front Sunroof,Status,Range: Open/Closed
005,3,Front Sunroof,Reversing,Range: ON/OFF
005,4,Front Sunroof,Front Switch,See Label File
; ????-xxx = Pre-Selection
; xxxx-?xx = Malfunction
; xxxx-x?x = Pull
; xxxx-xx? = Pressure
;
006,0,Rear Sunroof
006,1,Rear Sunroof,Position,Range: 0.0...100.0 %
006,2,Rear Sunroof,Reversing,Range: ON/OFF
006,3,Rear Sunroof,Front Switch,1xx = Malfunction\nx1x = Close\nxx1 = Open
006,4,Rear Sunroof,Rear Switch,1xx = Malfunction\nx1x = Close\nxx1 = Open
;
007,0,Roof Blinds
007,1,Roof Blinds,Position,Range: 0.0...100.0 %
007,2,Roof Blinds,Reversing,Range: ON/OFF
007,3,Roof Blinds,Front Switch,1xx = Malfunction\nx1x = Close\nxx1 = Open
007,4,Roof Blinds,Rear Switch,1xx = Malfunction\nx1x = Close\nxx1 = Open
;
008,1,LIN Status
; ?xxxx = Child Safety Lock
; x?xxx = Sunroof Enabling
; xx?xx = Communication to Roof Blinds
; xxx?x = Communication to Rear Sunroof
; xxxx? = Communication to Front Sunroof
008,2,LIN Signals
; 00111111,Bin. Bits,
; ?xxxxxxx = Comfort Closing
; x?xxxxxx = Comfort Opening
; xx?xxxxx = Roof Blinds learning run successful
; xxx?xxxx = Sunroof standardized
; xxxx?xxx = Rear Sunroof learning run successful
; xxxxx?xx = Rear Sunroof standardized
; xxxxxx?x = Front Sunroof learning run successful
; xxxxxxx? = Front Sunroof standardized
008,3,Vehicle Speed
008,4,Outside,Temperature
;
009,3,Rear Lid,Detection 1,Range: 0.00...6.50 V
009,4,Rear Lid,Detection 2,Range: 0.00...6.50 V
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Comfort System II (J773) Coding
C01,+0000001 = Electric Windows installed
; Coding Indicator Bit
C02,+0000002 = Open Sky System installed (PR-3FU)
C03,+0000004 = 3rd Seat Row NOT installed (PR-5KM/5KY)
C04,+0000008 = North American Region (PR-A8U)
C05,+0000256 = Comfort Opening Front Sunroof
C06,+0000512 = Comfort Opening Rear Sunroof
C07,+0001024 = Comfort Opening Roof Blinds
C08,+0002048 = Comfort Closing Roof Blinds
C09, 
C10,Note #1: Coding Value is the Sum of the individual Options!
C11,Note #2: You can also use the Coding Assist/Helper!
;
;
;---------------------------------------------------
;
; converted coding
; (short coding displayed as long coding for easier modifications)
;
;---------------------------------------------------
;
;
LC,02,0,Electric Windows installed
; Coding Indicator Bit
LC,02,1,Open Sky System installed (PR-3FU)
LC,02,2,3rd Seat Row NOT installed (PR-5KM/5KY)
LC,02,3,North American Region (PR-A8U)
LC,02,7=,Additional Coding Details can be found in Byte 01!
LC,01,0,Comfort Opening Front Sunroof
LC,01,1,Comfort Opening Rear Sunroof
LC,01,2,Comfort Opening Roof Blinds
LC,01,3,Comfort Closing Roof Blinds
LC,01,7=,Additional Coding Details can be found in Byte 02!
LC,00,7=,Coding Details can be found in Byte 01 && Byte 02!
;
;
;---------------------------------------------------
;
; selective output test
;
;---------------------------------------------------
;
;
T1502,Fog Light Rear Left (L46)
T1506,Fog Light Rear Right (L47)
T1518,Back-Up Light Left (M16)
T1519,Back-Up Light Right (M17)
T2911,Side Marker Light Rear Left (M37)
T2912,Side Marker Light Rear Right (M38)
T2913,Trunk and Interior Lights
T2919,Front Sunroof: Open/Raise
T2920,Front Sunroof: Close/Lower
T2921,Rear Sunroof: Open/Raise
T2922,Rear Sunroof: Close/Lower
T2923,Roof Blinds: Open
T2924,Roof Blinds: Close
T2960,Bumper Light Rear Left
T2961,Bumper Light Rear Right
T2995,Decalibration Front Sunroof
T2996,Decalibration Rear Sunroof
T2997,Decalibration Roof Blinds
;
