;
; VCDS Label File
;
; Copyright © 2015+ Ross-Tech, LLC
;
; Skoda Fabia/Roomster (5J) / VW Polo (9N)
;
; Component: J255 - A/C Heating Electronics (#08) - Climatronic
;
; P/N:  ??0-907-044-???
;
; includes measuring blocks and basic setting
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 5J-08.LBL
; 6Q0-907-044.LBL
;
; created on 27/Jan/2015 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 27/Jan/2015
;
; requires VCDS 14.10.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks & basic setting
;
;---------------------------------------------------
;
;
001,1,Compressor,Shut-Off Code,Specification: 0/6/7\n\n0 = Compr. ON\n1 = Comp. OFF: Refrigerant Pressure too high (> 32 bar)\n2 = Compr. OFF: Blower Faulty (Voltage < 3 V)\n3 = Compr. OFF: Refrigerant Pressure too low (< 2 bar)\n6 = Compr. OFF: ECON Mode active\n7 = Compr. OFF: A/C System OFF\n8 = Compr. OFF: Outside Temperature too low (< 3.0 °C)\n9 = Compr. OFF: Blower OFF\n10 = Compr. OFF: Vehicle System Voltage too low (< 10.1 V)\n11 = Compr. OFF: Engine Temperature too high (> 118 °C)\n13 = Compr. OFF: Vehicle System Voltage too high (> 17 V)\n14 = Compr. OFF: Evaporator Temperature too low\n16 = Compr. OFF: Compressor Activation faulty\n17 = Compr. OFF: No or implausible Signal Pressure Sensor\n18 = Compr. OFF: Vehicle Speed Shut-Off
; 0 = Compr. ON
; 1 = Comp. OFF: Refrigerant Pressure too high (> 32 bar)
; 2 = Compr. OFF: Blower Faulty (Voltage < 3 V)
; 3 = Compr. OFF: Refrigerant Pressure too low (< 2 bar)
; 6 = Compr. OFF: ECON Mode active
; 7 = Compr. OFF: A/C System OFF
; 8 = Compr. OFF: Outside Temperature too low (< 3.0 °C)
; 9 = Compr. OFF: Blower OFF
; 10 = Compr. OFF: Vehicle System Voltage too low (< 10.1 V)
; 11 = Compr. OFF: Engine Temperature too high (> 118 °C)
; 13 = Compr. OFF: Vehicle System Voltage too high (> 17 V)
; 14 = Compr. OFF: Evaporator Temperature too low
; 16 = Compr. OFF: Compressor Activation faulty
; 17 = Compr. OFF: No or implausible Signal Pressure Sensor
; 18 = Compr. OFF: Vehicle Speed Shut-Off
001,2,Engine Speed,,Range: 0...10000 RPM
001,3,Vehicle Speed,,Range: 0...255 km/h
001,4,Standing Time
;
B001,0,Flap Motors: Stop Position learning
B001,1, , , 
B001,2, , , 
B001,3, , , 
B001,4, , , 
;
002,0,Motor for Temperature Regulator Flap (V68)
002,1,Potentiom. (G92),(actual),Range: 0...255
002,2,Potentiom. (G92),(specified),Range: 0...255
002,3,Stop/Learned,(Cooling),Range: 0...255\nSpecification (saved after Basic Setting): 200...250
002,4,Stop/Learned,(Heating),Range: 0...255\nSpecification (saved after Basic Setting): 5...50
;
003,0,Center Flap Control Motor (V70) / Potentiometer (G112)
003,1,Potentiom. (G112),(actual),Range: 0...255
003,2,Potentiom. (G112),(specified),Range: 0...255
003,3,Stop/Learned,(Impact Vent),Range: 0...255\nSpecification (saved after Basic Setting): 200...250
003,4,Stop/Learned,(Stop/Footwell),Range: 0...255\nSpecification (saved after Basic Setting): 5...50
;
004,0,Defroster Flap Control Motor (V107) / Potentiometer (G135)
004,1,Potentiom. (G135),(actual),Range: 0...255
004,2,Potentiom. (G135),(specified),Range: 0...255
004,3,Stop/Learned,(Open),Range: 0...255\nSpecification (saved after Basic Setting): 200...250
004,4,Stop/Learned,(Closed),Range: 0...255\nSpecification (saved after Basic Setting): 5...50
;
005,0,Air Flow Flap Control Motor (V71) / Potentiometer (G113)
005,1,Potentiom. (G113),(actual),Range: 0...255
005,2,Potentiom. (G113),(specified),Range: 0...255
005,3,Stop/Learned,(Max. Airflow),Range: 0...255\nSpecification (saved after Basic Setting): 200...250
005,4,Stop/Learned,(Recirculation),Range: 0...255\nSpecification (saved after Basic Setting): 5...50
;
006,1,Outside Air,Temp. (filtered)
006,3,Outside Air,Temp. (unfiltered)
006,4,Sunlight,Intensity (G107),Range: 0.0...100.0 %
;
007,0,Interior Temperatures
007,1,Temperature at,Center Outl. (G191)
007,2,Temperature at,Floor Outlet (G192)
007,3,Temperature at,A/C Panel (G56)
007,4,Temperature at,Evaporator (G263)
;
008,0,Fresh Air Blower (V2)
008,1,Fresh Air (V2),Blower (spec.),Range: 0.0...20.0 V
008,2,Fresh Air (V2),Blower (act.),Range: 0.0...20.0 V
008,3,Voltage,(Terminal 15),Range: 0.0...20.0 V\nSpecification: 10.5...14.0 V
008,4,Fresh Air Blower,(V2) Load,Range: 0.0...100.0 %
;
009,0,Map Cooling
009,1,Map Cooling,Relay/Valve,Range: ON/OFF
009,2,Map Cooling,(Engine),Range: ON/OFF
009,3,Fresh Air Blower,(V2) Stage 1,Range: ON/OFF
009,4,Fresh Air Blower,(V2) Stage 2,Range: ON/OFF
;
010,0,Fresh Air Blower (V2) && Aux. Heater
010,1,Aux. Heater,Request,Range: ON/OFF
010,2,Aux. Heater,Status,Range: ON/OFF
010,3,Wiper Motor,Status,Range: ON/OFF
010,4,Coolant,Temperature (G62)
;
011,1,Dimming,(Terminal 58d),Range: 0.0...100.0 %
011,2,Idle Speed,Increase,Range: ON/OFF
011,4,Refrigerant,Pressure (G65),Specification: 2.0...32.0 bar 
;
012,0,Compressor
012,3,Compressor Speed
012,4,Compressor Load,,Range: 0.0...22.0 Nm
;
080,0,Advanced Control Module Identification I
080,1,Identification
080,2,Revision
080,3,Production,Date
080,4,Manufacturer &,Test Stand Number
;
