;
; VAG-COM label file
;
; VW EuroVan (7D)
;
; component: engine (#01) - AXK
;
; ECU p/n: 022 906 032 F
;
; includes measuring blocks & coding
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 02-01.LBL
; 022-906-032-AXK.LBL (2.8l E   @ 204 HP - AXK)
;
; modified by Sebastian Stange
; sebastian@ross-tech.com
;
; last modification: 03/21/2005
;
; ready for VAG-COM 405.0 and above
;
;
;---------------------------------------------------
;
; coding informations
;
;---------------------------------------------------
;
;
C00,Eurovan (7D) - ECU Coding
C01,XXX?X - ESP (1 = with ESP / 0 = without ESP)
C02,XXXX? - Transmission (3 = automatic transmission)
;
;
;---------------------------------------------------
;
; readiness
;
;---------------------------------------------------
;
;
;700.8: readiness steps, pointing to AXK-new.clb
O,022-906-032-AXK
;
;
;---------------------------------------------------
;
; measuring block informations
;
;---------------------------------------------------
;
1,0,Basic functions (at idle)
1,1,Engine RPM,(idle),Specified value: 650 - 750 RPM
1,2,Coolant,temperature,Specified value: 80 - 110 C
1,3,O2 sensor,before cat.,Specified value: -10.0 to 10.0 %
1,4,Adjustment,requirements,see label
;X0000000 No malfunctions seen by OBD
;0X000000 no meaning/not used
;00X00000 A/C compressor switched off
;000X0000 Idle switch closed
;0000X000 O2 sensor regulation OK
;00000X00 Throttle valve closed
;000000X0 RPMs below 2000
;0000000X Coolant temp above 80 C
;
2,0,Mass Air Flow (MAF) sensor
2,1,Engine RPM,(idle),Specified value: 650 - 750
2,2,Engine load,,Specified value: 12 - 26 %
2,3,Injection,timing,Specified value: 1.0 - 4.0 ms
2,4,Mass air,taken in,Specified value: 3.0 - 5.0 g/s
;
3,0,Mass Air Flow (MAF) sensor
3,1,Engine RPM,(idle),Specified value: 650 - 750
3,2,Mass air,taken in,Specified value: 3.0 - 5.0 g/s
3,3,Throttle valve,angle,Specified value: 0.2 - 4.0 %
3,4,Ignition,angle,Specified value: 9 - 15 deg BTDC
;
4,0,Basic functions (at idle)
4,1,Engine RPM,(idle),Specified value: 650 - 750
4,2,Voltage,to ECU,Specified value: 12.0 - 15.0 V
4,3,Coolant,temperature,Specified value: 80 - 110 C
4,4,Intake air,temperature,Specified value: -48 - 143 C
;
5,0,Basic functions (at idle)
5,1,Engine RPM,(idle),Specified value: 650 - 750
5,2,Engine load,,Specified value: 12 - 26 %
5,3,Speed,,Specified value: 0 km/h
5,4,Operating,condition (idle)
;
6,0,Basic functions (at idle)
6,1,Engine RPM,(idle),Specified value: 650 - 750
6,2,Engine load,,Specified value: 12 - 26%
6,3,Intake air,temperature,Specified value: -48 - 143 C
6,4,High correction,factor,Specified value: -50 - 10 %
;
7,0,Undocumented
;
8,0,Undocumented
;
9,0,Undocumented
;
10,0,Ignition
10,1,Engine speed,(idle),Specified value: 650 - 750
10,2,Engine load,,Specified value: 12 - 26 %
10,3,Throttle valve,angle,Specified value: 0.2 - 4.0 %
10,4,Ignition,angle,Specified value: 9 - 15 deg BTDC
;
11,0,Undocumented
;
12,0,Undocumented
;
13,0,Undocumented
;
14,0,Ignition - misfire recognition
14,1,Engine speed,(idle),Specified value: 650 - 750
14,2,Engine,load,Specified value: 15 - 25%
14,3,Number of,misfires,Specified value: 0
14,4,Misfire,recognition,Specified value: activated
;
15,0,Undocumented
;
16,0,Undocumented
;
17,0,Undocumented
;
18,0,Undocumented
;
19,0,Undocumented
;
20,0,Undocumented
;
21,0,Undocumented
;
22,0,Ignition - knock control (cyl. 1-2)
22,1,Engine speed,,Specified value: 630 - 6800
22,2,Engine load,,Specified value: 10 - 100 %
22,3,angle retard.,#1 via knock contr.,Specified value: 0 - 12.0 KW
22,4,angle retard.,#2 via knock contr.,Specified value: 0 - 12.0 KW
;
23,0,Ignition - knock control (cyl. 3-4)
23,1,Engine speed,,Specified value: 630 - 6800
23,2,Engine load,,Specified value: 10 - 100 %
23,3,angle retard.,#3 via knock contr.,Specified value: 0 - 12.0 KW
23,4,angle retard.,#4 via knock contr.,Specified value: 0 - 12.0 KW
;
24,0,Ignition - knock control (cyl. 5-6)
24,1,Engine speed,,Specified value: 630 - 6800
24,2,Engine load,,Specified value: 10 - 100 %
24,3,angle retard.,#5 via knock contr.,Specified value: 0 - 12.0 KW
24,4,angle retard.,#6 via knock contr.,Specified value: 0 - 12.0 KW
;
25,0,Undocumented
;
26,0,Undocumented
;
27,0,Undocumented
;
28,0,Ignition - knock control
28,1,Engine speed,,Specified value: 2200 - 6800
28,2,Engine load,,Specified value: 10 - 100 %
28,3,Coolant,temperature,Specified value: 40 - 110 C
28,4,Knock sensor,test,Specified value: Sys OK (Test on/Test off/Sys. OK/Sys. not OK)
;
29,0,Undocumented
;
30,0,Status O2 control
30,1,O2 status,sensor 1/bank 1,Specified value: 111 (before cat) > see label
30,2,O2 status,sensor 2/bank 1,Specified value: 111 (behind cat) > see label
;X11 Oxygen sensor heating on
;1X1 Oxygen sensor operationally ready
;11X Oxygen sensor control active
;
31,0,Undocumented
;
32,0,O2 sensor control - adaptation values
32,1,Sensor 1,Bank 1 (idle),Specified value:-5.4 - 5.4 % (add.)
32,2,Sensor ,Bank 1 (part throttle),Specified value: -10 - 10 % (mult.)
;
33,0,O2 sensor control - control values
33,1,O2 control,Bank 1,Specified value: -10 - 10 %
33,2,Sensor 1,Bank 1,Specified value: 1.400 - 1.600 V
;
34,0,O2 control - precat aging test
34,1,Engine speed,,Specified value: 2000 - 2300 RPM
34,2,Cat.,temperature,Specified value: >350 C
34,3,Dynamic,factor,Specified value: 0 - 2
34,4,Results,,Specified value: B1-S1 OK (Test OFF/Test ON/B1-S1 OK/ B1-S1 not OK)
;
35,0,Undocumented
;
36,0,O2 control behind cat. (idle) - basic setting (04)
36,1,O2,sensor,Specified value: 0.100 - 0.900 V
36,2,Results,,Specified value: B1-S2 OK (Test OFF/Test ON/B1-S2 OK/ B1-S2 not OK)
;
37,0,Undocumented
;
38,0,Undocumented
;
39,0,Undocumented
;
40,0,Undocumented
;
41,0,O2 heating - bank 1
41,2,sensor 1,bank 1,Specified value: Htg before cat. ON/Htg before cat. OFF/varies periodically
41,3,Res O2,before cat,Specified value: 0 - 25 kOhms
41,4,sensor 2,bank 1,Specified value: Htg after cat. ON/Htg after cat. OFF/varies periodically
;
42,0,Undocumented
;
43,0,O2 control behind cat. (aging) - basic setting (04)
43,1,Engine,speed,Specified value: 2000 - 2300 RPM
43,2,Cat.,temperature,Specified value: >350 C
43,3,O2 Sensor 2,Bank 1,Specified value: 0.00 - 1.00 V
43,4,Results,,Specified value: B1-S2 OK (Test OFF/Test ON/B1-S2 OK/ B1-S2 not OK)
;
44,0,Undocumented
;
45,0,Undocumented
;
46,0,O2 sensor control - cat. conv. test - basic setting (04)
46,1,Engine,speed,Specified value: 2000 - 2300
46,2,Cat.,temperature,Specified value: > 350 C
46,3,Cat.,conversion rate,Specified value: 0.0 - 100.0 %
46,4,Cat.,test,Specified value: Cat B1 OK (Test OFF/Test ON/Cat B1 OK/Cat B1 not OK)
;
47,0,Undocumented
;
48,0,Undocumented
;
49,0,Undocumented
;
50,0,RPM regulation - operating conditions
50,1,Engine,speed (idle),Specified value: 650 - 750
50,2,Engine speed,(specified),Specified value: 700 RPM
50,3,A/C,system,Specified value: A/C-high or A/C-low
50,4,A/C,compressor,Specified value: Compr. ON or Compr. OFF
;
51,0,Undocumented
;
52,0,Undocumented
;
53,0,Undocumented
;
54,0,RPM regulation
54,1,Engine,speed,Specified value: 650 - 750
54,2,Operation,condition,Values: idle/partial throttle/enrichment/deceleration
54,3,Throttle,Postion,Specified value: 0 - 97 %
54,4,Throttle,angle,Specified value: 0 - 100 %
;
55,0,RPM regulation - idle stabilization
55,1,Engine,(idle),Specified value: 650 - 750
55,2,Idle,control,Specified value: -5.0 - 10.0 %
55,3,Idle,control,Specified value: -5.0 - 5.0 %
55,4,Operation,condition,see label
;X0000 Pressure switch for power steering on (not indicated for 4 digit number block)
;0X000 Atomic batteries to speed or "no meaning"
;00X00 A/C system switched on
;000X0 Driving mode selected
;0000X A/C compressor switched on
;
56,0,RPM regulation - idle stabillzation
56,1,Engine,speed,Specified value: 650 - 750
56,2,Engine,speed,Specified value: 700 RPM
56,3,Idle,control,Specified value: -5.0 to 10.0 %
56,4,Operating,condition,see label
;X0000 Pressure switch for power steering on (not indicated for 4 digit number block)
;0X000 Atomic batteries to speed or "no meaning"
;00X00 A/C system switched on
;000X0 Driving mode selected
;0000X A/C compressor switched on
;
;
57,0,Undocumented
;
58,0,Undocumented
;
59,0,Undocumented
;
60,0,RPM regulation - adaptation EPC system
60,1,Throttle,Position (G187),Specified value: 3 - 93 %
60,2,Throttle,Position (G188),Specified value: 97 - 3 %
60,3,Adaption,step counter,Specified value: 0 - 8
60,4,Adaptation,test,Specified value: ADP OK (ADP in progress/ADP OK/ADP error)
;
61,0,RPM regulation - EPC system
61,1,Engine,speed,Specified value: 650 - 6500
61,2,Volt supply,to ECU,Specified value:12.0 - 15.0 V
61,3,Throttle,Position (G187),Specified value: 0 - 100 %
61,4,Operating,conditions,see label
;X0000 Pressure switch for power steering on (not indicated for 4 digit number block)
;0X000 Atomic batteries to speed or "no meaning"
;00X00 A/C system switched on
;000X0 Driving mode selected
;0000X A/C compressor switched on
;
62,0,RPM regulation - EPC system
62,1,Throttle,Position (G187),Specified value: 3 - 93 %
62,2,Throttle,Position (G188),Specified value: 97 - 3 %
62,3,Throttle,Position (G79),Specified value: 12 - 97 %
62,4,Throttle,Position (G185),Specified value: 4 - 49 %
;
63,0,RPM regulation - kick-dowm adaptation
63,1,Throttle,Position,Specified value: 70 - 97 %
63,2,Throttle,Poition (G185),Specified value: 80 - 100 %
63,3,Kick down,switch,Specified value: Kick down
63,4,Operating,test,Specified value: ADP OK (ERROR/operate/ADP in progress/ADP OK)
;
64,0,Undocumented
;
65,0,Undocumented
;
66,0,Cruise control system (idle)
66,1,Vehicle,speed,Specified value: O km/h
66,2,Brake,switch,see label
;X000 Cruise control switched free
;0X00 Always 0 for vehicles with automatic transmission
;00X0 Brake operated (brake pedal switch)
;000X Brake operated (brake light switch)
66,3,Speed stored, by cruise control
66,4,Cruise,switch,see label
;X000 Sliding cruise control switch on RES
;0X00 SET button pressed
;00X0 Sliding cruise control switch at OFF (not engaged or engaged)
;000X Sliding cruise control switch at OFF (only when engaged)
;
81,0,VIN & Immo ID (if Immo-3)
;
82,0,Flashing Informations
;
90,0,Power enhancements - exhaust camshaft
90,1,Engine,speed,Specified value: 650 - 6500
90,2,Operating,conditions,Specified value: on/off (camshaft adjustment)
90,3,Camshaft,adjustment,Specified value: 0 - 25 deg (actual crankshaft)
;
91,0,Power enhancement - intake camshaft
91,1,Engine,speed,Specified value: 650 - 6500
91,2,Duty,cycle,Specified value: 0 - 100 %
91,3,Specified angle,intake cam adj.,Specified value: 0 - 52 deg
91,4,Current angle,intake cam adj.,Specified value: 0 - 52 deg
;
92,0,Undocumented
;
93,0,Undocumented
;
94,0,Undocumented
;
95,0,Power enhancements - intake change over
95,1,Engine,speed,Specified value: 650 - 6500
95,2,Engine,load,Specified value: 0 - 120 %
95,3,Coolant,temperature,Specified value: 80 - 110 C
95,4,Status of,intake manifold,Specified value: IM-CO ON/IM-CO OFF
;
96,0,Undocumented
;
97,0,Undocumented
;
98,0,Undocumented
;
99,0,O2 sensor control - basic settings (04)
99,1,Engine,speed (idle),Specified value: 650 - 750
99,2,Coolant,temperature,Specified value: 80 - 110 C
99,3,O2 sensor,control,Specified value:-10.0 - 10.0%
99,4,Op condition,O2 control,Specified value: O2-Reg.ON/ O2-Reg.OFF
;
125,0,CAN-BUS Status (1 = OK / 0 = not OK)
125,1,Transmission
125,2,ABS
125,3,Instrument,cluster
;
134,0,Undocumented
;
137,0,Undocumented
;
