;
; VCDS Label File
;
; Copyright © 2006+ Ross-Tech, LLC
;
; Audi A3 (8P) / Audi A4 (8EC/8ED) / Audi A6 (4F) / Audi A8 (4E)
; Audi Q7 (4L) / Audi TT (8J) / VW Scirocco (13)
;
; Component: J431 - Headlight Range (#55)
;
; P/N: 8P0-907-357-??? / 8P3-907-357-???
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 8P-55.LBL
; 8P0-907-357.LBL
;
; includes measuring blocks, basic setting, adaptation, coding and selective output tests
;
; created on 30/May/2006 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 18/Apr/2012
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks & basic setting
;
;---------------------------------------------------
;
;
001,1,Voltage,(Terminal 15),Specification: min. 10.5 V
001,2,Light,(Terminal 56b),Specification: ON/OFF
001,3,Vehicle Speed
001,4,Acceleration
;
B001,0,Adjustment Position && Adjustment Learning
B001,1,Adjustment,Status, 
B001,2, , , 
B001,3, , , 
B001,4, , , 
;
002,1,Front Sensor (G78),(actual),Specification: 12.5...50.0 %
002,2,Rear Sensor (G76),(actual),Specification: 50.0...87.5 %
002,3,Actuator Motor,Activation
002,4,Time Constant
;
003,0,Brake && Engine Status
003,1,Brake
003,2,Brake Status,,Range: ON/OFF
003,3,Engine
003,4,Engine Status,,Range: ON/OFF
;
004,1,Voltage at,Light Input
004,2,Sensor,Voltage Supply
004,3,Basic Frequency,Sensor Front (G78)
004,4,Basic Frequency,Sensor Rear (G76)
;
005,1,Front Sensor (G78),(learned)
005,2,Rear Sensor (G76),(learned)
005,3,Movement,Front Suspension,Range: -127.0...+128.0 mm
005,4,Movement,Rear Suspension,Range: -127.0...+128.0 mm
;
125,0,CAN-Databus Communication (Powertrain)
125,1,Brake Electronics,(J104),Range: ABS 1/ABS 0\nSpecification: ABS 1
125,2,CAN-Gateway,(J533),Range: Gateway 1/Gateway 0\nSpecification: Gateway 1
125,3,Power Steering,(J500),Range: Steer. ang. 1/Steer. ang. 0\nSpecification: Steer. ang. 1
125,4,Engine,Electronics,Range: Engine 1/Engine 0\nSpecification: Engine 1
;
126,0,CAN-Databus Communication (Powertrain)
126,1,Instrument Cluster,(J285),Range: Instruments 1/Instruments 0\nSpecification: Instruments 1
126,2,Level Control,(J197),Range: Level 1/Level 0\nSpecification: Level 1
;
225,0,Electro Magnetic Compatibility (EMC) Counter
225,1,Brake Electronics,(J104)
225,2,CAN-Gateway,(J533)
225,3,Power Steering,(J500)
225,4,Engine,Electronics
;
226,0,Electro Magnetic Compatibility (EMC) Counter
226,1,Instrument Cluster,(J285)
226,2,Level Control,(J197)
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A001,0,Dynamic Control Strategy
A001,5,Dynamic Control Strategy
A001,6,4 = Standard
;
A002,0,Adjustment Range Front (Low Value)
A002,5,Adjustment Range Front (Low Value)
A002,6,1 = Standard
;
A003,0,Adjustment Range Front (High Value)
A003,5,Adjustment Range Front (High Value)
A003,6,7 = Audi A3 (8P)
A003,7,13 = Audi A4 (8E) / Audi A6 (4F)
;
A004,0,Adjustment Range Rear (Low Value)
A004,5,Adjustment Range Rear (Low Value)
A004,6,1 = Audi A4 (8E) / Audi A6 (4F)
A004,7,7 = Audi A3 (8P)
;
A005,0,Adjustment Range Rear (High Value)
A005,5,Adjustment Range Rear (High Value)
A005,6,13 = Standard
;
A006,0,Warning Lamp Enabling
A006,5,Warning Lamp Enabling
A006,6,0 = Warning Lamp Activation suppressed
A006,7,1 = Warning Lamp Activation enabled
;
A007,0,Terminal 61 Function Enabling
A007,5,Terminal 61 Function Enabling
A007,6,0 = Terminal 61 Function locked (Reference Run after Terminal 15 ON)
A007,7,1 = Terminal 61 Function enabled (Reference Run after Engine Start)
;
A008,0,Sensor Plausibility Enabling
A008,5,Sensor Plausibility Enabling
A008,6,0 = Sensor Malfunction Plausibility locked
A008,7,1 = Sensor Malfunction Plausibility enabled
;
A009,0,MIL Enabling
A009,5,MIL Enabling
A009,6,0 = MIL locked (in Output Test)
A009,7,1 = MIL enabled (in Output Test)
;
A010,0,Tourist Solution
A010,5,Tourist Solution
A010,6,When driving in countries where driving is performed on the
A010,7,opposite side as in the native country the headlights must
A010,8,be changed over to avoid blinding the oncoming traffic.
A010,9, 
A010,10,0 = Disabled
A010,11,1 = Enabled
A010,12, 
A010,13,Note: Only supported for 8P0-907-357-C @ 0020 or newer!
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Headlight Range Control (J431) Coding
C01,0000001 = Audi A3 (8P) Front-Wheel-Drive (FWD)
C02,0000002 = Audi A3 (8P) All-Wheel-Drive (AWD)
C03,0000003 = Audi A6 (4F) with Steel Suspension
C04,0000004 = Audi A6 (4F) with Air Suspension
C05,0000005 = Audi A4 (8E) & Audi A4 Cabriolet (8H)
C06,0000006 = Audi A8 (4E)
C07,0000007 = Audi Q7 (4L) with Steel Suspension
C08,0000008 = Audi Q7 (4L) with Air Suspension
C09,0000009 = Audi TT (8J) with Steel Suspension and Front-Wheel-Drive (FWD)
C10,0000010 = Audi TT (8J) with Steel Suspension and All-Wheel-Drive (AWD)
C11,0000011 = Audi TT (8J) with Magnetic Ride
C12,0000012 = Audi A3 (8P) with Single Frame Grill (SFG)
C13,0000013 = Audi A3 (8P) Cabriolet
C14,0000015 = VW Scirocco (13) with Standard Suspension
C15,0000016 = VW Scirocco (13) with Dynamic Chassis Control (DCC)
;
;
;---------------------------------------------------
;
; selective output test
;
;---------------------------------------------------
;
;
T1540,Headlight Range Control: Adjusting to Lowered Position
T1541,Headlight Range Control: Adjusting to Raised Position
T2232,Headlight Range Control: Adjusting to Delivery Position
;
