;
; VCDS Label File
;
; Copyright © 2010 Ross-Tech, LLC
;
; Audi R8 (42)
;
; Component: J525 - Sound System (#47)
;
; P/N: 420-035-223-???
;
; includes measuring blocks and coding
;
; created on 24/Apr/2010 by Sebastian Stange (sebastian@ross-tech.com)
;
; last modification on 24/Apr/2010
;
; requires VCDS 908.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Allgemein
001,1,Voltage,(Terminal 30),Specification: 9.0...15.0 V
001,2,Spannungs-,klemmen,x000xxx1 = Terminal S aktive\nx000xx1x = Terminal 15 aktive\nx000x1xx = Terminal X aktive\nx0001xxx = Terminal 50 aktive\n1000xxxx = Status invalid
;
002,0,System Status
002,1,Temperature,Analog Circuit
002,2,Temperature,Digital Circuit
002,3,Cooling Fan,Speed
002,4,Activation Input,,000 = Signal OFF\n001 = Signal ON
;
003,0,System Status
003,1,Microphone,Input Voltage
003,2,Vehicle Speed
;
080,0,Advanced Control Module Identification I
;
081,0,Advanced Control Module Identification II
081,1,Serial Number
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Sound System (J525) Coding
C01,00?xxxx: Noise Cancellation
C02,1 = Noise Cancellation inactive
C03,2 = Noise Cancellation via GALA from Radio (Sound System Standard)
C03,3 = Noise Cancellation via CAN
C04,4 = Noise Cancellation via Microphone/Amplifier (Sound System Premium)
C05,00x?xxx: Volume Adjustment
C06,0 = Volume Adjustment inactive
C07,1 = Volume Increase by 1dB / 2 = Volume Increase by 2dB
C08,3 = Volume Increase by 3dB / 4 = Volume Increase by 4dB
C09,5 = Volume Increase by 5dB / 6 = Volume Increase by 6dB (Standard)
C10,7 = Volume Reduction by 1dB / 8 = Volume Reduction by 2dB
C11,9 = Volume Reduction by 3dB
C12,00xx?xx: Activation
C13,1 = Activation via Signal Wire (Standard)
C14,2 = Activation via (Audio Source) Signal Level
C15,00xxx?x: Vehicle Type
C16,1 = Audi R8 (423) Coupé
;2 = Audi R8 (42) Roadster
C17,00xxxx?: Options
C18,1 = Left-Hand-Drive (LHD)
C19,2 = Right-Hand-Drive (RHD)
;
