;
; VAG-COM label file 3D0-907-040.lbl
;
; VW Phaeton (3D) - up to and including model year 2006 
;
; component: Auto HVAC - 4 Zone Climatronic  -J255-  (#08)
;
;
; p/n: 3D0 907 040 F  Component: Climatronic D1 1132   Coding: 0000001 (2004 Phaeton W12 NAR) (Brent)
; p/n: 3D0 907 040 G  Component: Climatronic D1 1145   Coding: 0000002 (2004 Phaeton W12 NAR) (David C)
; p/n: 3D0 907 040 G  Component: Climatronic D1 1132   Coding: 0000001 (2004 Phaeton W12 NAR) (Mike M)
; p/n: 3D0 907 040 F  Component: Climatronic D1 1132   Coding: 0000001 (2004 Phaeton W12 ROW) (Daniel)
; p/n: 3D0 907 040 H  Component: Climatronic D1 2021   Coding: 0000001 (2005 Phaeton V8 NAR) (Robert)
; p/n: 3D0 907 040 H  Component: Climatronic D1 2021   Coding: 0000001 (2004 Phaeton W12 ROW) (DD AM 2662)
; p/n: 3D0 907 040 H  Component: Climatronic D1 2021   Coding: 0000001 (2005 Phaeton V6 TDI ROW) (Alex)
; p/n: 3D0 907 040 J  Component: Climatronic D1 2031   Coding: 0000002 (2006 Phaeton W12 NAR) (jyoung8607)
; p/n: 3W0 907 040 G  Component: Climatronic BY  614   Coding: 0000001 (Bentley ROW)
; p/n: 3W0 907 040 B  Component: Climatronic BY  614   Coding: 0000002 (Bentley NAR)
;
; created on 28/Aug/2005 by Michael Moore (Moore@Ross-Tech.com)
; updated on 06/Oct/2006 by Michael Moore (Moore@Ross-Tech.com)
; updated on 12/Sep/2011 by Sebastian Stange (Sebastian@Ross-Tech.com)
; re-written on 7/Dec/2011 by Jason Young (jyoung8607@gmail.com)
; updated 13/Dec/2011 by Jason Young (jyoung8607@gmail.com)
; updated 3/Jan/2012 by Jason Young (jyoung8607@gmail.com)
;
;
;
001,0,AC Compressor and Refrigerant Status
001,1,Compressor,Shut-Off Reason,Display Range: 0...22\nSee label file for list of reason codes
001,2,Evaporator,Temp. (G308),Display Range: -40...60°C\nAfter evaporator in air conditioning enclosure
001,3,Refrigerant,Temp. (G395),Display Range: -40...155°C\nBetween compressor high-pressure line and condenser
001,4,Refrigerant,Pressure (G395),Display Range: 0...38 bar\nBetween compressor high pressure line and condenser
; Compressor shut-off codes:
;  0 = Compressor ON: AC switched on - all requirements met
;  1 = Refrigerant pressure too high: > 32 bar
;  2 = Blower motor malfunction: actual voltage < 3 V
;  3 = Refrigerant pressure too low: < 2 bar (depending on outside temperature)
;  4 = (not used)
;  5 = Engine not running or engine runtime < 4 seconds
;  6 = ECON mode activated
;  7 = AC shut off - blower speed 0
;  8 = Outside temperature too low: < -8°C/-5°C
;  9 = Both outside temperature sensors malfunctioning
; 10 = (not used)
; 11 = Engine temperature too high
; 12 = ECU requested shutoff (overheat/kickdown/etc)
; 13 = Voltage too high: Terminal 15 > 17V
; 14 = (not used)
; 15 = (not used)
; 16 = Compressor activation circuit fault - N280 signal missing or implausible
; 17 = Refrigerant pressure monitor circuit fault - G65 signal missing or implausible
; 18 = Intervention load management - A/C stage 2
; 19 = Refrigerant loss - current drive cycle only
; 20 = Refrigerant loss - permanent
; 21 = -8°C/-5°C < outside temperature < 1°C/3°C and no recirc air request
; 22 = -8°C/-5°C < outside temperature < 1°C/3°C and interior temp < 10°C
;
002,0,Fresh Air Blower (V2) / Control Unit for Fresh Air Blower (J126)
002,1,V2 Blower,Voltage (Actual),Display Range: 0.0...13.0 V
002,2,V2 Blower,Voltage (Spec.),Display Range: 0.0...13.0 V
002,3,V2 Blower,Speed,Display Range: 0.0...100.0 %
002,4,Supply Voltage,Terminal 30,Display Range: 0...18 V
;
; MVB 003 F1 may track V50 pump or request to engine-specific recirculation
; pump, comes on with residual heat. VW sources say "via CAN" when V50 is
; directly controlled by Climatronic, so may point toward V51/V55/V36/?
;
003,0,Temperature Monitoring
003,1,Coolant Pump,,Display Range: ON/OFF
003,2,Outside Temp,Ambient (G17),Display Range: -40...60°C
003,3,Outside Temp,HVAC Intake (G89),Display Range: -40...60°C
003,4,V210 Blower,RPM,Display Range: 0...9950/min\nExpected: ~2700 RPM\nPulls air across cabin temperature sensor G56
;
004,0,Pump Valve Controls and Heat Exchanger Temperatures
004,1,Regulation Valve,Left (N175),Display Range: 0.0...100.0 %
004,2,Exchanger Temp,Left (G306),Display Range: 0...100°C
004,3,Regulation Valve,Right (N176),Display Range: 0.0...100.0 %
004,4,Exchanger Temp,Right (G307),,Display Range: 0...100°C
;
; MVB 005 data sources:
;
; F1 Recirc request and F2 air quality MVB baseline taken from VCDS label
; file 4B0-820-043-MY2 for which a similar sensor is used. Updated based
; on observed behavior for jyoung8607's 2006 NAR Phaeton.
;
; Operation principle data based on Bentley Publishers eBahn docs:
; Volkswagen > Phaeton > 2004-2006 Heating, Ventilation and Air Conditioning
;   80 - Heating and A/C Unit, Disassembling and Assembling
;     Air Quality Sensor, Function
;
005,0,Air Recirculation Status and Air Quality Sensor (G238) Status
005,1,Recirculation,Requested,0 = Recirculation NOT requested\n10 = Recirculation requested by Air Quality Sensor (G238)\n11 = Recirculation requested by G238 but rejected (Automatic Recirculation inactive)\n12 = Recirculation requested by G238 but rejected (compressor OFF)\n13 = Recirculation requested by G238 but rejected (defrost active)\n20 = Manual Recirculation active\n25 = Recirculation active (vehicle startup or 30 second additional recirc time to dampen on/off change cycling)\n30 = Recirculation active (wiper/headlamp washer active)\n40 = Recirculation active (high ambient temperature)\n50 = Recirculation active (A/C inactive/blower speed 0)\n60 = Partial Recirculation active
;   0 = Recirculation NOT requested
;  10 = Recirculation requested by Air Quality Sensor (G238)
;  11 = Recirculation requested by G238 but rejected (Automatic Recirculation inactive)
;  12 = Recirculation requested by G238 but rejected (compressor OFF)
;  13 = Recirculation requested by G238 but rejected (defrost active)
;  20 = Manual Recirculation active
;  25 = Recirculation active (vehicle startup or 30 second additional recirc time to dampen on/off change cycling)
;  30 = Recirculation active (wiper/headlamp washer active)
;  40 = Recirculation active (high ambient temperature)
;  50 = Recirculation active (A/C inactive/blower speed 0)
;  60 = Partial Recirculation active
005,2,Air Quality,Sensor (G238),0 = Missing Signal from Air Quality Sensor (G238)\n1 = Recirculation requested: Low Increase in oxidisable Gases \n2 = Recirculation requested: High Increase in oxidisable Gases\n3 = Recirculation requested: Low Increase in reducible Gases\n4 = Recirculation requested: High Increase in reducible Gases\n5 = Recirculation NOT requested (Fresh Air Mode/No Pollution recognised)\n7 = Recirculation NOT requested (Fresh Air Mode/No Pollution recognised)\n254 = No Signal from Air Quality Sensor (G238) sensor not yet ready / engine start-up\n255 = No Signal from Air Quality Sensor (G238) engine shut down
;   0 = Missing Signal from Air Quality Sensor (G238) unknown
;   1 = Recirculation requested: Low Increase in oxidisable Gases
;   2 = Recirculation requested: High Increase in oxidisable Gases 
;   3 = Recirculation requested: Low Increase in reducible Gases
;   4 = Recirculation requested: High Increase in reducible Gases
;   5 = Recirculation NOT requested (Fresh Air Mode/No Pollution recognised)
;   7 = Recirculation NOT requested (Fresh Air Mode/No Pollution recognised)
; 254 = No Signal from Air Quality Sensor (G238) sensor not yet ready / engine start-up
; 255 = No Signal from Air Quality Sensor (G238) engine shut down
005,3,Heated Windshield,,Display Range: ON/OFF\nWithout respect to whether heated windshield is equipped on vehicle
005,4,Refrigerant Loss,Shutoff Count,Number of compressor shut-off procedures due to refrigerant loss
;
006,0,Interior Air Distribution Temperatures
006,1,Dash Panel,Console (G56),Display Range: -40...100°C
006,2,Dash Panel Vent,Center (G191),Display Range: -40...100°C
006,3,Rear Center Vent,Left (G311),Display Range: -40...100°C
006,4,Rear Center Vent,Right (G312),Display Range: -40...100°C
;
007,0,Rear Left and Rear Right Air Distribution with PTC Heating
007,1,PTC Heater Load,Left (Z42),Display Range: 0.0...100.0 %
007,2,Temp After PTC,Left (G309),Display Range: -40...100°C
007,3,PTC Heater Load,Right (Z43),Display Range: 0.0...100.0 %
007,4,Temp After PTC,Right (G310),Display Range: -40...100°C
;
008,0,Windshield Temperature (G355) with Solar Load Sensor (G134)
008,1,Light Intensity,From Left Side,Display Range: 0.0...100.0 %
008,2,Light Intensity,From Right Side,Display Range: 0.0...100.0 %
008,3,Windshield,Temp. (G355),Display Range: -40...90.0°C\nG355 IR pickup from glass
008,4,Relative Humidity,,Display Range: 0%...100%
;
009,0,Compressor Regulating Valve (N280)
009,1,Regulator,Current (Spec.),Display Range: 0...1.275A
009,2,Regulator,Current (Actual),Display Range: 0...1.275A
009,3,Compressor,RPM,Display Range: 0...9950/min
009,4,Compressor,Load Torque,Display Range: 0...20 Nm
;
010,0,Flap Motor V107/G135: Front Windshield Defrost Vent
010,1,Current Value,,Display Range: 0...255
010,2,Specified Value,,Display Range: 0...255
010,3,Minimum Position,Blocked,Display Range: 0...255
010,4,Maximum Position,Open,Display Range: 0...255
;
011,0,Flap Motor V108/G139: Front Left Footwell Vent
011,1,Current Value,,Display Range: 0...255
011,2,Specified Value,,Display Range: 0...255
011,3,Minimum Position,Blocked,Display Range: 0...255
011,4,Maximum Position,Open,Display Range: 0...255
;
012,0,Flap Motor V109/G140: Front Right Footwell Vent
012,1,Current Value,,Display Range: 0...255
012,2,Specified Value,,Display Range: 0...255
012,3,Minimum Position,Blocked,Display Range: 0...255
012,4,Maximum Position,Open,Display Range: 0...255
;
013,0,Flap Motor V200/G318: Front Left Distribution Shutoff (Chest Vent/Defrost)
013,1,Current Value,,Display Range: 0...255
013,2,Specified Value,,Display Range: 0...255
013,3,Minimum Position,Blocked,Display Range: 0...255
013,4,Maximum Position,Open,Display Range: 0...255
;
014,0,Flap Motor V199/G317: Front Right Distribution Shutoff (Chest Vent/Defrost)
014,1,Current Value,,Display Range: 0...255
014,2,Specified Value,,Display Range: 0...255
014,3,Minimum Position,Blocked,Display Range: 0...255
014,4,Maximum Position,Open,Display Range: 0...255
;
015,0,Flap Motor V197/G315: Distribution Temperature Control - Heater Bypass Air
015,1,Current Value,,Display Range: 0...255
015,2,Specified Value,,Display Range: 0...255
015,3,Minimum Position,Blocked,Display Range: 0...255
015,4,Maximum Position,Open,Display Range: 0...255
;
016,0,Flap Motor V198/G316: Distribution Temperature Control - Heated Air
016,1,Current Value,,Display Range: 0...255
016,2,Specified Value,,Display Range: 0...255
016,3,Minimum Position,Open,Display Range: 0...255
016,4,Maximum Position,Blocked,Display Range: 0...255
;
017,0,Flap Motor V71/G113: Outside Air Flow / Backpressure - Under Hood Plenum
017,1,Current Value,,Display Range: 0...255
017,2,Specified Value,,Display Range: 0...255
017,3,Minimum Position,Blocked,Display Range: 0...255
017,4,Maximum Position,Open,Display Range: 0...255
;
018,0,Flap Motor V113/G142: Recirculation - Dash Panel Air Intake
018,1,Current Value,,Display Range: 0...255
018,2,Specified Value,,Display Range: 0...255
018,3,Minimum Position,Open,Display Range: 0...255
018,4,Maximum Position,Blocked,Display Range: 0...255
;
019,0,Flap Motor V206/G324: Front Left Distribution Split for Chest/Defrost Vents
019,1,Current Value,,Display Range: 0...255
019,2,Specified Value,,Display Range: 0...255
019,3,Minimum Position,Chest Vent,Display Range: 0...255
019,4,Maximum Position,Defrost,Display Range: 0...255
;
020,0,Flap Motor V205/G323: Front Right Distribution Split for Chest/Defrost Vents
020,1,Current Value,,Display Range: 0...255
020,2,Specified Value,,Display Range: 0...255
020,3,Minimum Position,Chest Vent,Display Range: 0...255
020,4,Maximum Position,Defrost,Display Range: 0...255
;
021,0,Flap Motor V213/G330: Dash Panel Indirect Ventilation Vents
021,1,Current Value,,Display Range: 0...255
021,2,Specified Value,,Display Range: 0...255
021,3,Minimum Position,Blocked,Display Range: 0...255
021,4,Maximum Position,Open,Display Range: 0...255
;
022,0,Flap Motor V110/G387: Center Left Dash Panel Vent
022,1,Current Value,,Display Range: 0...255
022,2,Specified Value,,Display Range: 0...255
022,3,Minimum Position,Blocked,Display Range: 0...255
022,4,Maximum Position,Open,Display Range: 0...255
;
023,0,Flap Motor V111/G388: Center Right Dash Panel Vent
023,1,Current Value,,Display Range: 0...255
023,2,Specified Value,,Display Range: 0...255
023,3,Minimum Position,Blocked,Display Range: 0...255
023,4,Maximum Position,Open,Display Range: 0...255
;
024,0,Flap Motor V207/G325: Left Dash Panel Design Cover
024,1,Target Position,Left,Display Range: Open/Closed\nExact positioning data is not reported for this device
;024,2,Unused
;024,3,Unused
;024,4,Unused
;
025,0,Flap Motor V208/G326: Center Dash Panel Design Cover
025,1,Target Position,Center,Display Range: Open/Closed\nExact positioning data is not reported for this device
;025,2,Unused
;025,3,Unused
;025,4,Unused
;
026,0,Flap Motor V209/G327: Right Dash Panel Design Cover
026,1,Target Position,Right,Display Range: Open/Closed\nExact positioning data is not reported for this device
;026,2,Unused
;026,3,Unused
;026,4,Unused
;
027,0,Flap Motor V204/G322: Rear Center Left - Heater Bypass Air
027,1,Current Value,,Display Range: 0...255
027,2,Specified Value,,Display Range: 0...255
027,3,Minimum Position,Blocked,Display Range: 0...255
027,4,Maximum Position,Open,Display Range: 0...255
;
028,0,Flap Motor V203/G321: Rear Center Right - Heater Bypass Air
028,1,Current Value,,Display Range: 0...255
028,2,Specified Value,,Display Range: 0...255
028,3,Minimum Position,Blocked,Display Range: 0...255
028,4,Maximum Position,Open,Display Range: 0...255
;
029,0,Flap Motor V202/G320: Rear Center Left - Heated Air
029,1,Current Value,,Display Range: 0...255
029,2,Specified Value,,Display Range: 0...255
029,3,Minimum Position,Open,Display Range: 0...255
029,4,Maximum Position,Blocked,Display Range: 0...255
;
030,0,Flap Motor V201/G319: Rear Center Right - Heated Air
030,1,Current Value,,Display Range: 0...255
030,2,Specified Value,,Display Range: 0...255
030,3,Minimum Position,Open,Display Range: 0...255
030,4,Maximum Position,Blocked,Display Range: 0...255
;
031,0,Flap Motor V212/G329: Rear Left Dist. Shutoff (B-Pillar/Footwell/Defrost)
031,1,Current Value,,Display Range: 0...255
031,2,Specified Value,,Display Range: 0...255
031,3,Minimum Position,Blocked,Display Range: 0...255
031,4,Maximum Position,Open,Display Range: 0...255
;
032,0,Flap Motor V211/G328: Rear Right Dist. Shutoff (B-Pillar/Footwell/Defrost)
032,1,Current Value,,Display Range: 0...255
032,2,Specified Value,,Display Range: 0...255
032,3,Minimum Position,Blocked,Display Range: 0...255
032,4,Maximum Position,Open,Display Range: 0...255
;
033,0,Flap Motor V196/G314: Rear Left Dist. Splitter (B-Pillar/Footwell/Defrost)
033,1,Current Value,,Display Range: 0...255
033,2,Specified Value,,Display Range: 0...255
033,3,Minimum Position,B-Pillar Only,Display Range: 0...255\nMulti-position motor ranging from B-Pillar to Defrost to Footwell
033,4,Maximum Position,Footwell Only,Display Range: 0...255\nMulti-position motor ranging from B-Pillar to Defrost to Footwell
;
034,0,Flap Motor V195/G313: Rear Right Dist. Splitter (B-Pillar/Footwell/Defrost)
034,1,Current Value,,Display Range: 0...255
034,2,Specified Value,,Display Range: 0...255
034,3,Minimum Position,B-Pillar Only,Display Range: 0...255\nMulti-position motor ranging from B-Pillar to Defrost to Footwell
034,4,Maximum Position,Footwell Only,Display Range: 0...255\nMulti-position motor ranging from B-Pillar to Defrost to Footwell
;
035,0,Rocker Switches - Dash Panel Vent Controls
035,1,Chest Vent,Left (E301),Display Range: Open/Closed/Not Oper.
035,2,Chest Vent,Ctr Left (E302),Display Range: Open/Closed/Not Oper.
035,3,Chest Vent,Ctr Right (E303),Display Range: Open/Closed/Not Oper. 
035,4,Chest Vent,Right (E304),Display Range: Open/Closed/Not Oper.
;
036,0,Rocker Switches - Rear Console Vent and Temp Differential Controls
036,1,Rear Ctr Vent,Left (E306),Display Range: Open/Closed/Not Oper.
036,2,Rear Ctr Vent,Right (E307),Display Range: Open/Closed/Not Oper.
036,3,Chest/Footwell,Diff. (E305),Display Range: Open/Closed/Not Oper.
;036,4,Unused
;
037,0,Defrost Shutoff Controls (Front Doors)
037,1,Driver's Door,Button (E323),Display Range: ON/OFF\nReceived via CAN from door control module (J386)
037,2,Defrost Blocked,Front Left,Display Range: ON/OFF
037,3,Passenger Door,Button (E324),Display Range: ON/OFF\nReceived via CAN from door control module (J387)
037,4,Defrost Blocked,Front Right,Display Range: ON/OFF
;
038,0,Defrost Shutoff Controls (Rear Doors)
038,1,Left B-Pillar,Button (E299),Display Range: ON/OFF
038,2,Defrost Blocked,Rear Left,Display Range: ON/OFF\nRear door defrost and rear indirect venting are the same thing
038,3,Right B-Pillar,Button (E300),Display Range: ON/OFF
038,4,Defrost Blocked,Rear Right,Display Range: ON/OFF\nRear door defrost and rear indirect venting are the same thing
;
039,0,Vehicle Information from CAN
039,1,Terminal 15,,Display Range: ON/OFF
039,2,Terminal X,,Display Range: ON/OFF
039,3,Parking Heater,,Display Range: ON/OFF
039,4,Parking Ventilation,,Display Range: ON/OFF
;
040,0,Vehicle Information from CAN (Compressor Related)
040,1,Engine Speed,Increase,Display Range: ON/OFF
040,2,Compressor,Operating,Display Range: ON/OFF
040,3,Compressor,Engine Disabled,Display Range: 0...1\n0 = No shutoff request\n1 = Shutoff request (kickdown/overtemp/etc)
040,4,Coolant Fan,,Display Range: 0%...100%
;
041,0,Vehicle Information from CAN (Engine and Coolant State)
041,1,Standing Time,Minutes,Display Range: 0.0...120.0 minutes
041,2,Vehicle,Speed,Display Range: 0...324km/h
041,3,Engine,RPM,Display Range: 0...9950/min
041,4,Coolant,Temperature,Display Range: -48...127°C
;
; MVB 042 F4 documented by VW but not observed on any of three test vehicles.
;
042,0,Vehicle Information from CAN (Miscellaneous)
042,1,Washer Fluid,Pump Active,Display Range: ON/OFF\nUsed as input into auto-recirculate function
;042,2,Unused
;042,3,Unused
042,4,Key Number,,Display Range: 0...15\nMay not be present on many vehicles
;
; MVB 043 F3 is not documented by VW and is not present on some, possibly
; older Climatronic modules (missing on -F, present on -H and -J with 2XXX
; generation software). Probably involved with load management but effect
; is unknown.
;
043,0,Vehicle Information from CAN (Intervention Load Management)
043,1,Load Control,PTC Heaters,Display Range: 0...4\n0 = No intervention / full power available\n1 = Stage 1 intervention / 75% available\n2 = Stage 2 intervention / 50% available\n3 = Stage 3 intervention / 25% available\n4 = Stage 4 intervention / 0% available
043,2,Load Control,Heated Windshield,Display Range: 0...1\n0 = No intervention / heating available\n1 = Intervention / no windshield heating
043,3,Unknown,,Display Range: ON/OFF
043,4,Load Control,Air Conditioning,Display Range: 0...3\n0 = No intervention / full speed available\n1 = Stage 1 intervention / blower motor limited to 30%\n2 = Stage 2 intervention / compressor disable\n3 = Stage 3 intervention / unknown
;
044,0,Potentiometer Reference Voltages
044,1,External Ref 1,Voltage,Display Range: 4.5V...5.5V\nExpected: 5.0V
044,2,External Ref 2/3,Voltage,Display Range: 4.5V...5.5V\nExpected: 5.0V
;044,3,Unused
;044,4,Unused
;
045,0,Unknown single-field data
045,1,Unknown
;045,2,Unused for single-field MVB
;045,3,Unused for single-field MVB
;045,4,Unused for single-field MVB
;
; MVB 046 not present on older Climatronic modules. 
;
; MVB 046 F1/F2/F3/F4 values never seem to change in the test vehicle.
; Readings are always 0/0/1/1; might be CAN bus communication states.
;
046,0,Unknown values
046,1,Unknown
046,2,Unknown
046,3,Unknown
046,4,Unknown
;
; MVB 047 not present on older Climatronic modules.
;
047,0,Windshield Temp and Humidity Sensor (G355) via Roof Electronics (J528)
047,1,Humidity,Cabin (G355),Display Range: 0.0...100.0 %
047,2,Temperature,Cabin (G355),G355 cabin air temperature
047,3,Temperature,Windshield (G355),G355 IR pickup from glass
047,4,Temperature,Reference (G355),G355 internally generated reference temperature (heater N340)
;
080,0,Advanced Control Module Identification I
080,1,Advanced,Identification I
;
082,0,Advanced Control Module Identification III
082,1,Advanced,Identification III
;
;---------------------------------------------------
;
; Adaptation
;
;---------------------------------------------------
;
A001,0,Flap Motor Basic Setting/Normalization
A001,5,Flap Motor Basic Setting/Normalization
A001,6,To initialize the Flap Motor Basic Setting/Normalization
A001,7,Enter "2" as new Value and press Test/Save. The Procedure
A001,8,start automatically and run for about 35 Seconds.
;
;---------------------------------------------------
;
; Basic settings - No basic settings blocks exist
;
;---------------------------------------------------
;
B001,0,*Use Adaptation Block 001 for Flap Motor Basic Settings*
