;
; VAG-COM Label File
;
; Audi A6 (4F) / Audi Q7 (4L)
;
; Component: J502 - Tire Pressure Monitoring (#65) - BASIS
;
; P/N: 4F0-910-273-???
;
; includes measuring blocks and coding
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 4F-65.LBL
; 4F0-910-273-BA.LBL
; 4F0-910-273-HI.LBL
;
; created on 28/May/2006 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification: 20/Mar/2008
;
; requires VAG-COM 505.1 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;

;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Tire Pressure Monitoring (J502) Coding
C01,0?xxxxx: Data Carrier
C02,2 = 1 Antenna + 4 Trigger @ 433 MHz (High / PR-7K3)
C03,3 = 1 Antenna + 4 Trigger @ 315 MHz (High / PR-7K4)
C04,0x?xxxx: Type
C05,0 = Rest of World (RoW)
C06,4 = USA
C07,+1 = Emergency Mode (Run Flat Tires)
C08,+2 = Extra Load
C09,0xx?xxx: Front Axle (Partial Load) I
C10,1 = 1.x bar / 2 = 2.x bar / 3 = 3.x bar
C11,0xxx?xx: Front Axle (Partial Load) II
C12,0 = x.0 bar / 1 = x.1 bar / 2 = x.2 bar / 3 = x.3 bar / 4 = x.4 bar
C13,5 = x.5 bar / 6 = x.6 bar / 7 = x.7 bar / 8 = x.8 bar / 9 = x.9 bar
C14,0xxxx?x: Rear Axle (Partial Load) I
C15,1 = 1.x bar / 2 = 2.x bar / 3 = 3.x bar
C16,0xxxxx?: Rear Axle (Partial Load) II
C17,0 = x.0 bar / 1 = x.1 bar / 2 = x.2 bar / 3 = x.3 bar / 4 = x.4 bar
C18,5 = x.5 bar / 6 = x.6 bar / 7 = x.7 bar / 8 = x.8 bar / 9 = x.9 bar
;
