;
; VCDS Label File
;
; Copyright © 2008+ Ross-Tech, LLC
;
; Audi A3 (8P)
;
; Component: R - Radio (#56) - Chorus/Concert/Symphony 2
;
; P/N: ??0-035-1??-???
;
; includes measuring blocks, adaptation, coding and selective output test
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 8P-56.LBL
; 8P0-035-1xx-56.LBL
;
; created on 23/Oct/2008 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 11/Jul/2012
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,General
001,1,Voltage,(Terminal 30),Specification: 9.0...15.0 V
001,2,Amplifier,Output,only if Amplifier installed
001,3,Telephone
001,4,Telephone,Mute Signal,Range: ON/OFF
;
002,0,Speaker/Line-Out (Front Left)
002,1,Location/Type
002,2,Status
;
003,0,Remote Feed Antenna I
003,1,Type
003,2,Component
003,3,Status
;
004,0,CD-Connection
004,1,Component
004,2,Status,,Display Range: OK/not OK
;
005,1,IF-Output
005,2,IF-Output,Status
;
080,0,Advanced Control Module Identification I
080,1,Identification
080,2,Revision
080,3,Production,Date
080,4,Manufacturer &,Test Stand Number
;
081,0,Advanced Control Module Identification II
081,1,Serial Number
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Radio (R) Coding
C01,0?xxxxx: Configuration I
C02,+1 = Satellite Radio installed / +2 = Digital Radio installed
C03,+4 = Vehicle Speed Display available
C04,0x?xxxx: Configuration II
C05,+1 = Front Speaker Monitoring inactive
C06,+2 = GALA-Function inactive / +4 = Long Wave Reception inactive
C07,0xx?xxx: Sound Characteristics
C08,0 = Linear Sound Characteristics
C09,1 = Audi A3 (8P1)
C10,2 = Audi A3 Sportback (8PA)
C11,0xxx?xx: Fader/BOSE/Amplifier
C12,+1 = Fader Display ON
C13,+2 = BOSE Display ON
C14,+4 = Amplifier Deactivation with incoming Call ON
C15,0xxxx?x: Options I
C16,+1 = Navigation System installed / +2 = Telephone installed
C17,+4 = Speech Recognition installed
C18,0xxxxx?: Options II
C19,+1 = Antenna Diversity installed / +2 = CD-Changer installed
C20,+4 = Multi-Function Steering Wheel installed
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A002,0,Remote Control: Frequency FM
;969
A002,1,Reception,Level,Unit: dBµV
;45.0
A002,5,Remote Control: Frequency FM
A002,6,The FM Frequency is being selected by entering the
A002,7,Value without Decimal Point (i.e. 968 for 96.8 MHz).
;
;A003,0,
;0
;A003,1,
;36.0
;
;A004,0,
;0
;A004,1,
;31.0
;
A005,0,Remote Control: Volume
A005,5,Remote Control: Volume
A005,6,Range: 0...30 dB
A005,7, 
A005,8,The selected Volume will stay active
A005,9,after closing the Diagnostic Session.
;
A006,0,Signal Position
A006,5,Signal Position
A006,6,0 = Fader Center / Balance Center
A006,7,1 = Fader Front / Balance Left
A006,8,2 = Fader Front / Balance Right
A006,9,3 = Fader Rear / Balance Left
A006,10,4 = Fader Rear / Balance Right
;
