;
; VCDS Label File
;
; Copyright © 2004+ Ross-Tech, LLC
;
; Audi A8 (4D)
;
; Component: J446 - Parking Aid (#76)
;
; P/N: 4D0-919-283-???
;
; includes measuring blocks, adaptation and coding
;
; created on 02/Feb/2004 by Dave Eaton (Dave.Eaton@clear.net.nz)
; updated on 22/Jul/2014 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 08/Sep/2014
;
; requires VCDS 12.12.2 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
;
001,0,Distance (Front)
001,1,Front Left,Sensor,Specification: 0...200 cm (255 cm = no obstacle recognized)
001,2,Front Left,Center Sensor,Specification: 0...200 cm (255 cm = no obstacle recognized)
001,3,Front Right,Center Sensor,Specification: 0...200 cm (255 cm = no obstacle recognized)
001,4,Front Right,Sensor,Specification: 0...200 cm (255 cm = no obstacle recognized)
;
002,0,Distance (Rear)
002,1,Rear Left,Sensor,Specification: 0...200 cm (255 cm = no obstacle recognized)
002,2,Rear Left,Center Sensor,Specification: 0...200 cm (255 cm = no obstacle recognized)
002,3,Rear Right,Center Sensor,Specification: 0...200 cm (255 cm = no obstacle recognized)
002,4,Rear Right,Sensor,Specification: 0...200 cm (255 cm = no obstacle recognized)
;
003,0,Resulting Distance / Vehicle Speed && Voltage
003,1,Resulting,Distance Front,Specification: 0...200 cm (255 cm = no obstacle recognized)
003,2,Resulting,Distance Rear,Specification: 0...200 cm (255 cm = no obstacle recognized)
003,3,Vehicle Speed,,Display Range: 0.0...255.0 km/h
003,4,Sensor,Voltage Supply
;
004,1,Confirmation,Tone,Range: Tone ON/Tone OFF
004,2,Reverese Gear,engaged,Range: Reverse YES/Reverse NO
004,3,Trailer hitched,,Range: Trailer YES/Trailer NO
004,4,Trunk/Boot,Status,Range: Lid open/Lid closed
;
005,0,Function Button (E266)
005,1,Function Button,(E266) operated,Range: Button YES/Button NO
005,2,Function LED,(E266) Status,Range: LED ON/LED OFF
;
006,0,Oscillation Time (Front)
006,1,Front Left,Sensor,Specification: max. 4.0 ms
006,2,Front Left,Center Sensor,Specification: max. 4.0 ms
006,3,Front Right,Center Sensor,Specification: max. 4.0 ms
006,4,Front Right,Sensor,Specification: max. 4.0 ms
;
007,0,Oscillation Time (Rear)
007,1,Rear Left,Sensor,Specification: max. 4.0 ms
007,2,Rear Left,Center Sensor,Specification: max. 4.0 ms
007,3,Rear Right,Center Sensor,Specification: max. 4.0 ms
007,4,Rear Right,Sensor,Specification: max. 4.0 ms
;
080,0,Advanced Control Module Identification I
080,1,Identification
080,2,Revision
080,3,Production,Date
080,4,Manufacturer &,Test Stand Number
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Parking Aid (J446) Coding
C01,?xxxx: Options
C02,0 = Trailer Hitch NOT installed
C03,1 = Trailer Hitch installed
C04,x?xxx: Transmission
C05,0 = Manual Transmission
C06,1 = Automatic Transmission
C07,xx?xx: Confirmation Sound
C08,0 = Reverse Gear Confirmation Sound inactive
C09,1 = Reverse Gear Confirmation Sound active
C10,xxx?x: Chassis
C11,0 = Limousine (Rest of World)
C12,2 = Limousine (North America)
C13,4 = S/RS-Variante Limousine (Rest of World)
C14,6 = S/RS-Variante Limousine (North America)
C15,xxxx?: Model
C16,8 = Audi A8 (4D)
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A001,0,Rear Buzzer Volume
A001,5,Rear Buzzer Volume
A001,6,Adaptation of the rear warning buzzer volume.
A001,7, 
A001,8,Range: 2...7 (quiet...loud)
;
A002,0,Rear Buzzer Frequency
A002,5,Rear Buzzer Frequency
A002,6,Adaptation of the rear warning buzzer frequency.
A002,7, 
A002,8,Range: 0...4 (0.5...2 kHz)
;
A003,0,Front Buzzer Volume
A003,5,Front Buzzer Volume
A003,6,Adaptation of the front warning buzzer volume.
A003,7, 
A003,8,Range: 2...7 (quiet...loud)
;
A004,0,Front Buzzer Frequency
A004,5,Front Buzzer Frequency
A004,6,Adaptation of the front warning buzzer frequency.
A004,7, 
A004,8,Range: 0...4 (0.5...2 kHz)
;
