;
; VCDS Label File
;
; Copyright © 2010 Ross-Tech, LLC
;
; Skoda Fabia (6Y)
;
; Component: J285 - Instrument Cluster (#17)
;
; P/N: 6Y0-920-??3-???
;
; includes measuring blocks, adaptation, coding, login and service reset
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 6Y-17.LBL
; 6Y-25.LBL
; 6Yx-9xx-xxx-17.LBL
; 6Y0-920-xx0-17.LBL
; 6Y0-920-xx3-17.LBL
; 6Y0-920-xx3-25.LBL
;
; created on 06/Dec/2010 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 06/Dec/2010
;
; requires VCDS 10.6.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,General
001,1,Vehicle Speed
001,2,Engine Speed
001,3,Oil Pressure,Switch 2,Range: Oil Pr. 2 <min / Oil Pr. 2 OK
001,4,Time
;
002,0,General
002,1,Odometer
002,2,Fuel Level
002,3,Fuel Sender,Resistance
002,4,Ambient,Temperature
;
003,0,General
003,1,Coolant,Temperature
003,2,Oil Level,,Range: Ok/n.Ok
003,3,Oil,Temperature
;
005,0,Service Interval Information I
005,1,Distance since,Service exceeded,Unit: 100 km
005,2,Time since,Service exceeded,Unit: 1 day(s)
005,3,Remaining Dist.,until Service,Unit: 100 km
005,4,Remaining Time,until Service,Unit: 1 day(s)
;
012,0,Adaptation Channels I
012,1,Adaptation,Channel
012,2,Mileage,since Service
012,3,Adaptation,Channel
012,4,Days,since Service
;
013,0,Adaptation Channels II
013,1,Adaptation,Channel
013,2,Minimum Mileage,to Service
013,3,Adaptation,Channel
013,4,Maximum Mileage to Service
;
014,0,Adaptation Channels III
014,1,Adaptation,Channel
014,2,Maximum Time,to Service
014,3,Adaptation,Channel
014,4,Minimum Time,to Service
;
050,0,General
050,1,Odometer
050,2,Engine Speed
050,3,Oil Temperature
050,4,Coolant,Temperature
;
060,0,Installation Information
;
125,0,CAN-Databus Powertrain (Communication)
125,1,Engine Electronics,,Range: Engine 1/Engine 0\nSpecification: Engine 1
125,2,Transmission,Electronics,Range: Transm. 1/Transm. 0\nSpecification: Transm. 1
125,3,Brake Electronics,(J104),Range: ABS 1/ABS 0\nSpecification: ABS 1
;
126,0,CAN-Databus Powertrain (Communication)
126,1,Steering Angle,Sensor (G85),Range: Steer. ang. 1/Steer. ang. 0\nSpecification: Steer. ang. 1
126,2,Airbag System,(J234),Range: Airbag 1/Airbag 0\nSpecification: Airbag 1
126,3,Steering Aid,(J500),Range: Steering 1/Steering 0\nSpecification: Steering 1
;
127,0,CAN-Databus Powertrain (Communication)
127,1,Central Electronics,(J519),Range: E.Load.Crtl 1/E.Load.Crtl 0\nSpecification: E.Load.Crtl 1
;
201,1,Distance Impulse Number
201,1,Distance Impulse,Number
;
202,0,Engine Hood Contact
202,1,Engine,Hood Contact,Range: open/closed (open if not installed)
;
221,0,Extended Service Interval (ESI)
221,1,Maximum Fuel,Quantity per Cyl.
221,2,Theoretical,Service Interval,Increments: 100 km
221,3,Annual Distance,Driven,Increments: 100 km
;
225,0,CAN-Databus Powertrain (Timeout)
225,1,Engine Electronics
225,2,Transmission,Electronics
225,3,Brake Electronics,(J104)
;
226,0,CAN-Databus Powertrain (Timeout)
226,2,Airbag System,(J234)
226,3,Steering Aid,(J500)
;
227,0,CAN-Databus Powertrain (Timeout)
227,1,Central Electronics,(J519)
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Instrument Cluster (J285) Coding
C01,??xxx: Equipment
C02,+02 = Seatbelt Warning installed
C03,+04 = Washer Fluid Warning installed
C04,+08 = Check Lamp for "Lamp/Bulp Diagnostic" installed
C05,+16 = Check Lamp for "Open Door(s)" installed
C07,xx?xx: Country
C08,0 = Germany (DE) / 1 = Europe (EU) / 2 = USA (US) / 3 = Canada (CDN)
C09,4 = Great Britain (GB) / 5 = Japan (JP) /6 = Saudi Arabia (SA) / 7 = Australia (AUS)
C10,xxx?x: Service Intervals
C11,0 = fixed Service Intervals without Oil Level/Temperature Sensor (PR-QG0)
C12,1 = flexible Service Intervals with Oil Level/Temperature Sensor (PR-QG1)
C13,2 = fixed Service Intervals with Oil Level/Temperature Sensor (PR-QG2)
C14,3 = without Service Intervals (USA/Canada)
C15,xxxx?: Engine Type (Distance Impulse Number)
C16,1 = All Engine/Transmission Combinations (Signal Source CAN: 23984)
C17,1 = All Engine/Transmission Combinations (Signal Source Speed Sensor: 3775)
C20,2 = 1.2l/40-47kW Gasoline Engines (Signal Source Speed Sensor: 3904)
;
;
;---------------------------------------------------
;
; Login
;
;---------------------------------------------------
;
;
L00,Instrument Cluster (J285) Login
; 21597 = Freischaltung EEPROM lesen/schreiben
L01,Note: Any Immobilizer related work like matching new Keys or replacing
L02,the Instrument Cluster you have to use Address 25 (Immobilizer) instead.
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A002,0,Service Reminder
A002,5,Service Reminder
A002,6,0 = Service NOT Due
A002,7,1 = Service Due
A002,8, 
A002,9,To reset the service reminder save 0 as new value.
;
A003,0,Consumption Correction
A003,5,Consumption Correction
A003,6,Standard Value: 100 %
A003,7,Display Range: 85...115 %
A003,8,Increments: 1 %
A003,9, 
A003,10,Calculation based on volume per distance (e.g. l/100km):
A003,11,New Adaptation Value = Old Adaptation Value * Calculated Consumption / Old Display Value
A003,12,Calculation based on distance per volume (e.g. MPG):
A003,13,New Adaptation Value = Old Adaptation Value * Old Display Value / Calculated Consumption 
;
A004,0,Language
A004,5,Language
A004,6,1 = German
A004,7,2 = English
A004,8,3 = French
A004,9,4 = Italian
A004,10,5 = Spanish
A004,11,6 = Portuguese
;
A009,0,Mileage/Odometer
A009,5,Mileage/Odometer
A009,6,Increments: 1 = 10 km or 1 = 10 mi
A009,7, 
A009,8,The distance can only be changed once until
A009,9,the current value is not over 100 km/62 mi.
;
A030,0,Tank Characteristic (Fuel Level Sensor)
A030,5,Tank Characteristic (Fuel Level Sensor)
A030,6,This channel is used to set the fuel gauge reserve mark
A030,7,therfor fill the tank with 7 l of fuel and correct the
A030,8,needle to hit the reserve mark. This is a parallel shift
A030,9,of the tank characteristic.
A030,10, 
A030,11,Standard: 128
A030,12,Range: 96...160 (-8.0...+8.0 l)
A030,13,Increments: 1 = 1 Ohm = 1/4 l
;
A035,0,Speed Threshold
A035,5,Speed Threshold
A035,6,This value represents the speed threshold of the
A035,7,dynamic oil pressure system. The threshold can be
A035,8,raised in increments of 250 RPM.
A035,9, 
A035,10,Standard: 0
A035,11,Range: 0...1000 U/min
A035,12,Increments: 250 U/min
;
A039,0,Oil Temperature/Level Sensor Installation
A039,5,Oil Temperature/Level Sensor Installation
A039,6,0 = Oil Temperature/Level Sensor not installed
A039,7,1 = Oil Temperature/Level Sensor installed
;
A040,0,Mileage since Service
A040,5,Mileage since Service
A040,6,Increments: 1 = 100 km
;
A041,0,Time since Service
A041,5,Time since Service
A041,6,Increments: 1 = 1 day(s)
;
A042,0,Minimum Mileage to Service
A042,5,Minimum Mileage to Service
A042,6,Increments: 1 = 100 km/mi
A042,7,150 = Standard (15.000 km)
A042,8,or (if coded to miles)
A042,9,093 = Standard (9.300 mi - ohne Longlife)
;
A043,0,Maximum Mileage to Service
A043,5,Maximum Mileage to Service
A043,6,Increments: 1 = 100 km/mi
A043,7,150 = fixed Service Intervals (15.000 km - w/o Longlife)
A043,8,300 = flexible Service Intervals (30.000 km - with Longlife)
A043,8,or (if coded to miles)
A043,9,00093 = fixed Service Intervals (9.300 mi - w/o Longlife)
A043,10,00180 = flexible Service Intervals (18.000 mi - with Longlife)
;
A044,0,Maximum Time to Service
A044,5,Maximum Time to Service
A044,6,Increments: 1 = 1 day(s)
A044,7,00365 = fixed Service Intervals (w/o Longlife)
A044,8,00730 = flexible Service Intervals (with Longlife)
;
A045,0,Oil Quality
A045,5,Oil Quality
A045,6,1 = fixed Service Intervals (w/o Longlife)
A045,7,2 = flexible Service Intervals (with Longlife)
;
A046,0,Total Consumption
A046,5,Total Consumption
A046,6,This value does not represent the actual consumption
A046,7,but is rather an arithmetic value for the service interval display.
;
A047,0,Soot Entry
A047,5,Soot Entry
A047,6,Arithmetic value used to calculate the amount of soot in
A047,7,the engine oil referenced to a distance of 100 km and used
A047,8,as comparison value for the service interval display.
;
A048,0,Thermal Load
A048,5,Thermal Load
A048,6,Arithmetic value used to calculate the thermal stress of
A048,7,the engine oil referenced to a distance of 100 km and used
A048,8,as comparison value for the service interval display.
;
A049,0,Minimum Time to Service
A049,5,Minimum Time to Service
A049,6,Increments: 1 = 1 day(s)
A049,7,00365 = Standard
;
;
;---------------------------------------------------
;
; Service Rückstellung
;
;---------------------------------------------------
;
;
RD,2,Service Reminder Status,1,
RD,40,ST_DSS,100,DIST
RD,41,ST_TSS,1,ST_D
RD,42,ST_MIDTS,100,DIST
RD,43,ST_MADTS,100,DIST
RD,44,ST_MATTS,1,ST_D
RD,45,ST_OQ,1,
RD,46,ST_TC,100,DIST
RD,47,ST_SQ,100,DIST
RD,48,ST_TL,100,DIST
RD,49,ST_MITTS,1,ST_D
;
RJ,0,0,Service Reset,,
RJ,0,1,2,0
;
