;
; VCDS Label File
;
; Copyright © 2009+ Ross-Tech, LLC
;
; VW Passat (35/3C)
;
; Component: J527 - Steering Wheel Electronics (#16)  (>= SW 0025)
;
; P/N: 3C0-953-549-???
;
; This file is part of a label file package,
; make sure you have all of the following files.
;
; 3C-16.LBL
; 3C0-953-549-SW20.LBL (<= SW 0020)
; 3C0-953-549-SW25.LBL (>= SW 0025)
;
; includes measuring blocks and coding
;
; created on 12/Jun/2009 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 04/Apr/2013
;
; requires VCDS 805.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,1,Blinker,,Display Range: Not Oper./Left/Right
001,2,Headlamp Flasher,,Display Range: Not Oper./Operated
001,3,High Beam,,Display Range: Not Oper./Operated
001,4,Front Wiper,,Display Range: Not Oper./Level/Stage Int./Stage 1/Stage 2
;
002,0,Wiper && Washer
002,1,Interval Stages,,Display Range: Stage 1/Stage 2/Stage 3/Stage 4
002,2,Wash Front,,Display Range: Not Oper./Operated
002,3,Wiping Rear,,Display Range: Not Oper./Operated/Not Installed
002,4,Washing Rear,,Display Range: Not Oper./Operated/Not Installed
;
003,1,Terminal Status
; ?xxxx = P-Contact
; x?xxx = S-Contact
; xx?xx = Terminal 75
; xxx?x = Terminal 15
; xxxx? = Terminal 50
003,2,Horn,,Display Range: Not Oper./Operated
003,3,Board Computer,,Display Range: Not Installed/Not Oper./Operated/Switch Reset/Switch UP/Switch DN/Switch Off
;
004,0,Cruise Control System (CCS) / Adaptive Cruise Control (ACC)
004,1,Main Switch,,Display Range: ON/OFF
004,2,CCS/ACC-Set,,Display Range: Not Oper./Operated/Accel/Delay/Stored Off
004,3,CCS/ACC-Status,,Display Range: Not Oper./Operated/Accel/Delay/Stored Off
;
005,1,Selector Lever,P Lock Switch
005,2,Selector Lever,P Position (CAN)
005,3,CCS Soleniod,,Display Range: ON/OFF
005,4,Ignition Key,Removal Lock
;
006,0,Multifunction Steering Wheel I
006,1,Communication,,Display Range: Not Installed/OK/not OK
006,2,Software Version
006,3,Hardware Version
006,4,Malfunction,recognized,Display Range: Yes/No
;
007,0,Multifunction Steering Wheel II
007,1,Vehicle Type
007,2,Vehicle Version
;
008,0,Multifunction Steering Wheel III
008,1,Thumb Wheel,(Left),Display Range: Not Installed/Not Oper.
008,2,Thumb Wheel,(Right),Display Range: Not Installed/Not Oper.
008,3,Tiptronic,(Down),Display Range: Not Installed/Not Oper./Operated
008,4,Tiptronic,(Up),Display Range: Not Installed/Not Oper./Operated
;
009,0,Multifunction Steering Wheel IV
009,1,Steering Wheel,Buttons
;
010,0,Heated Steering Wheel && Heated Seats
010,1,Steering Wheel,Heater,Display Range: Not Installed/OFF/ON\nSignal Type: Output
010,2,Temperature,,Display Range: Not Installed/Temperature\nSignal Type: Input
010,3,Steering Wheel,Heater Output,Signal Type: Output
010,4,Heated Seats,,Display Range: OFF/Stage\nSignal Type: Input
;
011,0,Dimming
011,1,Dimming,,Display Range: 0.0...100.0 %\nSignal Type: Input
011,2,Dimming,(Discrete),Display Range: 0.0...100.0 %\nSignal Type: Input
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Lensäulenelektronik (J527) Codierung
C01,0?xxxxx: Drive-Assist-Systems
C02,0 = with Drive-Assist-System-Message w/o Button
C03,1 = w/o Drive-Assist-System-Message w/o Button
C04,2 = with Drive-Assist-System-Message with Button
C05,3 = w/o Drive-Assist-System-Message with Button
C06,0x?xxxx: Multi-Function Control Module (J608)
C07,0 = J608 not installed / 1 = J608 installed (J527 as Master) / 2 = J608 installed (J608 as Master)
C08,0xx?xxx: Transmission
C09,0 = Manual Transmission / 1 = Automatic Transmission
C10,0xxx?xx: Multi-Function Steering Wheel (1-4 = LIN 1.3 / 5-8 = LIN 2.0)
C11,0 = Multi-Function Steering Wheel not installed
C12,1 OR 5 = Multi-Function Steering Wheel w/o Tiptronic and w/o Push-To-Talk (PTT) installed
C13,2 OR 6 = Multi-Function Steering Wheel with Tiptronic and no Push-To-Talk (PTT) installed
C14,3 OR 7 = Multi-Function Steering Wheel w/o Tiptronic and with Push-To-Talk (PTT) installed
C15,4 OR 8 = Multi-Function Steering Wheel with Tiptronic and with Push-To-Talk (PTT) installed
C16,0xxxx?x: Cruise Control System (CCS) and Adaptive Cruise Control (ACC)
C17,0 = Cruise Control System (CCS) not installed
C18,1 = 6 Position Cruise Control System (CCS) installed
C19,2 = 6 Position Adaptive Cruise Control (ACC) installed
C20,0xxxxx?: Rear Wiper and Wiper Stalk for Board Computer
C21,1 = Rear Wiper not installed / Wiper Stalk for Board Computer not installed
C22,2 = Rear Wiper installed / Wiper Stalk for Board Computer not installed
C23,3 = Rear Wiper not installed / Wiper Stalk for Board Computer installed
C24,4 = Rear Wiper installed / Wiper Stalk for Board Computer installed
;
