;
; VCDS Labeldatei
;
; Ford Galaxy (7M) / Seat Alhambra (7M) / VW Sharan (7M)
;
; Component: J362 - Immobilizer (#25)
;
; P/N: 7M0 953 257 ?
;
; includes measuring blocks, coding, adaptation and login
;
; created on 10/Feb/2009 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 30/Apr/2009
;
; requires VCDS 805.1 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,General
001,1,Number of,adapted Keys,Specification: 1...8
001,2,Reader Coil,Status,Specification: 1 = OK\n\n0 = not OK\n1 = OK
001,3,Key Status,(Transponder),Specification: 1 = OK\n\n0 = not OK (possibly defective)\n1 = OK
001,4,Variable Code,authorized,Specification: 1 = Yes\n\n0 = No\n1 = Yes
;
002,0,General (from 09/1997)
002,1,Key Learning,Time,(in Seconds)
002,2,Number of Keys,(specified),Specification: 0...8
002,3,Number of Keys,(actual),Specification: 0...8
002,4,Key Matching,Status,?xxx = Fault Status (0 = No Fault / 1 = Fault)\nx?xx = Adaption (0 = finished / 1 = running)\nxx?x = Current Key (0 = OK / 1 = Not OK)\nxxx? = Current Adaptation (0 = OK / 1 = Not OK)
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Immobilizer (J362) Coding
C01,The coding displays the used baud rate on the w-line for
C02,communication between immobilizer and engine control unit.
C03, 
C04,through 08/1997:
C05,09600 = all Models (Standard)
C06, 
C07,from 09/1997:
C08,The coding/baud rate will be automatically determined by the control module.
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;

;
;
;---------------------------------------------------
;
; login
;
;---------------------------------------------------
;
;
L00,Immobilizer (J362) Login
L01,Prior to Key Learning or adapting a new USED Immobilizer
L02,Control Module the Vehicle specific PIN/SKC (IMMO-Login)
L03,of the new USED Immobilizer Control Module has to be used
L04,to enable the adaptation.
L05,You'll find the PIN/SKC on the Key Tag of the additional
L06,Key (of the Donor Car) or you can acquire it through your
L07,responsible Distribution Center or Importer.
;
