;
; VAG-COM Label File
;
; Audi A6 (4F) / Audi A8 (4E) / Audi Q7 (4L)
;
; Component: R36 - Telephone Bluetooth (#77) - PR-9ZW
;
; P/N: 4F1-910-336-???
;
; includes measuring blocks, coding and adaptation
;
; created on 28/Nov/2006 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification: 28/Nov/2006
;
; requires VAG-COM 505.1 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;

;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Telephone Bluetooth (R36) Coding
C01,?0x00xx: Cradle/Charger
C02,0 = No Cell Phone Cradle/Charger installed
C03,1 = 1 Cell Phone Cradle/Charger installed
C04,2 = 2 Cell Phone Cradles/Chargers installed 
C05,x0?00xx: Vehicle Type
C06,4 = Audi A6 (4F) Sedan
C07,5 = Audi A6 (4F) Avant/Wagon/Allroad
C08,6 = Audi A8 (4E)
C09,7 = Audi Q7 (4L) 
C10,x0x00?x: Voice Control Language
C11,0 = Voice Control OFF
C12,1 = German / 2 = English
C13,3 = French / 4 = Italian
C14,5 = Spanish / 6 = Portuguese
C15,7 = Czech
C16,9 = Speaker depend Voice Selection 
C17,x0x00x?: MMI System
C18,1 = MMI High
C19,2 = MMI Standard 
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A007,0,Microphone Sensitivity
;
A008,0,Delay Time
A008,5,Delay Time
A008,6,Adjustment of the delay times to compensate the
A008,7,audio component delay and acoustic running times.
A008,8, 
A008,9,Range: 0...12 ms
;
A096,0,Optical Performance
A096,5,Optical Performance
A096,6,The optical performance of the MOST bus can be adapted.
A096,7, 
A096,8,0 = Normal Performance
A096,9,3 = Reduced Performance (-3 dB)
;
A133,0,Bluetooth
A133,5,Bluetooth
A133,6,0 = Bluetooth OFF
A133,7,1 = Bluetooth ON
;
A135,0,Bluetooth Pass Key
A135,5,Bluetooth Pass Key
A135,6,Set the 4-digit Bluetooth pass key using this channel.
;
