;
; VAG-COM Label File
;
; Audi A4 (8D) / VW Passat (3B)
;
; Component: J104 - Brake Electronics (#03) - Bosch 5.3 ABS/EDS/ASR
;
; P/N: 8E0-614-111-??? / 3B0-614-111-???
;
; includes measuring blocks and coding
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 3B-03.LBL
; 8E-03.LBL
; 8E0-614-111-ABS.LBL (Bosch 5.3 ABS)
; 8E0-614-111-EDS.LBL (Bosch 5.3 ABS/EDS)
; 8E0-614-111-ASR.LBL (Bosch 5.3 ABS/EDS/ASR)
; 8E0-614-111-ESP.LBL (Bosch 5.3 ABS/EDS/ASR/ESP)
;
; created on 31/Mar/2007 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification: 31/Mar/2007
;
; requires VAG-COM 405.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Wheel Speed
001,1,Wheel Speed,Front Left,Display Range: 0.0...255.0 km/h
001,2,Wheel Speed,Front Right,Display Range: 0.0...255.0 km/h
001,3,Wheel Speed,Rear Left,Display Range: 0.0...255.0 km/h
001,4,Wheel Speed,Rear Right,Display Range: 0.0...255.0 km/h
;
002,0,Status Bits
002,1,Brake Light Switch,,Display Range: 0/1
002,2,Return Flow Pump,,Display Range: 0/1
002,3,Solenoid Valve,Relay,Display Range: 0/1
;
003,0,Traction Control (ASR)
003,1,Engine Speed
003,2,Engine Torque,,0.0 % = Schubphase\n20.0...30.0 % = Idle\n100.0 % = Maximum Torque
003,3,ASR-Button,,0 = Not Oper.\n1 = Operated
;
004,0,Electronic Differential Lock (EDL)
004,1,Standing,Time
004,2,EDL-Shut Off,Over Temp.,0 = EDL during the last 20 start cycles not deactivated\n1 = EDL during the last 20 start cycles deactivated
004,3,EDL/ASR-Shut Off
;
;
;---------------------------------------------------
;
; Coding
;
;---------------------------------------------------
;
;
C00,Brake Electronics - Bosch 5.3 (J104) Coding
C01,000?x: Engine
C02,0 = Gasoline Engine 2.4l-2.8l (without CAN-Databus)
C03,1 = Diesel Engine
C04,2 = Gasoline Engine 1.8T
C05,3 = Gasoline Engine 2.4l-2.8l (with CAN-Databus) 
C06,000x?: Transmission
C07,0 = Manual Transmission (012) (without CAN-Databus)
C08,1 = Automatic Transmission (01V) (with CAN-Databus)
C09,2 = Manual Transmission (01E) (with CAN-Databus)
C10,3 = Multitronic (01J) (with CAN-Databus)
C11,3 = Automatic Transmission (01V) (without CAN-Databus) 
;
