;
; VCDS Label File
;
; Copyright © 2007-2011 Ross-Tech, LLC
;
; Seat Ibiza (6L)
;
; Component: J285 - Instrument Cluster (#17)
;
; P/N: 6L0-920-??0-??? / 6L0-920-??1-???
;
; includes measuring blocks, adaptation, coding and service reset
;
; This file is part of a label files package,
; make sure you have all of the following files.
;
; 6L-17.LBL
; 6L0-920-xx0-17.LBL  (< MY 2006)
; 6L0-920-xx3-17.LBL  (MY 2007 >)
;
; created on 22/Oct/2007 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 07/Feb/2011
;
; requires VCDS 10.6.3 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,General
001,1,Vehicle Speed
001,2,Engine Speed
001,3,Oil Pressure,Switch 2,Range: Oil Pr. 2 <min / Oil Pr. 2 OK
001,4,Time
;
002,0,General
002,1,Odometer
002,2,Fuel Level
002,3,Fuel Sender,Resistance
002,4,Ambient,Temperature
;
003,0,General
003,1,Coolant,Temperature
;
022,0,Immobilizer I
022,1,Engine Start,permitted,Specification: 1 = Yes\nRange: 0 = No / 1 = Yes
022,2,Engine (ECU),responds,Specification: 1 = Yes\nRange: 0 = No / 1 = Yes
022,3,Key Status,,Specification: 1 = Key OK\nRange: 0 = Key not OK / 1 = Key OK
022,4,Number of,adapted Keys,Specification: 1...4
;
023,0,Immobilizer II
023,1,Variable Code,authorized,Specification: 1 = Yes\nRange: 0 = No / 1 = Yes
023,2,Key Status,(Transponder),Range: 0 = Not Locked / 1 = Locked
023,3,Fixed Code,authorized,Specification: 1 = Yes\nRange: 0 = No / 1 = Yes
023,4,Immobilizer,Status,Specification: 6 (Immobilizer adapted)
; 1 = End of Assembly Line: NEW (Delivery Condition of New Instrument Cluster)
; 2 = End of Assembly Line: VIN adapted
; 3 = End of Assembly Line: ECU adapted
; 4 = Customer Service: NEW (Delivery Condition of Replacement Instrument Cluster)
; 5 = Customer Service: Instrument Cluster adapted
; 6 = Customer Service: Keys adapted (Normal Condition)
; 7 = Customer Service: Key Adaptation active
;
024,0,Immobilizer III (Lock-Time)
024,1,Lock-Time,Instrument Cluster
024,2,Lock-Time,Engine (ECU)
024,3,Lock-Time,Emergency Unlock
024,4,Lock-Time,Transponder
;
025,0,Immobilizer IV
025,1,Immobilizer,Communication,0 = No Communication\n1 = Communication via CAN-Databus\n2 = Communication via W-Line
;
050,0,General
050,1,Odometer
050,2,Engine Speed
050,3,Oil Temperature
050,4,Coolant,Temperature
;
125,0,CAN-Databus Communication (Powertrain)
125,1,Engine,,Specification: Engine 1\nRange: Engine 0/Engine 1
125,2,Transmission,,Range: Transm. 0/Transm. 1
125,3,Brake Electronics,(J104),Specification: ABS 1\nRange: ABS 0/ABS 1
;
126,0,CAN-Databus Communication (Powertrain)
126,2,Airbags,(J234),Specification: Airbag 1\nRange: Airbag 0/Airbag 1
126,3,Steering Angle,Sensor (G85),Specification: Steer. ang. 1\nRange: Steer. ang. 0/Steer. ang. 1
;
127,0,CAN-Databus Communication (Powertrain)
127,1,Central Electronics,(J519),Specification: E.Load.Crtl 1\nDisplay Range: E.Load.Crtl 1/E.Load.Crtl 0
;
201,1,Distance Impulse,Number
;
202,1,Engine Hood,Contact,Range: Open/Closed (Not Installed = Open)
;
225,0,CAN-Databus Timeout (Powertrain)
225,1,Engine
225,2,Transmission
225,3,Brake Electronics,(J104)
;
226,0,CAN-Databus Timeout (Powertrain)
226,2,Airbags,(J234)
226,3,Steering Angle,Sensor (G85)
;
227,0,CAN-Databus Timeout (Powertrain)
227,1,Central Electronics,(J519)
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Instrument Cluster (J285) Coding
C01,??xxx: Options
C02,+01 = Brakepad Warning active
C03,+02 = Seatbelt Warning active
C04,+04 = Washer Fluid Warning active
C05,xx?xx: Country
C06,0 = Germany / 1 = Europe
C07,4 = Great Britain (GB)
C08,6 = Saudi Arabia
C09,xxx?x: Cylinders
C10,3 = 3-Cylinders
C11,4 = 4-Cylinders
C12,xxxxx?: Distance Impulse Number (K-Value)
C13,2 = Engine Code BJX/BKV
C14,3 = Engine Code BBY/AUA/BKY
C15,4 = Engine Code AMF/BAY/ATD/AXR
C16,5 = Engine Code AZL/BBX/ASZ/BLT
C17,6 = Engine Code BBZ/AUB
C18,7 = Engine Code BNV/BMS/BNM/AZQ/BME/BAH
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A002,0,Service Reminder
A002,5,Service Reminder
A002,6,0 = Service NOT Due
A002,7,1 = Service Due
A002,8, 
A002,9,To reset the service reminder save 0 as new value.
;
A003,0,Consumption Correction
A003,5,Consumption Correction
A003,6,Standard Value: 100 %
A003,7,Display Range: 85...115 %
A003,8,Increments: 1 %
A003,9, 
A003,10,Calculation based on volume per distance (e.g. l/100km):
A003,11,New Adaptation Value = Old Adaptation Value * Calculated Consumption / Old Display Value
A003,12,Calculation based on distance per volume (e.g. MPG):
A003,13,New Adaptation Value = Old Adaptation Value * Old Display Value / Calculated Consumption 
;
A004,0,Language
A004,5,Language
A004,6,1 = German
A004,7,2 = English
A004,8,3 = French
A004,9,4 = Italian
A004,10,5 = Spanish
A004,11,6 = Portuguese
;
A005,0,Maximum Distance to Oil Service (OEL)
A005,5,Maximum Distance to Oil Service (OEL)
A005,6,15 = 15.000 km (Standard)
A005,7, 
A005,8,Resolution: 1 = 1000 km
;
A006,0,Maximum Distance to Inspection (IN1)
A006,5,Maximum Distance to Inspection (IN1)
A006,6,30 = 30.000 km (Standard)
A006,7, 
A006,8,Resolution: 1 = 1000 km
;
A007,0,Maximum Time to Inspection (IN2)
A007,5,Maximum Time to Inspection (IN2)
A007,6,12 = 12 Month (Standard)
A007,7, 
A007,8,Resolution: 1 = 1 Month
;
A009,0,Mileage/Odometer
A009,5,Mileage/Odometer
A009,6,Resolution: 1 = 10 km
A009,9,The distance can only be changed once until
A009,10,the current value is not over 100 km.
;
A010,0,Distance to Oil Service (OEL)
A010,5,Distance to Oil Service (OEL)
A010,6,150 = 15.000 km (Standard)
A010,7, 
A010,8,Resolution: 1 = 100 km
;
A011,0,Distance to Inspection (IN1)
A011,5,Distance to Inspection (IN1)
A011,6,300 = 30.000 km (Standard)
A011,7, 
A011,8,Resolution: 1 = 100 km
;
A012,0,Time to Inspection (IN2)
A012,5,Time to Inspection (IN2)
A012,6,360 = 360 Days (Standard)
A012,7, 
A012,8,Resolution: 1 = 1 Days
;
A021,0,Immobilizer - Key Adaptation
A021,1,Alte Schlüssel
A021,2,Anzahl
A021,5,Immobilizer - Key Adaptation
;
A030,0,Tank Characteristic (Fuel Level Sensor)
A030,5,Tank Characteristic (Fuel Level Sensor)
A030,6,This channel is used to set the fuel gauge reserve mark
A030,7,therfor fill the tank with 7 l of fuel and correct the
A030,8,needle to hit the reserve mark. This is a parallel shift
A030,9,of the tank characteristic.
A030,10, 
A030,11,Standard: 128
A030,12,Range: 120...136 (-2.0...+2.0 l)
A030,13,Increments: 1 = 1 Ohm = 1/4 l
;
A035,0,Speed Threshold
A035,5,Speed Threshold
A035,6,This value represents the speed threshold of the
A035,7,dynamic oil pressure system. The threshold can be
A035,8,raised in increments of 250 RPM.
;
A039,0,Oil Level Sensor Adaptation
A039,5,Oil Level Sensor Adaptation
A039,6,Determines if the TOG Sensor is installed or not.
;
;
;---------------------------------------------------
;
; service reset
;
;---------------------------------------------------
;
;
RD,2,Service Reminder Status,1,
RD,5,Maximum Distance to Oil Service (OEL),1000,km
RD,6,Maximum Distance to Inspection (IN1),1000,km
RD,7,Maximum Time to Inspection (IN2),1,Month
RD,10,Distance to Oil Service (OEL),100,km
RD,11,Distance to Inspection (IN1),100,km
RD,12,Time to Inspection (IN2),1,Days
;
RJ,0,0,Service Reset (OIL),,
RJ,0,1,10,150
;
RJ,1,0,Service Reset (INSP),,
RJ,1,1,10,150
RJ,1,2,11,300
;
RJ,2,0,Service Reset (OIL &  INSP),,
RJ,2,1,10,150
RJ,2,2,11,300
RJ,2,3,12,360
;
