;
; VCDS label file
;
; VW Lupo 3L (6E) / VW Polo (6N) 
;
; Component: Engine (#01) - AVY/ARC
;
; P/N: 036 906 033 ??
;
; includes measuring blocks, coding and readiness
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 03-01.LBL
; 036-906-033-AVY.LBL  (1.6l 16V   @ 125 HP - AVY/ARC)
;
; created on 25/FEB/2012 by Russell Capper 
;
; last modification: 25/MFEB/2012
;
; requires VCDS 803.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks & basic setting
;
;---------------------------------------------------
;
;
001,0,Basic Functions
001,1,Engine Speed,,Specification (Idle): 800...900 RPM
001,2,Coolant,Temperature,Specifiation: 80.0...110.0 °C
001,3,Lambda,Controller,Specification: -15.0...15.0 %
001,4,Basic Setting,Requirements,see labelfile
; 1xxxxxxx - Coolant temperature above 80 °C
; x1xxxxxx - Engine speed below 2000 RPM
; xx1xxxxx - Throttle valve closed
; xxx1xxxx - Lambda regulation correct
; xxxx1xxx - State of idle
; xxxxx1xx - A/C system compressor deactivated
; xxxxxx1x - Catalytic converter over 300 °C
; xxxxxxx1 - No malfunction detected by Self-Diagnosis
;
002,0,Basic Functions
002,1,Engine Speed,,Specification (Idle): 800...900 RPM 
002,2,Engine Load,,Specification: 12.0...30.0 %
002,3,Injection,Timing,Specification: 1.0...3.0 ms
002,4,Intake manifold,pressure,Specification: 250...500 mbar
;
003,0,Basic Functions
003,1,Engine Speed,,Specification (Idle): 800...900 RPM 
003,2,Intake manifold,pressure,Specification: 250...500 mbar
003,3,Throttle Drive,Angle Sensor 1,for EPC (G187) | Specification: 0.8...4.5 %
003,4,Ignition,Timing Angle,Specification: -5.0...10.0 °BDTC
;
004,0,Basic Functions
004,1,Engine Speed,,Specification (Idle): 800...900 RPM
004,2,Voltage Supply,,Specification: 11.5...15.0 V
004,3,Coolant,Temperature,Specifiation: 80.0...110.0 °C
004,4,Intake Air,Temperature,Specification: -48.0...142.5 °C
;
005,0,Basic Functions
005,1,Engine Speed,,Specification (Idle): 800...900 RPM 
005,2,Engine Load,,Specification: 12...30 %
005,3,Vehicle Speed,,Specification: 0 km/h
005,4,Load Status,,Display Range: Idling/Part Throttle/Enrichment/Overrun/Wide Open Throttle (WOT)
;
006,0,Basic Functions
006,1,Engine Speed,,Specification (idle): 800...900 RPM 
006,2,Engine Load,,Specification: 12...30 %
006,3,Intake Air,Temperature,Specification: -48.0...142.5 °C
006,4,Elevation Corr.,Factor,Specification: -50.0...20.0 %
;
010,0,Ignition
010,1,Engine Speed,,Specification (idle): 800...900 RPM 
010,2,Engine Load,,Specification: 12...30 %
010,3,Throttle valve,Angle Sensor 1,for EPC (G187),Specification: 0.8...4.5 %
010,4,Ignition,Timing Angle,Specification: -5.0...10.0 °BDTC
;
012,0,Ignition Position of Camshaft in respect to Crankshaft
012,1,Engine Speed,,Specification (Idle): 800...900 RPM 
012,2,Engine Load,,Specification: 12...30 % 
012,3,No of Crank tooth,low to high,Specification: 26...29
012,4,No of Crank tooth,high to Low,Specification: 88...90
;
014,0,Ignition Misfire Recognition
014,1,Engine Speed,,Specification (Idle): 800...900 RPM 
014,2,Engine Load,,Specification: 12...100 %
014,3,Misfire,(total),Specification: 0...20
014,4,Misfire,recognition,Specification: activated | Display Range: Activated/Blocked
;
015,0,Ignition (Misfire Recognition Cyl.1 to Cyl.3)
015,1,Misfire,Cylinder 1,Specification: 0...5
015,2,Misfire,Cylinder 2,Specification: 0...5
015,3,Misfire,Cylinder 3,Specification: 0...5
015,4,Misfire,recognition,Specification: activated | Display Range: Activated/Blocked
;
016,0,Ignition (Misfire Recognition Cyl. 4)
016,1,Misfire,Cylinder 4,Specification: 0...5
016,4,Misfire,recognition,Specification: activated | Display Range: active/Blocked
;
020,0,Ignition (Knock Control Cyl.1 to Cyl.4)
020,1,Timing Retardation,Cylinder 1,Specification: 0.0...12.0 °CA
020,2,Timing Retardation,Cylinder 2,Specification: 0.0...12.0 °CA
020,3,Timing Retardation,Cylinder 3,Specification: 0.0...12.0 °CA
020,4,Timing Retardation,Cylinder 4,Specification: 0.0...12.0 °CA
;
022,0,Ignition (Knock Control Cylinder 1 & 2)
022,1,Engine Speed,(G28),Specification: 800...6500 RPM
022,2,Engine Load,,Specification: 12...100 %
022,3,Timing Retardation,Cylinder 1,Specification: 0.0...12.0 °CA
022,4,Timing Retardation,Cylinder 2,Specification: 0.0...12.0 °CA
;
023,0,Ignition Timing Angle Retardation
023,1,Engine Speed,(G28),Specification: 800...6500 RPM 
023,2,Engine Load,,Specification: 12...100.0 %
023,3,Timing Retardation,Cylinder 3,Specification: 0.0...12.0 °CA
023,4,Timing Retardation,Cylinder 4,Specification: 0.0...12.0 °CA
;
028,0,Ignition Knock Control
028,1,Engine Speed,,Specification: 2500...6500 RPM
028,2,Engine Load,,Specification: 40.0...100.0 %
028,3,Coolant,Temperature,Specification: 80.0...110.0 °C
028,4,Result,Knock Sensor Test,Display Range: Test ON/Test OFF/Syst. OK/Syst. not OK,Specification: Sys. OK
;
030,0,Oxygen Sensor Status
030,1,Bank 1,Sensor 1,Before Catalyst,Specification: 111
; 1xx - Sensor heater
; x1x - Oxygen sensor ready
; xx1 - Lambda regulation active
030,2,Bank 1,Sensor 2,After Catalyst,Specification: 111
; 1xx - Sensor heater
; x1x - Oxygen sensor ready
; xx1 - Lambda regulation active
;
031,0,Lambda Control (idle)
031,1,Lambda Control,Bank 1 (actual),Specification: 0.9600...1.0400
031,2,Lambda Control,Bank 1 (specified),Specification: 0.9900...1.0100
;
032,0,Lambda Control (Mixture Adaptation before catalyst)
032,1,Lambda,Bank 1 (add.),Adaptation at idle speed,Specification: -10.0...10.0 %
032,2,Lambda,Bank 1 (mult.),Adaptation at part Load,Specification: -10.0...10.0 %
;
033,0,Lambda Control (Mixture Adaptation before catalyst)
033,1,Bank 1,Lambda Control,Specification: -15.0...15.0 %
033,2,Bank 1 Voltage,of Oxygen Sensors,Specification: 1.4...1.6 V
;
034,0,Oxygen Sensor Ageing Test (Before Catalyst)
034,1,Engine Speed,idle,Specification: 800...900 RPM
034,2,Catalytic Converter,Bank 1 Temp,Specification: Min 340.0 °C 
034,3,Dynamic Factor,Bank 1 Sensor 1,Specification: 1.0...4.0
034,4,Lambda,Ageing Check,Specification: Test OFF/Test ON/B1-S1 OK/B1-S1 not OK,Specification: B1-S1 ok
;
B034,0,Lambda Control Ageing Test (Before Catalyst)
; "Activate" Basic Setting
; Firmly press Brake Pedal and Throttle Pedal at once
; Engine Speed increases automatically > Field 4 = Test ON
; Wait until Field 4 shows "B1-S1 OK"
B034,1,Engine Speed,(G28),Specification: 800...900 RPM
B034,2,Catalytic Converter,Bank 1 Temp,Specification: Min. 340.0 °C 
B034,3,Dynamic Factor,Bank 1 Sensor,Specification: 1.0...4.0
B034,4,Result,Lambda Aging,Range: Test ON/Test OFF/B1-S1 not OK/B1-S1 OK, Specification: B1-S1 OK
;
041,0,Lambda Control (Lambda Sensor Heating)
041,2,Heater Condition,,Specification: Htg.S1 OFF/Htg.S1 ON
041,3,Resistance,Bank 1 Sensor 2,Specification: 
041,4,Heater Condition,,Specification: Htg.S2 OFF/Htg.S2 ON
;
043,0,Lambda Control Ageing Test (After Catalyst)
043,1,Engine Speed,(G28),Specification: 800...900 RPM
043,2,Catalytic Converter,Temperature,Specification: Min. 340.0 °C
043,3,Lambda Voltage,Bank 1 Sensor 2,,Specification: 0.00...1.00 V
043,4,Result,Aging Check,Display Range: Test ON/Test OFF/B1-S2 OK/B1-S2 n.OK\nSpecification: Test OFF
;
B043,0,Lambda Control Ageing Check: Bank 1 Sensor 2)
; "Activate" Basic Setting
; Firmly press Brake Pedal and Throttle Pedal at once
; Engine Speed increases automatically > Field 4 = Test ON
; Wait until Field 4 shows "B1-S2 OK"
B043,1,Engine Speed,(G28),Specification: 800...900 RPM
B043,2,Catalytic Converter,Temperature,Specification: Min. 340.0 °C
B043,3,Lambda Voltage,Bank 1 Sensor 2,,Specification: 0.00...1.00 V
B043,4,Result,Aging Check,Display Range: Test OFF/Test ON/B1-S2 OK/B1-S2 n.OK,Specification: B1-S2 OK
;
046,1,Engine Speed,,Secification: 1300...1500 RPM
046,2,Catalytic Converter,Temperature,Specification: min. 340 °C
046,3,Catalytic Converter,Effect,Specification: min. 1 %
046,4,Cat Conversion,Test,Specification: Test OFF/Test ON/Cat B1 OK/Cat B1 not OK,Specification: Cat B1 OK
;
050,0,Speed Regulation at idle
050,1,Engine Speed,Actual,Specification (AC OFF): 800...900 RPM | Specification (AC On): 850...930 RPM
050,2,Engine Speed,(Specified),Specification (AC OFF): 830 RPM | Specification (AC On): 900 RPM
050,3,Condition,of A/C system,Specification: ON/OFF
050,4,Operating condition,of A/C Compressor,Display Range: Compr.ON/Compr.OFF
;
054,0,Speed Regulation Whilst Driving
054,1,Engine Speed,,Specification: 800...6500 RPM
054,2,Load Status,,Display Range: Idle/Partial Throttle/Enrichment/Overrun/Wide Open Throttle (WOT)
054,3,Acc. Pedal,Position(G79),Specification: 0...100 %)
054,4,Throttle Valve,Angle (G187),Specification: 0.0...100 %
;
055,0,Speed Regulation Idling stabilisation
055,1,Engine Speed,,Specification: 800...900 RPM 
055,2,Idle Regulator,,Specification: -10.0...20.0 %
055,3,Idle Stabilization,Adaptation value,Specification: -10.0...10.0 %
055,4,Load Status,,see labelfile
; --1xx - Air conditioning system switched on
; --xx1 - Air conditioner compressor switched on
;
056,0,Speed Regulation Idling Speed Stablisation
056,1,Engine Speed,,Specification: 800...900 RPM
056,2,Engine Speed,(Specified),Specification: 830 RPM
056,3,Idle Regulator,,Specification: -10.0...20 %
056,4,Load Status,,see labelfile
; --1xx - Air conditioning system switched on
; --xx1 - Air conditioner compressor switched on
;
057,0,Speed Regulation at idle
057,1,Engine Speed,Actual,Specification (AC OFF): 800...900 RPM | Specification (AC On): 850...930 RPM
057,2,Engine Speed,(Specified),Specification (AC OFF): 830 RPM | Specification (AC On): 900 RPM
057,3,Condition,of A/C system,Specification: ON/OFF
057,4,Operating condition,of A/C Compressor,Display Range: Compr.ON/Compr.OFF
;
060,0,Speed Regulation (Throttle Body Adaptation)
060,1,Throttle Valve,Angle Sensor 1,for EPC (G187),Specification: 0.0...100.0 %
060,2,Throttle Valve,Angle Sensor 2,for EPC (G188),Specification: 100.0...0.0 %
060,3,Self-Adaptation,Steps Counter,Specification: 0...8
060,4,Throttle Adaption Cond.,Specification: ADP runs/ADP OK/ADP ERROR
;
B060,0,Electronic Throttle (Throttle Body Adaptation)
; "Activate" Basic Setting and do not press Throttle
; Wait until Field 4 shows "ADP OK"
B060,1,Throttle Valve,Sensor 1 (G187),Specification: 0.0...100.0 %
B060,2,Throttle Valve,Sensor 2 (G188),Specification: 100.0...0.0 %
B060,3,Throttle Adaptation,Steps Counter,Specification: 0...8
B060,4,Throttle Valve Adp.,Range: ADP RUN/ADP OK/ADP ERROR, Specification: ADP OK
;
061,0,Speed Regulation (EPC System)
061,1,Engine Speed,,Specification: 800...6500 RPM
061,2,Voltage Supply,,Specification: 11.5...15.0 V
061,3,Throttle Drive,Angle Sensor 1,for EPC (G187) | Display Range: 0...100 %
061,4,Load Status,,see labelfile
; --1xx - Air conditioning system switched on
; --xx1 - Air conditioner compressor switched on
;
062,0,Speed Regulation (EPC System)
062,1,Throttle Drive,Angle Sensor 1,for EPC (G187),Specification: 0.0...100.0 %
062,2,Throttle Drive,Angle Sensor 2,for EPC (G188),Specification: 100.0...0 %
062,3,Throttle Pedal,Position (G79),Specification: 0.0...98.0 %
062,4,Accel Pedal,Position Sender 2 (G185),Specification: 0...49.0 %)
;
066,0,Idle Speed Regulation (Additional Signals)
066,1,Vehicle Speed,(Current),Specification: 0 km/h
066,2,Switch Status,,See Label File
; -xx1 = Brake Light Switch (F)
; -x1x = Brake Pedal Switch (F47)
; -1xx = Clutch Pedal Switch(F36)
;
091,0,Performance Increase Camshaft Adjustment 
091,1,Engine Speed,(G28),Specification: 800..6500 RPM
091,2,Engine Load,,Specification: 40.0...100.0 %
091,3,Camshaft Adjustm.,Status,Range: ON/OFF,Specification: ON
091,4,Camshaft,Adjustment angle,Specification: -1.0...40.0 °ATDC  
;
093,0,Performance Increase Camshaft Adjustment (Phase Position)
093,1,Engine Speed,(G28),Specification: 800...6500 rpm
093,2,Engine Load,Specification: 0.0...100.0 %
093,3,Adjustment Pos,Inlet Cam,Specification: -1.0...8.0 °ATDC
;
094,0,Performance Increase Camshaft Adjustment (Intake)
094,1,Engine Speed,(G28),Specification: 2500...6000 rpm
094,2,Camshaft Adjustm.,Status,Range: CS ctrl.ON / CS ctrl. OFF,Specification: CS ctrl. ON
094,3,Result,Bank 1,Range: Test ON/Test OFF/Syst. OK/Syst. not OK
;
B094,0,Performance Increase Camshaft Adjustment (Intake)
; "Activate" Basic Setting
; Set Engine Speed to 2500...6000 rpm
; Vehicle Stationary, engine runs at increased idling speed
B094,1,Engine Speed,(G28),Specification: 2500...6000 rpm
B094,2,Camshaft Adjustm.,Status,Range: CS ctrl.ON / CS ctrl. OFF,Specification: CS ctrl. ON
B094,3,Result,Bank 1,Range: Test ON/Test OFF/Syst. OK/Syst. not OK
;
;
125,0,CAN-Databus Communication (Powertrain)
125,1,Anti-Lock Brake system,Status,Specification: ABS 1,ABS 0
125,3,Combi Instrument Cluster,,Specification: Combi 1
125,4,Airbag system,Status, Specification: Airbag 1
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Engine (J220) Coding
C01,000?x: Additional Functions
C02,+1 = ABS
C03,+2 = Airbag
C04,+3 = ABS and Airbag
C05,000x?: Transmission
C06,1 = 5-speed Manual Transmission
C07,2 = 6-speed Manual Transmission
C08,3 = Automatic Transmission
;
;
;---------------------------------------------------
;
; readiness
;
;---------------------------------------------------
;
;
O,036-906-033-AVY
;
