;
; VAG-COM Label File
;
; Audi A4 (8D)
;
; Component: J285 - Instrument Cluster (#17)
;
; P/N: 8D?-919-0??-???
;
; includes measuring blocks, adaptation, coding, login and service reset
;
; This file is part of a redirection package,
; make sure you have all of the following files.
;
; 8D-17.LBL
; 8D0-919-0xx-17.LBL  (MY 1995-1997)
; 8D0-919-xxx-17.LBL  (MY 1998-1999)
; 8D0-920-xxx-17.LBL  (MY 2000+)
;
; created by Mike Sauve (www.alientech.net)
; updated on 15/Sep/2003 by Alexey V. Gubin
; updated on 27/Feb/2007 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification: 01/Jan/2008
;
; requires VAG-COM 610.0 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,General
001,1,Vehicle Speed
001,2,Engine Speed
001,3,Oil Pressure,Switch 2,Range: Oil Pr. 2 <min / Oil Pr. 2 OK
;
002,0,General
002,1,Odometer
002,2,Fuel Level
;
003,0,General
003,1,Coolant,Temperature
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Instrument Cluster (J285) Coding
C01,??xxx: Options
C02,+01 = Brake Pad Warning active
C03,+02 = Seatbelt Warning active
C04,+04 = Washer Fluid Warning active
C05,+16 = Navigation active 
C06,xx?xx: Country
C07,0 = Germany (D) / 1 = Europe (EU) / 2 = USA (US)
C08,3 = Canada (CDN) / 4 = Great Britain (GB)
C09,5 = Japan (JP) / 6 = Saudi Arabia (SA) / 7 = Australia (AUS) 
C10,xxx?x: Cylinder
C11,4 = 4-Cylinder
C12,6 = 6-Cylinder
C13,8 = 8-Cylinder
C14,xxxx?: Engine
C15,0 = TDI-Engine
C16,2 = 4-Cylinder and 6-Cylinder Gasoline-Engine
C17,3 = 8-Cylinder Gasoline-Engine
C18,4 = Turbo-Engine
;
;
;---------------------------------------------------
;
; login
;
;---------------------------------------------------
;
;
L00,Instrument Cluster (J285) Login
L01,13861 = Adaptation Enabling
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A02,0,Service Reminder
A02,5,Service Reminder
A02,6,Displayed Values:
A02,7,01 = Oil Service Due
A02,8,10 = Inspection Due
A02,9,11 = Oil Service and Inspection Due
A02,10, 
A02,11,New Values:
A02,12,00 = Reset Oil Service and Inspection
A02,13,01 = Reset Oil Service
A02,14,10 = Reset Inspection
;
A003,0,Consumption Correction
A003,5,Consumption Correction
A003,6,Standard Value: 100 %
A003,7,Display Range: 85...115 %
A003,8,Increments: 1 %
A003,9, 
A003,10,Calculation based on volume per distance (e.g. l/100km):
A003,11,New Adaptation Value = Old Adaptation Value * Calculated Consumption / Old Display Value
A003,12,Calculation based on distance per volume (e.g. MPG):
A003,13,New Adaptation Value = Old Adaptation Value * Old Display Value / Calculated Consumption 
;
;
;---------------------------------------------------
;
; service reset
;
;---------------------------------------------------
;
;
RD,2,Service Reminder Status,1,
RD,5,Distance to Oil Change (OEL),1000,km
RD,6,Distance to Inspection 1 (IN1),1000,km
RD,7,Time to Inspection 1 (IN1),10,Days
RD,8,Time to Inspection 2 (IN2),10,Days
;
RJ,0,0,Service Reset (OIL),,
RJ,0,1,2,10
;
RJ,1,0,Service Reset (INSP),,
RJ,1,1,2,1
;
RJ,2,0,Service Reset (OIL &  INSP),,
RJ,2,1,2,0
;
RJ,3,0,Individual Service Reset (OIL),,
RJ,3,1,5,15
;
RJ,4,0,Individual Service Reset (INSP),,
RJ,4,1,6,30
RJ,4,2,7,36
RJ,4,3,8,72
;
RJ,5,0,Individual Service Reset (OIL &  INSP),,
RJ,5,1,5,15
RJ,5,2,6,30
RJ,5,3,7,36
RJ,5,4,8,72
;
