;
; VCDS Label File
;
; Copyright © 2014+ Ross-Tech, LLC
;
; Audi A6 (4B)
;
; Component: J526 - Telephone/Telematics Control Module (#75)
;
; P/N: 8E0-035-616-???
;
; includes measuring blocks, adaptation and coding
;
; created on 01/May/2014 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modification on 01/May/2014
;
; requires VCDS 12.12.2 or newer
;
;
;---------------------------------------------------
;
; measuring blocks
;
;---------------------------------------------------
;
;
001,0,Telematics Status
001,1,Telematics
001,2,Telematics,Status,Range: Registered/Not Registered
001,3,Signal Strengths
001,4,Signal Strengths,Status,Range: 0.0...100.0 %
;
002,0,Emergency Battery && Satellites
002,1,Emergency,Battery
002,2,Emergency,Battery,Range: Empty/Low/Full
002,3,GPS Acqired,Sattelites
002,4,GPS Acqired,Sattelites,Range: 0.0...12.0
;
003,0,Cellular Telephone && OnStar Button
003,1,Cellular Telephone
003,2,Cellular Telephone,Status,Range: Connected/Not Connected
003,3,OnStar Button
003,4,OnStar Button,Status,Range: Operated/Not Oper.
;
004,0,Emergency Call && Hang-Up Button
004,1,Emergency Call,Switch
004,2,Emergency Call,Switch Status,Range: Operated/Not Oper.
004,3,Hang-Up Button
004,4,Hang-Up Button,Status,Range: Operated/Not Oper.
;
005,0,Terminal X Status
005,1,Terminal X,Status,Range: Terminal X ON/Terminal X OFF
;
020,0,Global Positioning System (GPS) Longitude I
020,1,GPS Longitude
020,2,GPS Longitude,Degrees
020,3,GPS Longitude,Minutes
020,4,GPS Longitude,Seconds
;
021,0,Global Positioning System (GPS) Latitude I
021,1,GPS Latitude
021,2,GPS Latitude,Degrees
021,3,GPS Latitude,Minutes
021,4,GPS Latitude,Seconds
;
022,0,Global Positioning System (GPS) Altitude I
022,1,GPS Altitude
022,2,GPS Altitude
;
023,0,Global Positioning System (GPS) Longitude II
023,1,GPS Longitude
023,2,GPS Longitude,Degrees
023,3,GPS Longitude,Minutes
023,4,GPS Longitude,Seconds
;
022,0,Global Positioning System (GPS) Latitude II
022,1,GPS Latitude
022,2,GPS Latitude,Degrees
022,3,GPS Latitude,Minutes
022,4,GPS Latitude,Seconds
;
025,0,Global Positioning System (GPS) Altitude II
025,1,GPS Altitude
025,2,GPS Altitude
;
026,0,Global Positioning System (GPS) Date
026,1,GPS Date
026,2,GPS Date,Day
026,3,GPS Date,Month
026,4,GPS Date,Year
;
027,0,Global Positioning System (GPS) Time
027,1,GPS Time
027,2,GPS Time,Hours
027,3,GPS Time,Minutes
027,4,GPS Time,Seconds
;
028,0,Global Positioning System (GPS) Direction / Dilution of Precision
028,1,GPS Direction
028,2,GPS Direction
028,3,GPS Dilution,of Precision
028,4,GPS Dilution,of Precision
;
029,0,Speed Signal && GSM Antenna
029,1,Speed Signal
029,2,Speed Signal,Status,Range: 0.0...52.0
029,3,GSM Antenna
029,4,GSM Antenna,Status,Range: OK/Short Circuit/Open Circuit
;
030,0,Vehicle && Emergency Battery
030,1,Vehicle Battery
030,2,Vehicle Battery,Voltage,Range: 0.0...20.0 V
030,3,Emergency Battery
030,4,Emergency Battery,Voltage,Range: 0.0...25.0 V
;
125,0,CAN-Databus Communication (Infotainment)
125,1,Instruments,(J285),Range: Instrum. 1/Instrum. 0/Instrum. 1-W\nSpecification: Instrum. 1
125,2,Steering Wheel,Control Module,Range: St. Wheel 1/St. Wheel 0/St. Wheel 1-W\nSpecification: St. Wheel 1
125,3,Radio System,,Range: Radio 1/Radio 0/Radio 1-W\nSpecification: Radio 1
125,4,Navigation System,,Range: Navig. 1/Navig. 0/Navig. 1-W\nSpecification: Navig. 1
;
126,0,CAN-Databus Communication (Infotainment)
126,1,CAN-Databus,Infotainment
126,2,CAN-Databus,Infotainment,Range: Bus OK/Bus Not OK\nSpecification: Bus OK
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;SW:8E0-035-616-A   HW:8E0-035-616-A ---  Telematics
;Component:Telematik USA1    , Coding:0002033
;
C00,Telephone/Telematics Control Module (J526) Coding
C01,000?xxx: Model
C02,2 = Audi A6 (4B)
C03,000x?xx: Steering Wheel
C04,0 = Multi-Function Steering Wheel (MFSW) NOT installed
C05,3 = Multi-Function Steering Wheel (MFSW) & Voice Recognition installed
C06,000xx?x: Navigation
C07,0 = Navigation System NOT installed
C08,3 = Navigation System (Generation 4) installed
C09,000xxx?: Radio/Sound System
C10,2 = Radio Generation II w/o Sound System installed
C11,3 = Radio Generation II with Sound System installed
;
;
;---------------------------------------------------
;
; adaptation
;
;---------------------------------------------------
;
;
A003,0,Transport/Service Mode
A003,1,Transport/Service Mode
A003,2,Status
A003,5,Transport/Service Mode
A003,6,The Telematic System is disabled while Transport Mode is active to reduce Battery
A003,7,Drain while the Vehicle is stored or being transported for a longer Period of Time.
A003,8, 
A003,9,0 = Transport/Service Mode OFF
A003,10,1 = Transport/Service Mode ON
;
;A007,0,
;0
;A007,1,
;Test call
;A007,2,
;OFF 
;
A008,0,Emergency Battery
A008,1,Emergency Battery
A008,2,Status
A008,5,Emergency Battery
A008,6,Before disconnecting the Vehicle Battery the Emergency Battery needs to be switched-off
A008,7,and switched back on when reconnecting the Vehicle Battery. After replacing the Emergency
A008,8,Battery the Telematics Control Module needs to reset the Battery Time Register (i.e. how long
A008,9,the Emergency Battery had been used/powered with the Vehicle Battery being disconnected/low).
A008,10, 
A008,11,0 = Emergency Battery ON
A008,12,1 = Emergency Battery ON (Time Register Reset)
A008,13,2 = Emergency Battery OFF
;
;A099,0,
;0
;A099,1,
;Test OFF 
;
