;
; VCDS Label File
;
; Copyright © 2004-2012 Ross-Tech, LLC
;
; VW Touareg (7L)
;
; Component: J527 - Steering Wheel Electronics (#16)
;
; P/N: 7L6-953-549-???
;
; includes measuring blocks and coding
;
; created on 18/Oct/2004 by Sebastian Stange (Sebastian@Ross-Tech.com)
;
; last modified on 12/Apr/2012
;
; requires VCDS 805.0 or higher
;
;
;---------------------------------------------------
;
; measuaring blocks
;
;---------------------------------------------------
;
;
001,1,Blinker,,Specified value: inactive/links/rechts
001,2,Headlamp,flasher,Specified value: inactive/active
001,3,High beam,,Specified value: inactive/active
001,4,Signal horn,,Specified value: inactive/active
;
002,1,Wiping,,Specified value: inactive/Intervall/Stufe 1/Stufe 2
002,2,Interval,potentiometer,Specified value: off/level 1, 2 , 3/Poti n.Ok.
002,3,Front washing,,Specified value: inactive/active
002,4,Voltage,terminal 30
;
003,1,Rear windshield,wiping,Specified value: inactive/active
003,2,Rear washing,,Specified value: inactive/active
;
004,1,Steering column,adjustment,Specified value: inactive/raise/lower/forward/backward
004,2,Easy Entry,switch,Specified value: on/off
;
005,0,CSO-signals
005,1,Terminal P,,Specified value: on/off
005,2,Terminal S,,Specified value: on/off
005,3,Terminal X,,Specified value: on/off
005,4,Terminal 15,,Specified value: on/off
;
006,1,Terminal X,switched on,Specified value: yes/no
006,2,Heatet seat,status,Specified value: off/[level]
006,3,Steering wheel,heater enabled,via Vehicle VSCM (Specified value: yes/no)
;
007,0,Steering wheel heating
007,1,Heater status,,Specified value: not installed/on/off
007,2,Temperature,sensor,Specified value: not installed/[level]
;
012,1,CCS+ switch,,Specified value: inactive/active
012,2,CCS- switch,,Specified value: inactive/active
012,3,SET button,,Specified value: inactive/active
012,4,RESET button,,Specified value: sinactive/active
;
013,1,CANCEL button,,Specified value: inactive/active
013,2,CCS ON/OFF,button,Specified value: inactive/active
013,3,Illumination,button,Specified value: inactive/active
;
014,1,Vol+ button,,Specified value: inactive/active
014,2,Vol- button,,Specified value: inactive/active
014,3,Telephone button,,Specified value: inactive/active
014,4,PTT button,,Specified value: inactive/active
;
015,1,Button OK,,Specified value: inactive/active
015,2,Abort button,,Specified value: inactive/active
015,3,Menu button,,Specified value: inactive/active
;
080,0,Advanced Control Module Identification I
;
081,0,Advanced Control Module Identification II
;
125,0,CAN-Databus Communication
125,1,Instrument Cluster,(J285),Range: Instruments 1/Instruments 0\nSpecification: Instruments 1
125,2,Electrical,Ignition Lock,Range: El.Ign.Lock 1/El.Ign.Lock 0\nSpecification: El.Ign.Lock 1
125,3,Battery,Management,Range: Batt.Mgmt 1/Batt.Mgmt 0\nSpecification: Batt.Mgmt 1
125,4,Seat Memory,Driver,Range: Memory 1/Memory 0
;
;
;---------------------------------------------------
;
; coding
;
;---------------------------------------------------
;
;
C00,Steering Wheel Electronics (J527) Coding
C01,00xx?xx: Heated Steering Wheel
C02,0 = Heated Steering Wheel not installed
C03,1 = Heated Steering Wheel installed (via Seat Heating)
C04,2 = Heated Steering Wheel installed (via Multi-Function-Steering-Wheel Button)
C05,00xxx?x: Multi-Function Steering Wheel
C06,0 = Multi-Function Steering Wheel NOT installed
C07,1 = Multi-Function Steering Wheel (High) with 6 Buttons (CCS) installed
C08,2 = Multi-Function Steering Wheel (High) with 6 Buttons (CCS/ACC) installed
C09,3 = Multi-Function Steering Wheel (Low) with 4 Buttons (CCS) installed
C10,00xxxx?: Steering Column Adjustment
C11,1 = Steering Column Adjustment not installed
C12,2 = Steering Column Adjustment installed
;
